{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["Dual speed Polisher (112)","Monodisk Burnisher (100)","Auto Scrubber (2)","Janitor Trolley Complete (100)"],"not_rendered":{"images":1,"defined_names":6},"read":"whole","date_system":"1900"}

{"sheet":"Dual speed Polisher (112)","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,4,6],[7,1,7,6],[17,1,17,6],[24,2,24,6],[34,2,34,6],[39,2,39,6]]}
["ANNEXURE A. : TECHNICAL SPECIFICATION"]
["GT/GDH/125/2024-THE SUPPLY, DELIVERY AND MAINTEANCE OF RIDE ON POLISHERS AND ACCESSORIES, AS WELL AS VARIOUS ITEMS ASSOCIATED WITH POLISHERS GAUTENG DEPARTMENT OF HEALTH FACILITIES FOR A PERIOD OF THREE YEARS"]
["ANNEXURE A:TECHNICAL SPECIFICATION EVALUATION FOR DUAL SPEED POLISHERS"]
["Note:                                                                                                                                                                                                                                                                                                                                                                     1.  Bidders are required to indicate compliance/non-compliance with the specification by typing 'YES/NO' on each line item on column C.                                                                                                                                                                                                                                                                                                                                                 2. In the case where an equivalent or better option is provided, bidders must type the full description of the equivalent or better item on column D. Comments on the equivalent item must be provided on Column E.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              3. Bidder is required provide details of the product offer on column F.                                                                                                                                                                                                                                                                                                                   4. Bidder to provide reference to brochure (page number) / technical data sheet / supporting documents  on column G.                                                                                                                                                                                                                                                                                                                                                                                                                            "]
[]
["A","B","C","D","E","F","G"]
["Item no.","Technical Specification","Comply (Yes/No)","Provide Equivalent/Better          (if applicable)","Comments on Equivalent/Better","Details of Product Offer                                           (Provide your answers in this Column. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification) /  Supporting Document"]
["A","High Speed Polisher"]
["A.1"," dualspeed polisher"]
["A.2","Strong Induction Motor"]
["A.3","Direct Drive"]
["A.4","Vacum capability"]
["A.5","Brush presure adjustment function"]
["A.6","LED display 6 inch or more"]
["A.7","Floating Pad system"]
["A.8","Ergonomic adjustable handles with hieght regulation capabilities"]
["A.9","Low working height "]
["B","Wheels"]
["B.1","Two (2) allterrain castor wheels "]
["B.2","Must have safety lock-out switch"]
["B.3","Non- marking wheels"]
["B.4","Should allow for high maneuouvrability"]
["B.5","Wheels size 200mm suitable for both inside and outside"]
["B.6","Electric Spray system capabilities / function"]
["C","Technical Specification"]
["C.1","Working width - 505 mm"]
["C.2","Brush speed between  - 150-500 RMP"]
["C.3","Voltage 220 -240V"]
["C.4","Frequency - 50Hz"]
["C.5","Brush mrating- 133Wotor "]
["C.6","Brush contact preasure should be adjustable - 0/5kg"]
["C.7","Power supply cable Length - maximum - 20 meters"]
["C.8","Noise Level - <60dbA"]
["C.9","Direct transmission"]
["D","Dimensions"]
["D.1","Hieght max - 1150mm "]
["D.2","Length  max  -  800mm"]
["D.3","Width max  - 580mm"]
["D.4","Weight between  - 40-50kg"]
["E","Accessories Optional"]
["E.1","Filter Bag - (If applicable)"]
["E.2","Polisher pads"]

{"sheet":"Monodisk Burnisher (100)","index":1,"n_rows":47,"n_cols":7,"rows_kept":47,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,4,6],[7,2,7,6],[17,2,17,6],[24,2,24,6],[35,2,35,6],[40,2,40,6]]}
["ANNEXURE A. : TECHNICAL SPECIFICATION"]
["GT/GDH/125/2024-THE SUPPLY, DELIVERY AND MAINTEANCE OF RIDE ON POLISHERS AND ACCESSORIES, AS WELL AS VARIOUS ITEMS ASSOCIATED WITH POLISHERS GAUTENG DEPARTMENT OF HEALTH FACILITIES FOR A PERIOD OF THREE YEARS "]
["ANNEXURE A: TECHNICAL SPECIFICATION EVALUATION FOR MONODISK SPEED BURNISHER"]
["Note:                                                                                                                                                                                                                                                                                                                                                                     1.  Bidders are required to indicate compliance/non-compliance with the specification by typing 'YES/NO' on each line item on column C.                                                                                                                                                                                                                                                                                                                                                 2. In the case where an equivalent or better option is provided, bidders must type the full description of the equivalent or better item on column D. Comments on the equivalent item must be provided on Column E.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              3. Bidder is required provide details of the product offer on column F.                                                                                                                                                                                                                                                                                                                   4. Bidder to provide reference to brochure (page number) / technical data sheet / supporting documents  on column G.                                                                                                                                                                                                                                                                                                                                                                                                                            "]
[]
["A","B","C","D","E","F","G"]
["Item no.","Technical Specification","Comply (Yes/No)","Provide Equivalent/Better          (if applicable)","Comments on Equivalent/Better","Details of Product Offer                                           (Provide your answers in this Column. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification) /  Supporting Document"]
["A","High Speed Burnisher: Features"]
["A.1","Ultra- high dual speed burnisher"]
["A.2","Strong Induction Motor"]
["A.3","Drive board 17INCH"]
["A.4","Drive must be of plastic gears"]
["A.5","Pad holder size 17inch"]
["A.6","Low working height "]
["A.7","Suctioning function"]
["A.8","Scrubbing function capabilities"]
["A.9","Polishing function capabilities"]
["B","Wheels"]
["B.1","Two (2) allterrain castor wheels "]
["B.2","Must have safety lock-out switch"]
["B.3","Non- marking wheels"]
["B.4","Should allow for high maneuouvrability"]
["B.5","Wheels size 200mm suitable for both inside and outside"]
["B.6","Have Dust pick-up function and or attachement"]
["C","Technical Specification"]
["C.1","Working width - 430 -505 mm"]
["C.2","Brush speed - 1500  RMP"]
["C.3","Voltage 220 -240V"]
["C.4","Frequency - 50Hz"]
["C.5","Brush motor rating- 1000 - 1300W "]
["C.6","Brush contact preasure should be adjustable -43.3g/cm2"]
["C.7","Brush motor should allow for under - ride height - minimum of - 330mm"]
["C.8","Power supply cable Length - maximum - 20 meters"]
["C.9","Noise Level - <60dbA"]
["C.10","Direct transmission"]
["D","Dimensions"]
["D.1","Height max - 1200mm "]
["D.2","Length  max  -  550mm"]
["D.3","Width maximum - 450mm"]
["D.4","Weight maximum - 45kg"]
["E","Accessories Optional"]
["E.1","Filter Bag - (If applicable)"]
["E.2","Standard brush 17 inch - or applicable size"]
["E.3","Polishing brush 17 inch - or applicable size"]
["E.4","Suction kit - applicable consumables"]
["E.5","Scrubbing Disk 17 inch - or applicable size"]
["E.6","Carborundum disk 17 inch -or applicable size"]

{"sheet":"Auto Scrubber (2)","index":2,"n_rows":52,"n_cols":7,"rows_kept":52,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,4,6],[7,2,7,6],[23,2,23,6],[29,2,29,6],[45,2,45,6],[50,2,50,6]]}
["ANNEXURE A. : TECHNICAL SPECIFICATION"]
["GT/GDH/125/2024-THE SUPPLY, DELIVERY AND MAINTEANCE OF RIDE ON POLISHERS AND ACCESSORIES, AS WELL AS VARIOUS ITEMS ASSOCIATED WITH POLISHERS GAUTENG DEPARTMENT OF HEALTH FACILITIES FOR A PERIOD OF THREE YEARS "]
["ANNEXURE A: TECHNICAL SPECIFICATION EVALUATION FOR AUTO SCRUBBERS"]
["Note:                                                                                                                                                                                                                                                                                                                                                                     1.  Bidders are required to indicate compliance/non-compliance with the specification by typing 'YES/NO' on each line item on column C.                                                                                                                                                                                                                                                                                                                                                 2. In the case where an equivalent or better option is provided, bidders must type the full description of the equivalent or better item on column D. Comments on the equivalent item must be provided on Column E.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              3. Bidder is required provide details of the product offer on column F.                                                                                                                                                                                                                                                                                                                   4. Bidder to provide reference to brochure (page number) / technical data sheet / supporting documents  on column G.                                                                                                                                                                                                                                                                                                                                                                                                                            "]
[]
["A","B","C","D","E","F","G"]
["Item no.","Technical Specification","Comply (Yes/No)","Provide Equivalent/Better          (if applicable)","Comments on Equivalent/Better","Details of Product Offer                                           (Provide your answers in this Column. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification) /  Supporting Document"]
["A","Ride-on Scrubber dryer: Features"]
["A.1","Scrubber dryer suitable for heavy traffic areas"]
["A.2","Suitable to clean all types of floor ( i.e tiles, vinyl, sealed wood, marble, concreate etc)"]
["A.3","Must use mechanics to lift and lower the brush or squeegee"]
["A.4","Auomatic reduction of speed control"]
["A.5","Must have ERGONOMIC seat with safety switch"]
["A.6","Built in squeegee hanging system on recovery tank for easy machine transfere on narrow areas."]
["A.7","Intergrated on-board charger for  plug-in and battery charge"]
["A.8","Have opening  to th erecovery tank ( for easy cleaning)."]
["A.9","Intuitive dash board that allows for  user friendly and easy to operate."]
["A.10","Front and rear bumpers"]
["A.11","Battery charger"]
["A.12","Recovery empty hose"]
["A.13","Disk deck must have two (2) brushes"]
["A.14","Water level indicater"]
["A.15","Must have padholder and squeegee storage on board."]
["B","Wheels"]
["B.1","Three (3) all terrain  wheels "]
["B.2","Non- marking wheels"]
["B.3","Should allow for high maneuouvrability"]
["B.4","Wheels size 20- 25 cm suitable for both inside and outside"]
["B.5","Capability to cover - minimum of 4410sq meter/ hour ( Productivity rate)"]
["C","Technical Specification"]
["C.1","Drive motor - 500hp (w)  or above"]
["C.2","Brush motor - 2 x 300(w) or above"]
["C.3","Vacuum Motor power - 500hp (w)  or above"]
["C.4","Battery type - 6V 24Ah/ C20AGM ( 4pieces) or equivalent or better"]
["C.5","Sound preasure valve - 69db(A)) or better"]
["C.6","Cleaning / working width - 710mm or more"]
["C.7","Maximum climbing rate - 10%"]
["C.8","Solution tank - 120liters"]
["C.9","Recovery tank - 120liters"]
["C.10","Brush pressure - 35-40kg"]
["C.11","Brush speed - 200 - 205 RMP"]
["C.12","Brush diameter - 2 x 355mm or better"]
["C.13","Maximum speed - 6km/h or more"]
["C.14","Battery compartment  size - 610 x 408 x365"]
["C.15","Charging system - 24V - 25 V or better"]
["D","Dimensions"]
["D.1","Hieght max - 1580mm "]
["D.2","Length  max  -  1230mm"]
["D.3","Width maximum - 760mm"]
["D.4","Weight maximum - 225kg"]
["E","Accessories Optional"]
["E.1","Drive polisher pads compatible to the machine"]

{"sheet":"Janitor Trolley Complete (100)","index":3,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,4,6],[7,2,7,6],[18,2,18,6],[23,2,23,6]]}
["ANNEXURE A. : TECHNICAL SPECIFICATION"]
["GT/GDH/125/2024-THE SUPPLY, DELIVERY AND MAINTEANCE OF RIDE ON POLISHERS AND ACCESSORIES, AS WELL AS VARIOUS ITEMS ASSOCIATED WITH POLISHERS GAUTENG DEPARTMENT OF HEALTH FACILITIES FOR A PERIOD OF THREE YEARS "]
["ANNEXURE A: TECHNICAL SPECIFICATION EVALUATION FOR JANITOR TROLLEY"]
["Note:                                                                                                                                                                                                                                                                                                                                                                     1.  Bidders are required to indicate compliance/non-compliance with the specification by typing 'YES/NO' on each line item on column C.                                                                                                                                                                                                                                                                                                                                                 2. In the case where an equivalent or better option is provided, bidders must type the full description of the equivalent or better item on column D. Comments on the equivalent item must be provided on Column E.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              3. Bidder is required to provide details of the product offer on column F.                                                                                                                                                                                                                                                                                                                   4. Bidder to provide reference to brochure (page number) / technical data sheet / supporting documents  on column G.                                                                                                                                                                                                                                                                                                                                                                                                                            "]
[]
["A","B","C","D","E","F","G"]
["Item no.","Technical Specification","Comply (Yes/No)","Provide Equivalent/Better          (if applicable)","Comments on Equivalent/Better","Details of Product Offer                                           (Provide your answers in this Column. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification) /  Supporting Document"]
["A","Janitor Trolley complete system"]
["A.1","Industrial or heavy  duty housekeeping janitor trolley"]
["A.2","Multifunctional cleaning services cart for public areas"]
["A.3","Polypropelene or polypropene (durable material) base that is resitant to scretches and dents"]
["A.4","Steel vertical frames ( rilsan or better)"]
["A.5","Mut have two (2) big buckets and wringers"]
["A.6","Must have 1x122l vinyl waste bag and bag cover"]
["A.7","Two or more : Broom base and holder"]
["A.8","Lockable door with deep storage drawer / shelf ( to keep cleaning agents)."]
["A.9","4x colour coded 6l bucket"]
["A.10","1x full tray and 1x shallow storage "]
["B","Wheels"]
["B.1","Four (4) allterrain heavy duty castor wheels "]
["B.2","Non- marking wheels"]
["B.3","Should allow for high maneuouvrability"]
["B.4","Wheels size 20- 25 cm suitable for both inside and outside"]
["C","Dimensions"]
["C.1","Height max - 1580mm "]
["C.2","Length  max  -  1230mm"]
["C.3","Width maximum - 760mm"]
["C.4","Weight maximum - 20-50kg"]