{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"merged":[[0,1,0,3]]}
[null,"BOM -RFWT Balance Main Flow Meter Installation "]
["Item No.","Description ","Unit ","Quantity ","Rate ","Amount "]
[null,"PRELIMINARIES  AND GENERAL "]
[1,"Site Establishment for: Delivery of Kitchen Converted Container Fitted with Single Bowl Sink with a Work Top, Fitted with Undercounter Cupboard. L-6m; W-3m (Inclusive of Transportation and Handling)","Once Off",1]
[2,"Site Establishment for: Delivery of Storage Container, Enclosed with No Windows L-12m; W-2.5m (Inclusive of Transportation and Handling)","Once Off",1]
[3,"Site Establishment for: Delivery of Split Male and Female Ablution L-6m; W-3m (Inclusive of Transportation and Handling)","Once Off",1]
[4,"Site De-Establishment for: Collection of Kitchen Converted Container Fitted with Single Bowl Sink with a Work Top, Fitted with Undercounter Cupboard. L-6m; W-3m (Inclusive of Transportation and Handling)","Once Off",1]
[5,"Site De-Establishment for: Collection of Storage Container, Enclosed with No Windows L-12m; W-2.5m (Inclusive of Transportation and Handling)","Once Off",1]
[6,"Site De-Establishment for: Delivery of Split Male and Female Ablution L-6m; W-3m (Inclusive of Transportation and Handling)","Once Off",1]
[null,"Standard PPE "]
[7,"SANS standard Flame Retard PPE (1 pair per year)","No.",10]
[8,"SANS Hard Hat (1 pair  per year)","No.",10]
[9,"SANS standard eye googles (1 pair per year)","No.",10]
[10,"SANS standard safety boots (Steel toe) (1 pair per year)","No.",10]
[11,"SANS standard ear muffs (1 pair per year)","No.",10]
[12,"SANS Micro Flex Hand Gloves (1 pair per month)","No.",30]
[13,"Safety file ","No.",10]
[14,"Medicals - Entry ","Per Person ",10]
[15,"Police Clearance Certification","Per Person ",10]
[]
[null,"HIRING CONTAINER"]
[16,"Kitchen Converted Container Fitted with Single Bowl Sink with a Work top, Fitted with Undercounter Cupboard. L-6m; W-3m 9 (Hiring cost will be paid on a monthly basis) ","Monthly ",9]
[17,"Storage Container, Enclosed with No Windows L-12m; W-2.5m (Hiring cost will be paid on a monthly basis) ","Monthly ",9]
[18,"Split Male and Female Ablution Container L-6m; W-3m (Hiring cost will be paid on a monthly basis) ","Monthly ",9]
[]
[null,"HUMAN RESOURCES "]
[19,"Control System Technical Specialist Engineer -Electronic Engineering Diploma or bachelor’s degree with a minimum of 5 years. (ECSA Registered PrEng/ PrTech Eng. ) (60 days)","Hours",480]
[20,"Electrical Technical Specialist -Electronic Engineering Diploma or bachelor’s degree with a minimum of 5 years experience (ECSA Registered PrEng/ PrTech Eng. ) (60 days)","Hours",480]
[21,"ABB 800xA System Techinical Specialist -Electrical Electronic Engineering Diploma or bachelor’s degree and Diploma Industrila (20 days)","Hours",160]
[22,"Communications network and IT with a minimum of 5 years (20 days)","Hours",160]
[23,"Auto- Cad Technician - Documentation of Drawings (5-10 years experience) (60 days)","Hours",480]
[24,"Site Supervisor -Project Management with minimun 5 years experience (68 days)","Hours",544]
[25,"Safety Officer - Safety Certificate (0 to 3 years experience) (68 days) ","Hours",544]
[26,"Quality Controller/QC Inspector -Electronic Engineering Diploma or bachelor’s degree (20 days)","Hours",160]
[27,"Semi-skilled employee  (0 to 3 years experience) (68 Days) ","Hours",544]
[28,"General Workers (0 to 3 years experience) (68 Days)","Hours",544]
[]
[null," EQUIPMENT "]
[29,"Flow Meters - (Ultrasonic Flow  meter)","No",10]
[30,"Instrument Cables UVG16","M",3500]
[31,"SWA power cable","M",3500]
[32,"Size 2 cable gland","Each",50]
[33,"10A, 5kA Single pole miniature circuit breakers","Each",10]
[34,"10A, 5kA Double pole miniature circuit breakers","Each",10]
[35,"Wire mesh cable tray","M",500]
[null,"Cable Accessories "]
[36,"Cable trays 2m (Stainless Steal) 2m ","No",300]
[37,"Cable ties (Black SANS standard)","No ",2000]
[38,"Black Insulation Tape (SANS Standard)","No",100]
[39,"Cable conduits (Stainless steel) 2m","No",300]
[40,"Junction boxes (240mm by 300mm) stainless steel ","Each",10]
[]
[null,"COMMISSIONING AND TESTING "]
[41,"Commissioning and Testing (Inclusive of Report)","No.",1]