	SPECIFICATION

	
	Description
· Supply and install Sunpro vertical blinds/ blockout; color: putty corn; description – prestigious tiltrak vertical blind system. Slats 127mm, 90mm & 63mm system; standard rail is white powder coated aluminum  SABS awarded; 
·                                    And
· Supply and install Sunpro roller blinds / putty corn silk (blockout). Nylon chain controlled system that prevents the blinds from automatically rolling down. Must have an aluminum head rail system for strength and stability – Standerton office.
· Quotation to include removal of old damaged blinds and orderly disposal of material


NB:
Please note that the installation will be done in 1st floor and 2nd floor and the installation will be done after hours,
Mandatory Requirements
1. Prospective bidder to have CIDB grade 1GB and higher
2. Public Liability Insurance at R1m and above
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‘The assessment of functionality and capability will be performed in terms of the below technical evaluation

criteria
T Technical evaluation criteria Weight
Criteria o0y
Company. ‘Qualification
Experience ® 5 years’ experience in the professional installation of blinds to meet
industry standards (10) 20
Competent team, equipment and tools - CVs (10)
References | Positive Client endorsement references Letters (at least 12 months) in respect of
similar service rendered: (Detailing Value, duration, scope Of Work of the
project) From Different Clients( Reference Letters from same client will be
regarded as 1 Lefter
One reference provided (5) 20
e Two references provided (10)
Three or more references provided (15)
«  Four or more references provided (20)
Health &
Safety ©  SHEFile (Risk Assessment, Personal Protective Equipment (PPE), 30
‘Tool Inspection and COVID-19 Protocol) (15)
«  COIDA National Department of Labour (15)
Contingency | *©  The service provider needs fo provide contingency plan in cases of work | 10
Plan interruptions due to labour strikes, vehicles and equipment breakdowns
@10y
Compressive Company profile
o Lessthan 5 years® experience (5) 20
o 5years experience and above(15)
TOTAL 100





