{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["A_GENERAL","B SITE CLEARANCE ERF COLLECTORS","C EARTHWORKS WATER CONNECTIONS","D PIPEWORK WATER CONNECTIONS","E EARTHWORKS SEWER ERF COLLECTO","F PIPEWORK SEWER ERF","G BEDDING SEWER ERF","H BUILDING WORK","SUMMARY"],"not_rendered":{"external_links":1,"defined_names":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"A_GENERAL","index":0,"n_rows":201,"n_cols":7,"rows_kept":201,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SANS 1200A","SECTION A: GENERAL "]
[null,"SANS 1200 AB","  "]
["A1","PSA 8.2.1","SCHEDULED FIXED-CHARGE AND VALUE-RELATED ITEMS"]
[]
["A1.1","PSA 8.3.1","Contractual Requirements","Sum","-","-"]
[]
["A1.2","PSA 8.3.1a","Contractors all risk insurance provided by Contractor (if not by Council as stated in Part T1.3 clause2.9 and Part C1.2 )"," Sum","-","-"]
[]
[null,"PSA 8.3.2","Establishment of Facilities on the Site"]
[]
["A2","PSA 8.3.2.1","Facilities for Engineer"]
[null,"PS7.1,PS7.2"]
["A2.1","PSAB 3.2","Furnished office for Resident Engineer suitable for site meetings"," Sum","-","-"]
[]
["A2.2","PSAB 8.1","One Cellular phone "," Sum","-","-"]
[]
["A2.3","PSAB 3.1 PSAB 5.1","Nameboards as per drawing (2No)"," Sum","-","-"]
[]
["A2.4","PSAB5.5,  5.6","Two survey assistants and equipment"," Sum","-","-"]
[]
["A2.5","PSAB 3.2 ","One Carport as specified"," Sum","-","-"]
[]
["A2.6","PS15          PSA 8.3.2.1","Provision of monthly as-built\" records to the Engineer\""," Sum","N/A","N/A","N/A"]
[]
["A2.7",null,"Ablution and latrine facilities","Sum","-","-"]
[]
["A3","8.3.2.2","Facilities for Contractor"]
[]
["A3.1","PS 6.2      PSA 4.2","Offices and storage sheds"," Sum","-","-"]
[]
["A3.2",null,"Workshops"," Sum","-","-"]
[]
["A3.3","PS 6.3","Living accommodation"," Sum","-","-"]
[]
["A3.4","PS7.3","Ablution and latrine facilities"," Sum","-","-"]
[]
["A3.5",null,"Tools and equipment"," Sum","-","-"]
[]
["A3.6","PS 6.1","Water supplies, electric power and communications"," Sum","-","-"]
[null,"PS7.3"]
["A3.7","8.3.2.2","Dealing with water (Subclause 5.5)"," Sum","-","-"]
[]
["A3.8","PS8.1","Access (Subclause 5.8)"," Sum","-","-"]
[]
["A3.9","PSA8.4.2.2","One facsimile facility"," Sum","N/A","N/A","N/A"]
[]
["TOTAL CARRIED FORWARD"]
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["BROUGHT FORWARD"]
[null,"SANS 1200 A  SANS 1200 AB"]
[]
["A3.10","PSA 8.4.2.2","Digital camera to take digital photographs of existing stuctures, obstructions and services and submit to the Engineer"," Sum","-","-"]
[]
[]
["A4","8.3.3 ","Other fixed-charge obligations"," Sum","-","-"]
[]
["A5","8.3.4","Removal of Site Establishment"," Sum","-","-"]
[]
["A6","PSA 8.4  ","SCHEDULED TIME-RELATED ITEMS"]
[]
["A6.1","8.4.1","Contractual Requirements","Month","………"]
[]
[null,"8.4.2","Operation and Maintenance of Facilities on Site, for Duration of Construction, except where otherwise stated"]
[]
["A6.2","PSA 8.4.2.1","Facilities for Engineer"]
[]
["A6.2.1","PSAB 3.2","Furnished office for Resident Engineer suitable for site meetings","Month","………"]
[]
["A6.2.2","PSAB 8.1","One Cellular phone","Month","………"]
[]
["A6.2.3","PSAB 3.1 PSAB 5.1","Nameboards as per drawing (2No)","Month","………"]
["A6.2.4","PSAB 5.5,  5.6","Two survey assistants and equipment","Month","………"]
[]
["A6.2.5","PSAB 3.2","One Carport as specified","Month","………"]
[]
["A6.2.6","PS 15                PSA 8.3.2.1","Provision of monthly as-built\" records to the Engineer\"","Month","N/A","N/A","N/A"]
[]
["A6.2.7",null,"Ablution and latrine facilities","Month","………"]
[]
["A6.3","PSA 8.4.2.2","Facilities for Contractor"]
[]
["A6.3.1","PS 6.2              PSA 4.2","Offices and storage sheds","Month","………"]
[]
["A6.3.2",null,"Workshops","Month","………"]
[]
["A6.3.3","PS 6.3","Living accommodation","Month","………"]
[]
["A6.3.4","PS7.3","Ablution and latrine facilities","Month","………"]
[]
["A6.3.5",null,"Tools and equipment","Month","………"]
[]
[]
["TOTAL CARRIED FORWARD"]
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["BROUGHT FORWARD"]
[]
["A6.3.6","PS 6.1 PS7.3","Water supplies, electric power and communications","Month","………"]
[]
["A6.3.7","8.3.2.2  PS8.11","Dealing with water (Subclause 5.5)","Month","………"]
[]
["A6.3.8","PS 8.1","Access (Subclause 5.8)","Month","………"]
[null,"8.3.2.2"]
["A6.3.9",null,"One facsimile facility","Month","N/A","N/A","N/A"]
[]
["A6.3.10","PSA 8.4.2.2","Digital camera to take digital photographs of existing stuctures and obstructions on the pipeline routes and submit to Engineer","Month","………"]
[]
["A6.3.11","8.4.3","Supervision for Duration of Construction","Month","………"]
[]
["A6.3.12","8.4.4","Company and Head Office Overhead Costs for the Duration of the Contract","Month","………"]
[]
["A6.3.13","8.4.5 ","Other Time-related Obligations","Month","………"]
[]
["A7","PSA 8.5 8.5","SUMS STATED PROVISIONALLY BY ENGINEER"]
[]
["A7.1","PSAB8.2","Provide allowance for Engineer's vehicle","Prov Sum","-","-",{"v":60000,"d":"60,000.00"}]
[]
["A7.1.1",null,"Contractor's cost and profit on item A7.1","%",{"v":60000,"d":"60,000.00"}]
[]
["A7.2","PSAB8.3","Electronic equipment for the Engineer","Prov Sum","-","-",{"v":30000,"d":"30,000.00"}]
[]
["A7.2.1",null,"Contractor's cost and profit on item A7.2","%",{"v":30000,"d":"30,000.00"}]
[]
["A7.3","PSAB8.4","Accommodation for the Engineer","Prov Sum","-","-",{"v":100000,"d":"100,000.00"}]
[]
["A7.3.1",null,"Contractor's cost and profit on item A7.3","%",{"v":100000,"d":"100,000.00"}]
[]
["A7.4","PSAB8-1","Allow for cellphone costs by the Engineer","Prov Sum","-","-",{"v":12000,"d":"12,000.00"}]
[]
["A7.4.1",null,"Overheads, charges and profit on item A7.4 above","%",{"v":12000,"d":"12,000.00"}]
[]
["A7.5","PSA 8.5","Provision for dayworks","Prov Sum","-","-",{"v":50000,"d":"50,000.00"}]
[]
["A7.5.1",null,"Overheads, charges and profit on item A7.5 above","%",{"v":50000,"d":"50,000.00"}]
[]
[null,"PSA 8.6","PRIME COST ITEMS"]
[]
["A7.6","PS8.6.2","Additional quality control test by approved laboratory instructed by the Engineer. (The cost of tests not conforming to standards shall not be included for payment)","PC Sum","-","-",{"v":15000,"d":"15,000.00"}]
[]
["A7.7",null,"Contractor's superintendance and administration of item A7.6 above"," %",{"v":15000,"d":"15,000.00"}]
[]
["TOTAL CARRIED FORWARD"]
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["BROUGHT FORWARD"]
[null,"PSA 8.8,DB8.3.7","TEMPORARY WORKS"]
["A7.8","PSA 8.8.2","Accommodation of traffic "," Sum","-","-"]
[]
[null,"PSA 8.8.4","Existing Services"]
[]
["A7.9","PSA5.4.3 PSA8.15","Alterations to existing services by authorities","PC Sum","-","-",{"v":250000,"d":"250,000.00"}]
[]
["A7.9.1",null,"Overheads,charges and profit"]
[null,null,"on item 7.9","%",{"v":250000,"d":"250,000.00"}]
[]
["A7.10","PSA8.8.4","Excavation by hand in soft material"]
[null,null,"to expose existing services","m3",50]
[]
["A7.11","PSA 5.4","Temporary protection, as required in terms of the project specification, of exposed services"," Sum","-","-"]
[]
["A7.12","PSA 8.8.5","Cost of Survey in Terms of the Land Survey Act"," Sum","-","-"]
[]
[null,"PSA 8.9","ADDITIONAL SURVEY"]
[]
["A7.13",null,"As instructed by the Engineer","PC Sum","-","-",{"v":20000,"d":"20,000.00"}]
[]
["A7.13.1",null,"Overheads, charges and profit on item A7.13 above","%",{"v":20000,"d":"20,000.00"}]
[]
["A8","PSA 8.11","MANAGEMENT OF SUBCONTRACTS","Month","………"]
[]
["A9",null,"HEALTH AND SAFETY"]
[]
["A9.1","PS8.7 PS8.9","Compliance with OHS Act and Regulations (Including the construction regulations 2003)","Sum","-","-"]
[]
["A9.1.1",null,"Allow for safety equipment for Sub-contractors","Prov Sum","-","-",{"v":100000,"d":"100,000.00"}]
[]
["A9.1.2",null,"Allow for medical fitness assesment of all workers","Prov Sum","-","-",{"v":50000,"d":"50,000.00"}]
[]
["A9.1.3",null,"Overheads, charges and profit on item A9.1.1 & A9.1.2 above","%",{"v":150000,"d":"150,000.00"}]
[]
["A10","PSA 8.10","TRAINING COURSES"]
[]
["A10.1",null,"Cost of Course","PC Sum","-","-",{"v":50000,"d":"50,000.00"}]
[]
["A10.2",null,"Handling cost and profit on item A10.1","%",{"v":50000,"d":"50,000.00"}]
[]
["A11",null,"COMMUNITY LIAISON OFFICER (CLO)"]
[]
["A11.1",null,"Allow for remuneration of community"]
[null,null,"liaison officer CLO","PC Sum","-","-",{"v":60000,"d":"60,000.00"}]
[]
["A11.2",null,"Handling cost and profit on item A10.1","%",{"v":60000,"d":"60,000.00"}]
[]
["A12",null,"PROJECT LIAISON COMMITTEE (PLC)"]
[]
["A12.1",null,"Allow for PLC costs","PC Sum","-","-",{"v":60000,"d":"60,000.00"}]
[]
["A12.2",null,"Handling cost and profit on item A11.1","%",{"v":60000,"d":"60,000.00"}]
[]
["A13","PSPA4","SITE FINISHING","Sum","-","-"]
["TOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"B SITE CLEARANCE ERF COLLECTORS","index":1,"n_rows":51,"n_cols":7,"rows_kept":51,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"SANS 1200 C","SECTION B: SITE CLEARANCE"]
[null,null,"(ERF SEWER AND WATER)"]
["B1","8.2 (L)","SCHEDULED ITEMS"]
[]
["B1.1","8.2.1 PSC 3.1","Clear and grub site","m2",{"v":11664,"d":"11,664"}]
[null,"PSC 5.1"]
[]
[null,"PSG8.2.5 PSC5.8","Take down existing fences and re-erect after completion of the works to original state"," m",{"v":7290,"d":"7,290"}]
[]
["B2","(L) PSC8.2.8","Demolish and remove structures/buildings and cart away unwanted material to spoil at dumpsite"," "]
[]
["B2.1",null,"a) Informal toilet structures and buildings smaller than 2,5m² irrespective of type of material"," No",450]
[]
["B2.2",null,"b) Buildings larger than 2,5 m² irrespective of type of material","No",36]
{"$rows_empty":35}
["TOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"C EARTHWORKS WATER CONNECTIONS","index":2,"n_rows":38,"n_cols":7,"rows_kept":38,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"SANS 1200 DB","SECTION C: EARTHWORKS (WATER CONNECTIONS)"]
[]
["C1",8.2,"SCHEDULED ITEMS"]
[]
[null,"PSDB8.3.2 PS 3 PS12","Excavation (PS DB 8.3.3.4)"]
[]
[null,"PSDB8.2.4 PSLB3.4.1"]
[]
[null,"PSDB 8.3.2  (L)","a) Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for 20-25mm Hdpe type iv pipes"]
[]
["C1.1",null,"1) Exceeding 0,0m but not exceeding 1,0m"," m³",875]
[]
["C1.2",null,"2) Exceeding 1,0m but not exceeding 2,0m"," m³","N/A","N/A","N/A"]
[]
["C1.3","PSAB 8.1","3) Exceeding 2,0m but not exceeding 3,0m"," m³","N/A","N/A","N/A"]
[]
["C2","PSDB 3.1      (L)","b) Extra-over items a) above for"]
[]
["C2.1",null,"1) Intermediate material"," m³",157]
[]
["C2.2",null,"2) Hard rock material"," m³",105]
[]
["C2.3","PLIS","3) Excavation in soft material by labour based methods for trenches shallower than 1,5m. Compaction by labour based methods is excluded."," m³",875]
[]
["C2.4","PSDB 5.5 ","c) Excavate and dispose of unsuitable material from trench bottom (provisional)"," m³","N/A","N/A","N/A"]
[]
["C2.5",null,"d) Hand excavation to expose existing services in a careful manner "," m³",75]
{"$rows_empty":9}
["TOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"D PIPEWORK WATER CONNECTIONS","index":3,"n_rows":41,"n_cols":7,"rows_kept":41,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"SANS 1200 LF","SECTION D: PIPEWORK (WATER CONNECTIONS)"]
[]
["D1",8.2,"SCHEDULED ITEMS"]
[null,"PSLF 8.2.1                     (L)","Provide Erf Connections Complete as per Drawing"]
[]
[null,null,"1) Erf Connections:"]
[]
[null,null,"a) Double Short"," No","N/A","N/A","N/A"]
[]
["D1.2",null,"b) Double Long"," No","N/A","N/A","N/A"]
[]
[null,null,"c) Single Long"," No","N/A","N/A","N/A"]
[]
["D1.4",null,"d) Single Short"," No","N/A","N/A","N/A"]
[null,"PSAB 8.1"]
[null,null,"2) Future Water Connections:"]
[]
["D1.5",null,"a) Future business","No","N/A","N/A","N/A"]
[]
["D1.6",null,"b) Future park","No","N/A","N/A","N/A"]
[]
["D1.7",null,"3) Standpipe complete as per drawing","No","N/A","N/A","N/A"]
[]
[null,null,"Pipes for erf connections"]
[]
["D2.1",null,"a) 20 mm ø HDPE/10 Type IV between meterbox and toilet structure","m",{"v":14580,"d":"14,580"}]
[]
["D2.2",null,"b) Extra-over Item a) for the removal of the elbow at the existing standpipe and the supply and installation of 20 mm ø galvanized T-piece complete including excavation and backfilling","No",482]
[]
["D3",null,"Miscellaneous"]
[]
["D3.1",null,"Alterations to water supply system","Prov Sum","-","-",{"v":500000,"d":"500,000.00"}]
[]
["D3.2",null,"Overheads, charges and profit on item H6.1 above","%",{"v":500000,"d":"500,000.00"}]
[]
[]
[]
[]
[]
["TOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"E EARTHWORKS SEWER ERF COLLECTO","index":4,"n_rows":162,"n_cols":7,"rows_kept":162,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"SANS 1200 D","SECTION E: EARTHWORKS (SEWER ERF COLLECTORS)"]
[]
["E1","PSD 8.3.14","Backfill of pit latrine holes"," m³","N/A","N/A","N/A"]
[]
[null,"SABS 1200 DB","EARTHWORKS (PIPE TRENCHES)"]
[]
["E2","8.2 PS 8.8","SCHEDULED ITEMS"]
[]
[null,"PSDB8.3.2 PS 3","Excavation (PS DB 8.3.3.4)"]
[null,"PSDB8.2.4 PSLB3.4.1"]
[null,"PSDB 8.3.2","a) Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for pipes up to 110mm dia. for total trench depth"]
[]
["E2.1","PSAB 8.1","1) Exceeding 0,0m but not exceeding 1,0m"," m³",{"v":1778,"d":"1,778"}]
[]
["E2.2","PSAB 8.1","2) Exceeding 1,0m but not exceeding 2,0m"," m³",742]
[]
["E2.3",null,"3) Exceeding 2,0m but not exceeding 3,0m"," m³","N/A","N/A","N/A"]
[]
[null,"PSDB 3.1","b) Extra-over items a) above for"]
[]
["E2.4",null,"1) Intermediate material"," m³",{"v":1008,"d":"1,008"}]
[]
[null,null,"2) Hard rock material"," m³",630]
[]
["E2.5","PLIS(L)","3) Excavation in soft material by labour based methods for trenches shallower than 1,5m. Compaction by labour based methods is excluded."," m³","N/A","N/A","N/A"]
[]
["E2.6","PSDB 5.5 ","c) Excavate and dispose of unsuitable material from trench bottom (provisional)"," m³",50]
[]
["E2.7",null,"d) Hand excavation to expose existing services in a careful manner "," m³",75]
[]
[]
[]
["TOTAL CARRIED FORWARD TO SUMMARY"]
{"$rows_empty":89}
[null,"PSAB8.2"]
[]
[]
[]
[null,"PSAB8.3",{"$nulls":4},{"v":20000,"d":"20,000.00"}]
[]
[]
[]
[null,"PSAB8.4"]
[]
[]
[]
[null,"PSAB8-1"]
{"$rows_empty":22}
[{"$nulls":6},"250.000.00"]
[]
[]
[{"$nulls":4},"250,000.00"]

{"sheet":"F PIPEWORK SEWER ERF","index":5,"n_rows":170,"n_cols":7,"rows_kept":170,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"SANS 1200 LD","SECTION F: PIPEWORK (SEWER ERF COLLECTORS)"]
[]
["F1",8.2,"SCHEDULED ITEMS"]
[]
[null,"8.2.1 (L)","Supply, Lay, Joint, Bed and Test 110ø Pipeline using:"]
[null,"PSLD8"]
["F1.1",null,"i) uPVC Solid Wall Class 34"," m","N/A","N/A","N/A"]
[]
["F1.2",null,"ii) uPVC Structured Wall Class 400","m","N/A","N/A","N/A"]
[]
["F1.3",null,"iii) \"Ultrapipe\" or similar approved (Solid Wall, class 400)"," m",{"v":6761,"d":"6,761"}]
[]
["F2","8.2.2 (L)","Extra-Over Item 8.2.1 for Specials:"]
[null,"PSLD8.2.2"]
[null,null,"a) Rodding eye (complete with fire hydrant box) using:"," "]
[null,"PSAB 8.1"]
["F2.1",null,"i) uPVC Solid Wall Class 34","No","N/A","N/A","N/A"]
[]
["F2.2",null,"ii) uPVC Structured Wall Class 400","No","N/A","N/A","N/A"]
[]
["F2.3",null,"iii) \"Ultrapipe\" or similar approved (Solid Wall, class 400)","No",244]
[]
[null,null,"b) 110ø plain 45 deg junction using:"," "]
[]
["F2.4",null,"i) uPVC Solid Wall Class 34","No","N/A","N/A","N/A"]
[]
["F2.5",null,"ii) uPVC Structured Wall Class 400","No","N/A","N/A","N/A"]
[]
["F2.6",null,"iii) \"Ultrapipe\" or similar approved (Solid Wall, class 400)","No",972]
[]
[null,null,"c) 110ø I.E. 45 deg junction using:"," "]
[]
["F2.7",null,"i) uPVC Solid Wall Class 34","No","N/A","N/A","N/A"]
[]
["F2.8",null,"ii) uPVC Structured Wall Class 400","No","N/A","N/A","N/A"]
[]
["F2.9",null,"iii) \"Ultrapipe\" or simmilar approved (Solid Wall, class 400)","No",482]
[]
[null,null,"d) 110ø 45 deg bend using:"]
[]
["F2.10",null,"i) uPVC Solid Wall Class 34","No","N/A","N/A","N/A"]
[]
["F2.11",null,"ii) uPVC Structured  Wall Class 400","No","N/A","N/A","N/A"]
[]
["F2.12",null,"iii) \"Ultrapipe\" or similar approved (Solid Wall, class 400)","No",{"v":1215,"d":"1,215"}]
[]
[null,null,"e) 160 x 110ø un-equal Y-junction using:"]
["F2.13",null,"i) uPVC Solid Wall Class 34","No","N/A","N/A","N/A"]
[]
["F2.14",null,"ii) uPVC Structured  Wall Class 400","No","N/A","N/A","N/A"]
[]
["F2.15",null,"iii) \"Ultrapipe\" or similar approved (Solid Wall, class 400)","No",122]
[]
["F2.16",null,"110mm End Caps","No",482]
[]
["F2.17",null,"Marker Posts as per detail drawing 20251/ES/700","No",482]
["TOTAL CARRIED FORWARD TO SUMMARY"]
{"$rows_empty":73}
[null,"PSAB8.2"]
[]
[]
[]
[null,"PSAB8.3",{"$nulls":4},{"v":20000,"d":"20,000.00"}]
[]
[]
[]
[null,"PSAB8.4"]
[]
[]
[]
[null,"PSAB8-1"]
{"$rows_empty":22}
[{"$nulls":6},"250.000.00"]
[]
[]
[{"$nulls":4},"250,000.00"]

{"sheet":"G BEDDING SEWER ERF","index":6,"n_rows":48,"n_cols":7,"rows_kept":48,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"SANS 1200 LB","SECTION G: BEDDING (SEWER ERF COLLECTORS)"]
[]
["G1",null,"SCHEDULED ITEMS"]
[]
[null,"8.2.1 PSLB3.4.1","Provision of Bedding from Trench Excavation with unlimited free haul distance"]
[]
[null,"PSLB8.1.6"]
[]
["G1.1","8.2.1","a) Selected granular material"," m³","N/A","N/A","N/A"]
[]
["G1.2","PSLB 5.1.3.5","b) Selected fill material"," m³","N/A","N/A","N/A"]
[]
[null,"8.2.2 (L)","Supply only of Bedding by Importation"]
[]
[null,"PSAB 8.1","From Commercial sources (Provisional)"]
[]
["G1.3",null,"a) Selected granular material"," m³",365]
[]
["G1.4","PSLB 5.1.3.5","b) Selected fill material"," m³",{"v":1094,"d":"1,094"}]
{"$rows_empty":27}
["TOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"H BUILDING WORK","index":7,"n_rows":46,"n_cols":7,"rows_kept":46,"flags":["formulas_cached_only"]}
["ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,null,"SECTION H : BUILDING WORK (TOILET STRUCTURES)"]
[]
["H1","PSPC","BUILDING WORK"]
[]
[null,"PSPC 6.2.1   (L)","New toilet structure, complete as shown on drawings"," "]
[]
["H1.1",null,"a) Groundworks and floorslab","No",482]
[]
["H1.2",null,"b) Brickwork and galvanized door","No",482]
[]
["H1.3",null,"c) Concrete roof slab","No",482]
[]
["H1.4",null,"d) Doorstop","No",482]
[]
["H2",null,"Disabled toilet structure, complete as shown on drawings including hand rails"," No",1]
[]
["H3","PSPC 6.2.3 (L)","Flush toilet sets"]
[]
["H3.1",null,"a) White glazed vitreous china"," No","N/A","N/A","N/A"]
[]
["H3.2",null,"b) Rotomoulded polyethylene (as alternative)"," No","N/A","N/A","N/A"]
[]
["H3.3",null,"c) Vaal Sanitaryware \"Aquasave Slimline suite consisting of a vitreous china 90deg out washdown pan and matching 9 litre SISO polyporpylene to-flush cistern complete with lid, fitment and flushpipe (Prouduct code 750152) or similar approved.","No",486]
[]
["H4","PSPC 6.2.4 ","Wash trough"]
[]
["H4.1",null,"(a) Stainless steel"," No",486]
[]
["H4.2",null,"(b) Rotomoulded polyethylene (as alternative)"," No","N/A","N/A","N/A"]
[]
["H4.3",null,"(c) Fibre-cement (as alternative)"," No","N/A","N/A","N/A"]
[]
["H5","PSPC 6.2.5","Plumbing to Toilet"]
[]
["H5.1",null,"a) Sanitation complete as per drawing","No",486]
[]
["H5.2",null,"b) Water complete as per drawing","No",486]
[]
["H6",null,"Miscellaneous"]
[]
["H6.1",null,"Refurbishments at waste water treatment works","Prov Sum","-","-",{"v":1500000,"d":"1,500,000.00"}]
[]
["H6.2",null,"Overheads, charges and profit on item H6.1 above","%",{"v":1500000,"d":"1,500,000.00"}]
[]
["TOTAL CARRIED FORWARD TO SUMMARY "]

{"sheet":"SUMMARY","index":8,"n_rows":37,"n_cols":3,"rows_kept":37,"merged":[[1,0,1,2]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF QUANTITIES"]
["SECTION","DESCRIPTION","AMOUNT"]
["A","GENERAL"]
[]
["B","SITE CLEARANCE ERF COLLECTORS"]
[]
["C","EARTHWORKS WATER CONNECTIONS"]
[]
["D","PIPEWORK WATER CONNECTIONS"]
[]
["E","EARTHWORKS SEWER ERF COLLECTORS"]
[]
["F","PIPEWORK SEWER ERF COLLECTORS"]
[]
["G","BEDDING SEWER ERF COLLECTORS"]
[]
["H","BUILDING WORK (TOILETS)"]
[]
[null,"TOTAL OF PRICED ITEMS"]
[]
["CALCULATION OF TENDER SUM"]
[]
["NETT TOTAL OF TENDER","R"]
["ADD 10% CONTINGENCIES","R"]
[]
["SUB-TOTAL","R"]
[]
["ADD 15% VAT","R"]
[]
["TOTAL TENDER AMOUNT","R"]
[]
["SIGNATURE OF TENDERER:"]
[]
["SIGNED ON BEHALF OF:"]
[]
["DATE:"]