{"text_format":"3","workbook":"xls","n_sheets":13,"sheets":["CHAPTER 1","CHAPTER 2","CHAPTER 3","CHAPTER 4","CHAPTER 5","CHAPTER 6","CHAPTER 11","CHAPTER 20","1200DB","1200LB","Summary of Schedule","Socio-Economic","Summary of_Schedule"],"not_rendered":{"external_links":1,"defined_names":13},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CHAPTER 1","index":0,"n_rows":309,"n_cols":8,"rows_kept":309,"merged":[[17,2,17,3],[19,2,19,3],[21,2,21,3],[22,2,22,3],[49,2,49,3],[51,2,51,3],[53,2,53,3],[55,2,55,3],[88,2,88,3],[118,1,118,3],[135,1,135,2],[137,1,137,2],[139,1,139,2],[141,1,141,2],[142,1,142,3],[143,1,143,3],[145,1,145,3],[149,1,149,3]],"flags":["formulas_cached_only"]}
[{"$nulls":7},"CHAPTER 1"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C1.2","GENERAL REQUIREMENTS AND"]
[null,"PROVISIONS"]
[]
["C 1.2.4","Stake holders Liaison"]
[]
["SDA 8.10","Remuneration of the Project Liaison "]
[null,"Officer and members of the Project "]
[null,"Liaison Committee:"]
[]
[null,"(a)","Project  Liaison Officer",null,"month",null,{"v":6500,"d":"R 6,500.00"}]
[]
[null,"(b)","Project Liaison Committee",null,"-","Prov","Sum",{"v":30000,"d":"R 30,000.00"}]
[]
[null,"(c)","Training",null,"-","Prov","Sum",{"v":100000,"d":"R 100,000.00"}]
[]
[null,"(c)","Handling costs and profit with respect to "]
[null,null,"item B12.02(a) & (b) SDA 8.10 (a), (b) & (c)",null,"%"]
[]
["C 1.2.5","Safety"]
[]
["C 1.2.5.1","Health and safety plan",null,null,"lump Sum",1]
[]
["C 1.2.5.2","Implementation of health and safety plan",null,null,"month"]
[]
["C 1.2.6","Work adjacent to properties"]
[]
["C 1.2.6.2","Prevention and/or mitigation measures",null,null,"-","Prov","Sum",{"v":20000,"d":"R 20,000.00"}]
[]
["C 1.2.6.3","Handling costs, profit and all other charges in"]
[null," respect of item C1.2.6.2",null,null,"%",null,{"v":20000,"d":"R 20,000.00"}]
[]
["C 1.2.8","Dayworks"]
[]
["C 1.2.8.1","Personnel"]
[]
[null,"(a)","Unskilled Labourer",null,"hour",8]
[]
[null,"(b)","Semi-Skilled Labourer",null,"hour",8]
[]
[null,"(c)","Skilled Labourer",null,"hour",8]
[]
["C 1.2.8.2","Construction equipment"]
[]
[null,"(e)","TLB (CAT 416 or similar)",null,"hour",8]
[]
[null,"(f)","Excavator",null,"hour",8]
[]
[null,"(g)","Compressor plus jackhammer",null,"hour",8]
[]
[null,"(h)","Watercart (10 000 litre)",null,"hour",8]
[]
[null,"(i)","Other equipment"]
[]
[]
["C 1.2","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 1"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C1.2","Brought forward"]
[]
[]
[null,null,"(ii) Grid roller",null,"hour",8]
[]
[null,null,"(iii) Other equipment",null,"hour",8]
[]
["C 1.2.8.3","Vehicles"]
[]
[null,"(a)","Light Vehicle",null,"km",1.1]
[]
[null,"(b)","Flatbed Truck",null,"km",1.1]
[]
[null,"(c)","Dump Truck",null,"km",1.1]
[]
[null,"(d)","Other Vehicles",null,"km",1.1]
[]
["C 1.2.8.4","Materials"]
[]
[null,"(a)","Procurement of materials",null,"-","Prov","Sum",{"v":20000,"d":"R 20,000.00"}]
[]
[null,"(b)","Contractor's handling costs, profit and "]
[null,null,"all other charges in respect of "]
[null,null,"subitem B18.03(a)",null,"%",null,{"v":20000,"d":"R 20,000.00"}]
[]
["C 1.2.9","Disposal of non- usable material;"]
[]
["C 1.2.9.2","Material not identified at the time of tender",null,null,"-","Prov","Sum",{"v":10000,"d":"R 10,000.00"}]
[]
["C 1.2.9.3","handling costs, profit and all other charges in"]
[null," respect of subitem C 1.2.9.2",null,null,"%",null,{"v":10000,"d":"R 10,000.00"}]
[]
["C 1.3","CONTRACTOR'S ESTABLISHMENT ON "]
[null,"SITE AND GENERAL OBLIGATIONS"]
[]
["C 1.3.1","The Contractor's general obligations:"]
[]
["C 1.3.1.1","Fixed obligations",null,null,"lump sum",1]
[]
["C 1.3.1.2","Value-related obligations",null,null,"lump sum",1]
[]
["C 1.3.1.3","Time-related obligations",null,null,"month"]
[]
["C 1.3.2","Contract sign board",null,null,"m²",30]
[]
["C 1.4","FACILITIES FOR THE ENGINEER"]
[]
["C1.4.1","Site Accomodation "]
[]
["C1.4.1.1","Offices and conference room",null,null,"No",2]
[]
[]
[]
["C 1.4","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 1"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 1.4","Brought forward"]
[]
[]
["C1.4.1.2","Laboratories",null,null,"No",1]
[]
["C1.4.1.5","Store rooms inside the laboratory",null,null,"No",1]
[]
["C1.4.1.6","Car ports",null,null,"No",2]
[]
["C1.4.1.7","Ablution unit (equipped as specified)",null,null,"month"]
[]
["C1.4.1.13","Rented housing paid for by the Contractor "]
[null,"(Engineers Accomodation)",null,null,"-","Prov","Sum",{"v":50000,"d":"R 50,000.00"}]
[]
["C1.4.1.14","Contractor's handling costs, profit and all other charges in respect of item C1.4.1.13",null,null,"%",null,{"v":50000,"d":"R 50,000.00"}]
[]
["C 1.4.3","Items mearsured by number"]
[]
["C1.4.3.1","Office swivel chair",null,null,"No",1]
[]
["C1.4.3.5","Office desk with 3 drawers  (at least one "]
[null,"lockable drawer)",null,null,"No",1]
[]
["C 1.4.3.8","Conference table",null,null,"No",1]
[]
["C 1.4.3.10","Steel filing cabinets with drawers",null,null,"No",1]
[]
["C 1.4.3.13","220/250 volt power points",null,null,"No",2]
[]
["C 1.4.3.17","Double 80 watt fluorescent light fittings "]
[null,"complete with 100 watt globes",null,null,"No",1]
[]
["C 1.4.3.19","Wash hand basins complete with taps and drains",null,null,"No",1]
[]
["C 1.4.3.23","Fire extinguishers, 9,0kg, all purpose dry powder "]
[null,"type, complete, mounted on wall with brackets.",null,null,"No",1]
[]
["C 1.4.3.24","Air-conditioning units with, 2,2 kW minimum "]
[null,"capacity, mounted and with own power "]
[null,"connection",null,null,"No",1]
[]
["C 1.4.3.31","Rain Gauge",null,null,"No",1]
[]
["C 1.4.3.36","Measuring wheel",null,null,"No",1]
[]
["C 1.4.3.37","First Aid kit",null,null,"No",1]
{"$rows_empty":7}
["C 1.4","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 1"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 1.4","Brought forward"]
[]
[]
["C1.4.4","Prime-cost items and items paid for in "]
[null,"lump sum:"]
[]
["C 1.4.4.1","Provision of cellphones including pro-rata "]
[null,"rentals, and the cost of phone calls in conne-"]
[null,"ction with the administration of the contract",null,null,"PC Sum",1,{"v":20000,"d":"R 20,000.00"},{"v":20000,"d":"R 20,000.00"}]
[]
["C 1.4.4.2","Handling cost and profit in respect of item "]
[null,"C 1.4.4.1",null,null,"%",null,{"v":20000,"d":"R 20,000.00"}]
[]
["C 1.4.4.3","The provision of a direct independent teleph-"]
[null,"one line for the Engineer, including the monthly "]
[null,"rental charges and the cost of business calls",null,null,"PC Sum",1,{"v":1500,"d":"R 1,500.00"},{"v":1500,"d":"R 1,500.00"}]
[]
["C 1.4.4.6","Handling cost and profit in respect of item ",null,null,"%",null,{"v":1500,"d":"R 1,500.00"}]
[null,"C 1.4.4.3"]
[]
["C 1.4.4.5","The provision of internet connectivity and WiFi "]
[null,"data for Engineer’s site staff ",null,null,"PC Sum",1,{"v":15000,"d":"R 15,000.00"},{"v":15000,"d":"R 15,000.00"}]
[]
["C 1.4.4.6","Handling cost and profit in respect of item "]
[null,"C 1.4.4.5",null,null,"%",null,{"v":15000,"d":"R 15,000.00"}]
[]
["C 1.4.4.7","The provision of paper and ink for a "]
[null,"combination colour printer/copier/scanner ",null,null,"PC Sum",1,{"v":10000,"d":"R 10,000.00"},{"v":10000,"d":"R 10,000.00"}]
[]
["C 1.4.4.8","Handling cost and profit in respect of item "]
[null,"C 1.4.4.7",null,null,"%",null,{"v":10000,"d":"R 10,000.00"}]
[]
["C 1.4.4.9","The provision of a complete 220/250 volt single "]
[null,"electrical power installation, including all poles, "]
[null,"phase insulators, wiring, switchboards, main"]
[null,"connections, meters etc. ",null,null,"PC Sum",1,{"v":20000,"d":"R 20,000.00"},{"v":20000,"d":"R20,000.00"}]
[]
["C 1.4.4.10","Handling cost and profit in respect of item"]
[null," C 1.4.4.9",null,null,"%",null,{"v":20000,"d":"R 20,000.00"}]
[]
["BC1.4.4.17","Provision for one Laptop for the engineer",null,null,"PC Sum",1,{"v":20000,"d":"R 20,000.00"},{"v":20000,"d":"R 20,000.00"}]
[]
[null,"Handling cost and profit in respect of subitem "]
[null,"14.03 (b)(v) above",null,null,"%",null,{"v":20000,"d":"R 20,000.00"}]
[]
["C 1.4.5","Services at site offices, laboratories and "]
[null," site accomodation"]
[]
["C 1.4.5.1","Fixed Costs",null,null,"sum",1]
[]
[]
[]
[]
["C 1.5","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 1"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 1.5","Brought forward"]
[]
[]
["C 1.4.5.2","Running costs",null,null,"month"]
[]
["BC1.4.4.11","Engineers travelling on site",null,null,"-","Prov","Sum",{"v":50000,"d":"R 50,000.00"}]
[]
[null,"Handling cost and profit in respect of subitem "]
[null,"14.11 above",null,null,"%",null,{"v":50000,"d":"R 50,000.00"}]
[]
["C1.5","ACCOMMODATION OF TRAFFIC"]
[]
["C1.5.1","Accommodating of pedestrian and non-"]
[null,"motorised traffic "]
[]
["C1.5.1.1","Accommodation of pedestrian and non-",null,null,"month"]
[null,"motorised traffic"]
[]
["C1.5.2","Accommodation of vehicular traffic",null,null,"month"]
[]
["C1.5.4","Construction of temporary deviations",null,null,"km",1.1]
[]
["C1.5.5","Maintenance of temporary deviations"]
[]
["C1.5.5.9","Grading of temporary deviations and "]
[null,"existing roads used as detours",null,null,"km",1.1]
[]
["C1.5.5.10","Watering of temporary deviations and "]
[null,"existing roads used as detours",null,null,"kl",100]
[]
["C1.5.5.11","Other road maintenance work ordered"]
[null," by the Engineer ",null,null,"-","Prov","Sum",{"v":15000,"d":"R 15,000.00"}]
[]
["C1.5.5.12","Handling cost, profit and all other charges "]
[null,"in respect of item C1.5.6.11 ",null,null,"%",null,{"v":15000,"d":"R 15,000.00"}]
[]
["C1.6.1","CLEARING "]
[]
["C1.6.1.1","Clearing with machines and some hand labour "]
[null,"where necessary",null,null,"ha",{"v":0.8,"d":"0.80"}]
[]
["C1.6.1.2","Clearing with hand labour only when labour "]
[null,"enhanced work is specified",null,null,"ha",{"v":0.8,"d":"0.80"}]
[]
["C1.7","LOADING AND HAULING "]
[]
["C1.7.2.1","Hauling material for use in the Works and "]
[null,"off-loading it on site of the works"]
[]
[null,"(a)","Soil, gravel, crushed stone and pavement"]
[null,null," layer material",null,"m³- km",15000]
[]
[]
["Chapter 1","Total for Chapter 1.2 - Carried to summary"]

{"sheet":"CHAPTER 2","index":1,"n_rows":61,"n_cols":8,"rows_kept":61,"merged":[[60,1,60,3],[66,0,66,7]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 2"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C2.1","GENERAL REQUIREMENTS AND "]
[null,"TRENCHING FOR SERVICES"]
[]
["C2.1.1","Location, Identification and relocation"]
[null," of existing services"]
[]
["C2.1.1.3","Handling costs and profit in respect of item"]
[null," C2.1.1.2 above "]
[]
["C2.1.1.4","Permanent services relocation and or"]
[null,"protection work by the Contrcactor",null,null,"-","Prov","Sum",{"v":30000,"d":"R 30,000.00"}]
[]
["C 2.1.2","Existing services location, detection"]
[null," and verification"]
[]
["C2.1.2.5","Using hand excavation to locate, expose "]
[null,"and verify services",null,null,"m3",50]
[]
["C 2.1.19","Dealing with water during services"]
[]
["C2.1.19.2","Dealing with sub -surface water",null,null,"Lump sum","-"]
[]
["C2.1.27","Demolition of existing manholes,"]
[null," access chambers and other service  "]
[null,"structure consisting of:"]
[]
["C 2.1.27.1","Unreinforced concrete",null,null,"m3",10]
[]
["C2.1.27.2","Reinforced concrete",null,null,"m3",10]
[]
["C2.1.27.3","Masonry",null,null,"m3",10]
{"$rows_empty":22}
["Chapter 2","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"CHAPTER 3","index":2,"n_rows":303,"n_cols":8,"rows_kept":303,"merged":[[31,1,31,3],[187,19,187,20],[187,21,187,22],[248,19,248,20],[248,21,248,22],[302,1,302,3],[308,0,308,7]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 3"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C 3.1","DRAINS"]
[]
["C3.1.1","Excavation for open drains:"]
[]
["C3.1.1.1","Excavating all material situated within the "]
[null,"following depth ranges below the surface "]
[null,"level:"]
[]
[null,"(a)","0 m up to 1,5 m",null,"m3",300]
[]
["C3.1.1.2","Extra over sub-item C3.1.1.1 for excavation in "]
[null,"hard and boulder material, irrespective of depth",null,null,"m3",100]
[]
["C3.1.1.3","Extra over sub-item C3.1.1.1 for excavation in "]
[null,"stabilised existing road layers, irrespective of ",null,null,"m3",50]
[null,"depth"]
[]
["C3.1.2","Clearing shaping and disposal of accumulated"]
[null,"sediment in existing unlined open drains"]
[]
["C3.1.2.2","Using labour henced construction methods",null,null,"m3",40]
[]
["C3.1.3","Eccavation, clearing and desposal of sediment"]
[null,"in existing lined drains and drainage"]
[null,"accumulated system"]
[]
["C3.1.3.1","Using conventional methods"]
[]
[null,"(c) Concrete or other lined side drains",null,null,"m³",150]
[]
["C 3.1.4","Excavation and disposal of material for subsoil "]
[null,"drainage systems"]
[]
["C3.1.4.1","Excavating all material situated within the "]
[null,"following depth ranges below the surface "]
[null,"level:"]
[]
[null,"(a)","0 m up to 1,5 m",null,"m³",10]
[]
[null,"(b)","Exceeding 1,5 m and up to 3,0 m",null,"m³",10]
[]
["C3.1.4.2","Excavating soft material situated within 0 m to 1,5 m ",null,null,"m³",15]
[null,"below the surface using labour enhanced "]
[null,"construction methods"]
[]
["C3.1.4.4","Extra over sub-item C3.1.4.1 for excavation in ",null,null,"m³",10]
[null,"hard and boulder material, irrespective of depth"]
[]
[]
[]
[]
["C 3.3","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 3"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C 3.3","Brought forward"]
[]
[]
["C3.1.7","Natural permeable material in subsoil drainage "]
[null,"systems"]
[]
["C3.1.7.1","Crushed  stone obtained from cormmercial source",null,null,"m³",45]
[null,"(19.0 mm crushed stones)"]
[]
["C3.2.2.2","Using imported selected material"]
[]
[null,"(a)","From commercial sources (crusher)",null,"m³",15]
[]
["C3.1.9","Pipes in subsoil drainage systems:"]
[]
["C3.1.9.1","U-PVC pipes and fittings, normal duty, complete "]
[null,"with couplings, HDPE Flexible slotted 110mm pipe",null,null,"m",150]
[]
["C3.1.9.2","U-PVC pipes and fittings, normal duty, complete "]
[null,"with couplings: HDPE Flexible slotted 75mm pipe",null,null,"m",150]
[]
["C3.1.11","Geotextiles"]
[]
[null,"(F50 SA Polypropylene needled punched geotextile",null,null,"m²",400]
[null," blanket)"]
[]
["C3.1.13","Concrete outlet structure,Manhole boxes, "]
[null,"junction boxes and cleaning eyes for subsoil "]
[null,"drainage system"]
[]
["C3.1.13.1","Outlet structures ",null,null,"No",2]
[null,"(concrete V-drain, ref: 1093-CIV-DRG-400)"]
[]
["C3.1.14","Caps for subsoil drain pipes"]
[]
["C3.1.14.3","HDPE DN 75 mm caps",null,null,"No",5]
[]
["C3.1.14.4","HDPE DN 110 mm caps",null,null,"No",5]
{"$rows_empty":14}
["C 3.3","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 3"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C 3.3","Brought forward"]
[]
[]
["C3.2","CULVERTS"]
[]
["C3.2.1","Excavation for culvert structures:"]
[]
["C3.2.1.1","Excavating in all material situated within the "]
[null,"following depth ranges below the surface level:"]
[]
[null,"(a)","0 m to 1,5 m",null,"m³",550]
[]
[null,"(b)","Exceeding 1,5 m and up to 3,0 m",null,"m³",50]
[]
["C3.2.1.4","Extra over sub-item C3.2.1.1 for excavation in "]
[null,"hard or boulder material, irrespective of depth",null,null,"m³",50]
[]
["C3.2.2","Backfilling:"]
[]
["C3.2.2.1","Using the excavated material",null,null,"m³",980]
[]
["C3.2.2.2","Using imported selected material"]
[]
[null,"(a)","From commercial sources (crusher)",null,"m³",50]
[]
["C3.2.3","Concrete pipe culverts:"]
[]
["C3.2.3.2","On Class B bedding (900mm diameter)",null,null,"m",300]
[]
["C3.2.7","Cast in situ concrete and formwork:"]
[]
["C3.2.7.1","In Class B bedding, screeds, concrete backfill"]
[null,"and the encasing for pipes, including formwork,"]
[null," (25/19 concrete)",null,null,"m³",10]
[]
["C3.2.9","Prefabricated concrete inlets and outlets to "]
[null,"culverts",null,null,"No",4]
[]
["C3.2.10","Reinforcement:"]
[]
["C3.2.10.3","Welded steel fabric (MESH 245)",null,null,"kg",100]
[]
["C3.2.15","Manholes and catchpits with prefabricated "]
[null,"elements"]
[]
["C3.2.15.1","Prefabricated floors"]
[]
[null,"(a)","25 Mpa concrete floor "]
[null,null,"(1230mm x 1230mm x 150mm thick)",null,"No",5]
[]
[]
[]
["C 3.3","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 3"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 3.3","Brought forward"]
[]
[]
["C3.2.15.2","Prefabricated roofs"]
[]
[null,"(a)","Pre cast concrete "]
[null,null,"(512 mm x 990mm x 100mm)",null,"No",5]
[]
["C3.2.15.4","Extra-over item C3.2.15.1 for variation in the "]
[null,"depths of all types of concrete manholes with "]
[null,"prefabricated, or insitu concrete or brickwork "]
[null,"wall combinations deeper than 1.0m "]
[null,"designated for tendering purposes",null,null,"m",50]
[]
["C3.2.16","Brickwork (Culverts outlet)"]
[]
["C3.2.16.2","230 mm thick",null,null,"m²",100]
[]
["C3.2.17","Plaster",null,null,"m²",100]
[]
["C3.2.19","Accessories:"]
[]
["C3.2.19.2","Inlet grids or covers "]
[null,"(ref: 1086-CIV-DRG-405 and 407)",null,null,"No",2]
[]
["C3.2.19.4","Manhole covers or gratings (1200 X 600 X "]
[null,"100mm)",null,null,"No",5]
[]
["C3.2.20","Anchors for pipes",null,null,"No",5]
[]
["C3.2.22","Cutting of concrete pipes (as per drawing)",null,null,"No",10]
[]
["C3.2.24","Compaction of bedding for inlets, outlets, "]
[null,"manholes and catchpits;"]
[]
["C3.2.24.1","Preparation and compaction of in-situ bedding "]
[null,"material to 93 % of MDD (150mm Thick)",null,null,"m³",50]
[]
["C3.2.24.2","Extra-over sub-item C3.2.24.1 for compation to "]
[null,"93% of MDD (150mm thick)",null,null,"m³",50]
{"$rows_empty":12}
["C 3.3","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 3"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 3.3","Brought forward"]
[]
[]
["C3.3","CONCRETE KERBING, CONCRETE"]
[null,"CHANNELLING, CHUTES AND DOWNPIPES,"]
[null,"AND CONCRETE LININGS FOR OPEN DRAINS"]
[]
["C3.3.1","Concrete kerbing:"]
[]
["C3.3.1.1","Prefabricated kerbing"]
[]
[null,"(a)","Prefabricated barrier kerb, SABS 927 ",null,"m",{"v":1100,"d":"1,100"}]
[null,null,"fig 12"]
[]
[null,"(b)"," Transition kerb  class 25/19 ",null,"m",50]
[]
["C3.3.1.2","Cast in situ kerbing"]
[]
[null,"(a)"," Concrete edge beam ",null,"m3",25]
[]
["C3.3.8"," Linings for open drains: "]
[]
["C3.3.8.1","Cast in situ concrete Class 25/19 lining",null,null,"m³",300]
[]
["C3.3.8.2","Class U2 surface finish to cast in situ concrete",null,null,"m²",{"v":2000,"d":"2,000"}]
[]
["C3.3.9","Formwork to cast in situ concrete lining for"]
[null,"open drains (Class F2 surface finish): "]
[]
["C3.3.9.3","To ends of slabs ",null,null,"m²",200]
[]
["C3.3.11","Concrete screed or backfilling below kerbs",null,null,"m3",130]
[]
["C3.3.12","Reinforcement: "]
[]
["C3.3.13","Polymer film sheeting (250 micron) "]
[null,"for concrete-lined open drains",null,null,"m²",{"v":2000,"d":"2,000"}]
[]
["C3.3.12.3","Steel Mesh.ref.no.245",null,null,"kg",{"v":5500,"d":"5,500"}]
[]
["C3.3.16","Demolition and removal of existing kerbs",null,null,"m3",5]
{"$rows_empty":11}
["Chapter 3","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"CHAPTER 4","index":3,"n_rows":61,"n_cols":8,"rows_kept":61,"merged":[[60,1,60,3],[66,0,66,7]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 4"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
["C 4.1","BORROW MATERIALS"]
[]
["C4.1.3","Construction and maintenance of "]
[null,"temporary haul and access roads"]
[]
["C4.1.3.1","temporary unsealed roads",null,null,"km",1.1]
[]
["C4.1.4","Removing of the overburden "]
[]
["C4.1.4.1","In borrow pits",null,null,"m³",100]
[]
["C4.1.5","Excavating of materials in the borrowpit"]
[null," and quarries, material obtained from;"]
[]
["C4.1.5.1","Soft excavation",null,null,"m³",{"v":2100,"d":"2,100"}]
[]
["C4.1.5.2","Boulders excavation class A",null,null,"m³",900]
[]
["C4.1.5.3","Boulders excavation class B",null,null,"m³",100]
[]
["C4.1.5.4","Hard excavation (other than blasting)",null,null,"m³",50]
[]
["C4.1.12","Stockpilling the material"]
[]
["C4.1.12.2","Material directly from the excavation",null,null,"m³",{"v":3000,"d":"3,000"}]
[]
["C4.3","EXISTING ROAD MATERIALS"]
[]
["C 4.3.4","Saw-cutting existing materials within the "]
[null,"following average depth ranges"]
[]
["C 4.3.4.4","Concrete Material:"]
[]
[null,"(a)","Up to 50 mm",null,"m",500]
[]
["C4.3.13","Lifting of existing paving blocks"]
[]
["C4.3.13.2","Using labour enhanced methods of construction",null,null,"m²",800]
[]
["C4.3.14","Removing of existing road edging and services "]
[null,"structures"]
[]
["C4.3.14.2","Removing of existing road edging using labour "]
[null,"enhanced methods of construction"]
[]
[null,"(a)","kerbing and edge beam"]
[]
[null,null,"(i)","In situ concrete kerbing and edge beams","m³",40]
[]
[null,null,"(iii)","Precast concrete kerbing and in-situ concrete ","m",25]
[{"$nulls":3},"channel"]
[]
[]
[]
["Chapter 4","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"CHAPTER 5","index":4,"n_rows":117,"n_cols":8,"rows_kept":117,"merged":[[116,1,116,3],[122,0,122,7]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 5"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
[null,"EARTHWORKS AND PAVEMENT LAYERS "]
[null,"CONSTRUCTION"]
[]
["C5.1","ROADBED"]
[]
["C5.1.1","Roadbed construction and compaction "]
[]
["C5.1.1.2","Compaction of in-situ material to 93 % of MDD "]
[null,"(In situ-G7)",null,null,"m³",1100]
[]
["C5.1.2","Excavate material to spoil sites designated"]
[null,"by the Employer "]
[]
["C5.1.2.1","Excavate material to spoil from roadbed "]
[null,"construction, material obtained from:"]
[]
[null,"(a)","Soft excavation ",null,"m³",2400]
[]
[null,"(b)","Boulder excavation Class A ",null,"m³",550]
[]
[null,"(d)","Hard excavation (other than by blasting) ",null,"m³",190]
[]
["C5.1.4","Removal of unsuitable material to spoil "]
[]
["C5.1.4.1","In layer thicknesses of 200 mm and less "]
[]
[null,"(a)","Stable material",null,"m³",1000]
[]
["C5.1.5"," In-situ treatment of roadbed in hard material "]
[]
["C5.1.5.1","In situ treatment by ripping",null,null,"m³",1500]
[]
["C5.1.6","Roller-pass compaction"]
[]
["C5.1.6.1","Grid rollers",null,null,"m²",7000]
[]
["C5.1.6.2","vibratory roller",null,null,"m²",6600]
[]
["C5.2.2","Fill Construction"]
[]
["C5.2.2.1","Normal fill material in compacted layerthickness of "]
[null,"200mm and less:"]
[]
[null,"(a)","Compacted to 93% of MDD",null,"m³",500]
[]
["C5.2.2.4","Rock fill material all per Clause A.5.2.7.6",null,null,"m³",60]
[]
[]
[]
[]
["C 5.3","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 5"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 5.3","Brought forward"]
[]
[]
["C5.3","ROAD PAVEMENTLAYERS"]
[]
["C5.3.2","Construction of pavement layers"]
[]
["C5.3.2.1","Construction of layers using conventional "]
[null,"construction methods"]
[]
[null,"(c)","Gravel selected layer compacted to:"]
[]
[null,null,"(iii)","93% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150 mm "]
[{"$nulls":3},"(In situ G7)","m³",500]
[]
[null,"(l)","Gravel subbase(unstabilized material)"]
[null,null," compacted to:"]
[]
[null,null,"(i)","95% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150 mm (G6)","m³",{"v":1340,"d":"1,340"}]
[]
[null,"(m)","Gravel base (chemically stabilized material) "]
[null,null,"compacted to:"]
[]
[null,null,"(i)","97% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150 mm "]
[{"$nulls":3},"layer (C4)","m³",{"v":1340,"d":"1,340"}]
[]
["C5.3.2.2","Construction of layers using labour "]
[null,"enhancement:"]
[]
[null,"(m)","Sand layer (20mm thickness)",null,"m³",350]
[]
["C5.4","STABILISATION"]
[]
["C5.4.6","Addition of cementious stabilisation agents"]
[]
["C5.4.6.1","Cement (Ordinary Portland cement)",null,null,"t",30]
[]
["C5.4.10","Provision and application of water for curing",null,null,"kl",200]
{"$rows_empty":9}
["Chapter 5","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"CHAPTER 6","index":5,"n_rows":55,"n_cols":8,"rows_kept":55,"merged":[[54,1,54,3]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 6"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C6.2","SEGMENTAL BLOCK PAVING LAYERS"]
[]
["C6.2.1","Segmental block paving"]
[]
["C6.2.1.1","Concrete block paving"]
[null,"Type S-A interlocking paving blocks,"]
[null,"80mm thick, for the roadway",null,null,"m²",8200]
[]
["C6.2.3","Provision and application of approved herbicide "]
[null,"and ant poison"]
[]
["C6.2.3.1","Provision of material",null,null,"PC sum","-",{"v":20000,"d":"R20,000.00"}]
[]
["C6.2.3.2","Contractor's charges and profit added to the prime "]
[null,"cost sum",null,null,"%",null,{"v":20000,"d":"R20,000.00"}]
{"$rows_empty":32}
["Chapter 6","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"CHAPTER 11","index":6,"n_rows":177,"n_cols":8,"rows_kept":177,"merged":[[176,1,176,3]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 11"]
[]
[]
["ITEM",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C11.1","PITCHING, STONEWORK, CAST IN SITU "]
[null,"CONCRETE FOR PROTECTION AGAINST "]
[null,"EROSION"]
[]
["C11.1.2","Stone pitching",null,null,"m²",100]
[]
["C11.6","ROAD SIGNS"]
[]
["C11.6.1","Road sign boards with painted or coloured "]
[null,"semi-matt background.  Symbols, lettering and"]
[null,"borders in Class I retro-reflective material,"]
[null,"where the sign board is constructed from:"]
[]
["C11.6.1.1","Aluminium sheet (2.0 mm thick)"]
[]
[null,"(a)",null,"Area 0 to 0.5 m²","m²",10]
[]
["C11.6.1.6","Extra over item C11.6.1.1 for attaching "]
[null,"signboards to overhead gantry structures and "]
[null,"overheads to bridges"]
[]
["C11.6.1.7","Regulatory signs, permanent"]
[]
[null,"(a)",null,"600 mm diameter (1,4 mm chromadek "]
[{"$nulls":3},"flatsheeting)","No",10]
[]
[null,"(b)",null,"900 mm diameter (1,4 mm chromadek ",","]
[{"$nulls":3},"flatsheeting)","No",5,null,"Rate Only"]
[]
["C11.6.1.9","Warning signs, permanent"]
[]
[null,"(a)",null,"600 mm diameter (1,4 mm chromadek "]
[{"$nulls":3},"flatsheeting)","No",9]
[]
[null,"(b)",null,"900 mm diameter (1,4 mm chromadek "]
[{"$nulls":3},"flatsheeting)","No",5,null,"Rate Only"]
[]
["C11.6.2","Extra over on item C11.6.1 for usning"]
[]
["C11.6.2.1","Background of retro-reflective material of:"]
[]
[null,"(a)",null,"Class I","m²",10]
[]
["C11.6.2.2","Lettering, symbols and borders of retro-"]
[null,"reflective material of:"]
[]
[null,"(a)",null,"Class III","m²",10]
[]
[]
[]
["C 11.6","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 11"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 11.6","Brought forward"]
[]
[]
[]
["C11.6.3","Road sign supports (overhead road sign "]
[null,"structures excluded):"]
[]
["C11.6.3.1","Steel tubing (50 x 50 x 2mm Square tubing)"]
[null,"(2m long)",null,null,"No",20]
[]
["C11.6.3.2","Timber (100mm diameter)",null,null,"m",50]
[]
["C11.6.5","Excavation and backfilling for road sign "]
[null,"supports (not applicable to kilometre posts)"]
[]
["C11.6.5.1","Excavating soft material and backfilling",null,null,"m³",30]
[]
["C11.6.5.2","Excavating soft or intermediate material and "]
[null,"backfilling using labour enhanced construction "]
[null,"methods",null,null,"m³",5]
[]
["C11.6.5.3","Extra over item C11.6.5.1 and 2 for "]
[null,"cement-treated soil backfill",null,null,"m³",25]
[]
["C11.6.5.4","Extra over item C11.6.5.1 for hard material "]
[null,"excavation",null,null,"m³",1]
[]
["C11.7","ROAD MARKINGS AND ROAD STUDS"]
[]
["C11.7.1","Road markings"]
[]
["C11.7.1.1","White lines broken or unbroken (Arcrylic paint,"]
[null,"100 mm wide)",null,null,"km",1.1]
[]
["C11.7.1.2","Yellow lines broken or unbroken (Arcrylic paint,"]
[null,"100 mm wide)",null,null,"km",1.1]
[]
["C11.7.1.4","White lettering and smbols (Arcrylic paint)",null,null,"m²",80]
[]
["C11.7.1.5","Yellow lettering and smbols (Arcrylic paint)",null,null,"m²",80]
[]
["C11.7.1.8","Labour enhanced hand painted white lines "]
[null,"broken or unbroken  (Arcrylic paint, 100 mm wide)",null,null,"m²",80]
[]
["C11.7.1.9","Labour enhanced hand painted Yellow lines"]
[null,"broken or unbroken  (Arcrylic paint, 100 mm wide)",null,null,"m²",50]
[]
[]
[]
[]
["C 11.6","Carried forward"]
[]
[]
[{"$nulls":7},"CHAPTER 11"]
[]
[]
["ITEM NO",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
[{"$nulls":5},"TITY"]
[]
["C 11.6","Brought forward"]
[]
[]
["C11.7.5","Variations in rate of application:"]
[]
["C11.7.5.1","White paint",null,null,"litre",30]
[]
["C11.7.8","Setting out and premarking the lines "]
[null,"(excluding traffic-island markings, lettering "]
[null,"and symbols)",null,null,"km",1.1]
[]
["C11.8.1","Trimming "]
[]
["C11.8.1.1","Machine trimming",null,null,"m²",1200]
[]
["C11.9","FINISHING THE ROAD AND ROAD RESERVE "]
[null,"AND TREATING OLD ROADS"]
[]
["C11.9.1","Finishing the road and road reserve"]
[]
["C11.9.1.2","Single carriageway road",null,null,"km",2.2]
{"$rows_empty":30}
["Chapter 11","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"CHAPTER 20","index":7,"n_rows":58,"n_cols":8,"rows_kept":58,"merged":[[57,1,57,3]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"CHAPTER 20"]
[]
[]
["ITEM NO",null,"DESCRIPTION",null,"UNIT","QTY","RATE","AMOUNT"]
[]
[]
["C20.1","TESTING MATERIAL AND JUDGEMENT "]
[null,"OF WORKMANSHIP"]
[]
["C20.1.2","Special tests requested by the Engineer"]
[]
["C20.1.2.1","Employers's contribution to other concrete tests"]
[]
[null,"(d)","Test for concrete cover",null,"PC Sum",1,{"v":25000,"d":"R25,000.00"}]
[]
[null,null,"(i)","Handling costs and profit in respect of"]
[{"$nulls":3}," item C20.1.2.1(d)","%",null,{"v":25000,"d":"R25,000.00"}]
[]
["C20.1.2.2","Employers's contribution to other special tests"]
[]
[null,"(a)","Specify test",null,"PC Sum",1,{"v":25000,"d":"R25,000.00"}]
[]
[null,null,"(i)","Handling costs and profit in respect of"]
[{"$nulls":3}," item C20.1.2.2(a)","%",null,{"v":25000,"d":"R25,000.00"}]
{"$rows_empty":32}
["Chapter 20","Total for Schedule - Carried forward","Total for Section - Carried forward","Total for Section - Carried forward"]

{"sheet":"1200DB","index":8,"n_rows":189,"n_cols":9,"rows_kept":189,"hidden":true,"merged":[[0,0,0,5],[2,7,2,8],[64,0,64,8],[126,0,126,8],[190,0,190,8]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":7},"SECTION 1200 DB"]
[]
["PAYMENT"]
["REFERS","ITEM",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
["TO","NO",{"$nulls":4},"TITY"]
[{"$nulls":8},""]
["SABS","DB","EARTHWORKS (PIPE TRENCHES)",{"$nulls":5},""]
["1200 DB",{"$nulls":7},""]
[{"$nulls":8},""]
[null,null,"TRENCHES FOR WATER PIPES",{"$nulls":5},""]
[{"$nulls":8},""]
["PSDB","DB.01","Excavate in all materials for trenches, ",{"$nulls":5},""]
["8.3.2",null,"backfill, compact and dispose of surplus ",{"$nulls":5},""]
[null,null,"material:",{"$nulls":5},""]
[{"$nulls":8},""]
[null,null,".01","Pipes up to 450 mm dia for depths:",{"$nulls":4},""]
[]
[{"$nulls":3},"Hand excavation"]
[{"$nulls":8},""]
[{"$nulls":3},".01","Up to 1,0 m      ","m",50]
[]
[{"$nulls":3},"Mechanical excavation"]
[]
[{"$nulls":3},".01","Up to 1,0 m      ","m",50]
[{"$nulls":3},".02","Up to 1.5 m      ","m",null,null,"Rate Only"]
[]
[]
[]
[]
[null,null,".02","Pipes from 525 mm to 600 mm dia for depths:"]
[]
[{"$nulls":3},"Hand excavation"]
[]
[{"$nulls":3},".01","Up to 1,0 m      ","m",null,null,"Rate Only"]
[]
[{"$nulls":3},"Mechanical excavation"]
[]
[{"$nulls":3},".01","Up to 1,0 m      ","m",null,null,"Rate Only"]
[]
[]
[]
[]
[]
[]
[null,null,".01","Pipes from 750 mm to 900 mm dia for depths:"]
[]
[{"$nulls":3},"Hand excavation"]
[]
[{"$nulls":3},".01","Up to 1,0 m      ","m",null,null,"Rate Only"]
[]
[]
[null,"Total for Schedule- Carried forward"]
{"$rows_empty":8}
["1200 DB","Carried forward"]
[]
[]
[]
[]
[{"$nulls":8},"SECTION 1200 DB"]
[]
["PAYMENT"]
["REFERS","ITEM",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
["TO","NO",{"$nulls":4},"TITY"]
[]
[null,null,"Brought forward"]
[]
[{"$nulls":3},"Mechanical excavation",{"$nulls":4},""]
[{"$nulls":8},""]
[{"$nulls":3},".01","Up to 1,0 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".02","Up to 1.5 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".03","Up to 2,0 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".04","Up to 2.5 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".05","Up to 3.0 m      ","m",null,null,"Rate Only"]
[]
[null,null,".01","Pipes from 1200 mm to 1350 mm dia for depths:"]
[]
[{"$nulls":3},"Hand excavation"]
[]
[{"$nulls":3},".01","Up to 1,0 m      ","m",null,null,"Rate Only"]
[]
[{"$nulls":3},"Mechanical excavation",{"$nulls":4},""]
[]
[{"$nulls":3},".01","Up to 1,0 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".02","Up to 1.5 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".03","Up to 2,0 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".04","Up to 2.5 m      ","m",null,null,"Rate Only"]
[{"$nulls":3},".05","Up to 3.0 m      ","m",null,null,"Rate Only"]
[]
["PSDB","DB.02","Extra over item DB.01 above for:"]
["8.3.2"]
[null,null,".01","Intermediate excavation  ",null,"m3",10]
[]
[null,null,".02","Hard rock excavation     ",null,"m3",10]
[]
[null,null,".03","Hand excavation and backfill where "]
[{"$nulls":3},"ordered by the Engineer "]
[]
[{"$nulls":3},".01","Soft  excavation  ","m3",10]
[]
[{"$nulls":3},".02","Intermediate excavation  ","m3",10]
[]
[{"$nulls":3},".03","Hard excavation     ","m3"]
[]
[null,null,".04","Backfill stabilized with 5% cement "]
[{"$nulls":3},"where directed by the Engineer   ",null,"m3",20]
[]
[null,null,".05                       Soilcrete backfill where directed by ","Soilcrete backfill where directed by the"]
[{"$nulls":3},"Engineer ",null,"m3",20]
{"$rows_empty":7}
["1200 DB","Carried forward"]
[]
[]
[]
[{"$nulls":8},"SECTION 1200 DB"]
[]
["PAYMENT"]
["REFERS","ITEM",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
["TO","NO",{"$nulls":4},"TITY"]
[]
[null,null,"Brought forward"]
[]
[]
["PSDB","DB.03","Excavate and dispose of unsuitable "]
["8.3.2",null,"material from trench bottom ",null,null,"m3",20]
[]
[]
["PSDB","DB.04","Excavation ancillaries:"]
["8.3.3"]
[null,null,".01","Make up deficiency in backfill material:"]
[]
[{"$nulls":3},".01","From other necessary excavations "]
[{"$nulls":4},"on Site","m3",null,null,"Rate Only"]
[]
[{"$nulls":3},"0.3","By importation from commercial or "]
[{"$nulls":4},"off-site sources selected by the "]
[{"$nulls":4},"Contractor","m3",null,null,"Rate Only"]
[]
[null,null,".03","Compaction in road crossings     ",null,"m3",null,null,"Rate Only"]
[]
[null,null,"0.4","Careful excavation to locate and expose ",null,"m3"]
[{"$nulls":3},"existing services",{"$nulls":4},"Rate Only"]
{"$rows_empty":32}
["1200 DB","Total for Schedule - Carried forward"]

{"sheet":"1200LB","index":9,"n_rows":62,"n_cols":9,"rows_kept":62,"hidden":true,"merged":[[0,0,0,5],[2,7,2,8],[63,0,63,8]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":7},"SECTION 1200 LB"]
[]
["PAYMENT"]
["REFERS","ITEM",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
["TO","NO",{"$nulls":4},"TITY"]
[{"$nulls":8},""]
["SABS","LB","BEDDING (PIPES)",{"$nulls":5},""]
["1200 LB",{"$nulls":7},""]
[{"$nulls":8},""]
[null,null,"BEDDING FOR WATER PIPES",{"$nulls":5},""]
[]
["8.2.1","LB.01","Provision of bedding from trench "]
[null,null,"excavations:"]
[]
[null,null,".01","Selected granular material ",null,"m3",10]
[]
[null,null,".02","Selected fill material",null,"m3",10]
[]
["8.2.2","LB.02","Supply only of bedding by importation:"]
[]
[null,null,".01","From other necessary excavations:"]
[]
[{"$nulls":3},".01","Selected granular material","m3",10]
[]
[{"$nulls":3},".02","Selected fill material","m3",10]
[]
[null,null,".03","From commercial sources:"]
[]
[{"$nulls":3},".01","Selected granular material","m3",null,null,"Rate Only"]
[]
[{"$nulls":3},".02","Selected fill material ","m3",null,null,"Rate Only"]
{"$rows_empty":26}
[{"$nulls":8},""]
[]
["1200 LB","Total for Schedule - Carried forward"]

{"sheet":"Summary of Schedule","index":10,"n_rows":80,"n_cols":9,"rows_kept":80,"hidden":true,"merged":[[1,1,3,6],[6,7,6,8],[9,7,9,8],[12,7,12,8],[15,7,15,8],[17,7,17,8],[19,7,19,8],[21,7,21,8],[23,7,23,8],[25,7,25,8],[29,7,29,8],[31,7,31,8],[37,7,37,8],[39,7,39,8],[41,7,41,8],[43,7,43,8],[45,7,45,8],[47,7,47,8],[50,7,50,8],[52,7,52,8],[54,7,54,8],[56,7,56,8],[58,7,58,8],[60,7,60,8],[63,7,63,8],[65,7,65,8],[67,7,67,8],[69,7,69,8],[71,7,71,8],[73,7,73,8],[75,7,75,8],[76,7,76,8],[77,7,77,8],[78,7,78,8],[79,7,79,8]],"flags":["formulas_cached_only"]}
[]
[null,"SCM/TSW/04/2017  : The Construction of 2.0km Paved Road and Stormwater in Tswelopele Local Municipality, Phahameng/Bultfontein\n"]
[]
[]
[{"$nulls":8},"Total brought forward"]
[]
[null,1200,"GENERAL REQUIREMENTS AND",{"$nulls":3},"R"]
[null,null,"PROVISIONS"]
[]
[null,1300,{"$error":"#REF!"},{"$nulls":3},"R"]
[null,null,{"$error":"#REF!"}]
[]
[null,1400,{"$error":"#REF!"},{"$nulls":3},"R"]
[null,null,{"$error":"#REF!"}]
[]
[null,1500,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,1800,"PERSONNEL "]
[]
[null,2100,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,2200,"PREFABRICATED CULVERTS"]
[]
[null,2300,{"$error":"#REF!"},{"$nulls":3},"R"]
[null,null,{"$error":"#REF!"}]
[null,null,{"$error":"#REF!"}]
[]
[null,3100,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,3200,{"$error":"#REF!"},{"$nulls":3},"R"]
[null,null,{"$error":"#REF!"}]
[null,null,{"$error":"#REF!"}]
[null,null,{"$error":"#REF!"}]
[null,null,{"$error":"#REF!"}]
[]
[null,3300,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,3400,"PAVEMENT LAYERS"]
[]
[null,3400,{"$error":"#REF!"},{"$nulls":3},"R",0]
[]
[null,3500,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,3600,"CRUSHED STONE BASE"]
[]
[null,5100,{"$error":"#REF!"},{"$nulls":3},"R"]
[null,null,{"$error":"#REF!"}]
[]
[null,5200,"FOUNDATION,TRENCH EXCAVATION AND BACKFILL"]
[]
[null,5500,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,5700,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,5800,"TRIMMING"]
[]
[null,5900,{"$error":"#REF!"},{"$nulls":3},"R"]
[null,null,{"$error":"#REF!"}]
[]
[null,{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,8100,{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,"1200DB","EARTHWORKS (PIPE TRENCHES)",{"$nulls":3},"R"]
[]
[null,"1200LB","BEDDING (PIPES)",{"$nulls":3},"R"]
[]
[null,"1200LE",{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,"C",{"$error":"#REF!"},{"$nulls":3},"R"]
[]
[null,"Total of Schedules",{"$nulls":4},"R"]
[null,"CONTINGENCIES (5%)"]
[null,"TOTAL (EXCL. VAT)"]
[null,"VAT 14%"]
[null,"GRAND TOTAL (INCL. VAT)"]

{"sheet":"Socio-Economic","index":11,"n_rows":67,"n_cols":9,"rows_kept":67,"merged":[[0,0,0,5],[68,0,68,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":8},"SECTION A"]
[]
["PAYMENT"]
["REFERS","ITEM",null,null,"DESCRIPTION","UNIT","QUAN-","RATE","AMOUNT"]
["TO","NO",{"$nulls":4},"TITY"]
[{"$nulls":8},""]
[null,null,"SOCIO-ECONOMIC REQUIREMENTS"]
[]
["C10.1",null,"Community participation"]
[]
[null,"(a)","Cost of community participation and PLC "]
[null,null,"support ",null,null,"Prov Sum",{"v":1,"d":"1.00"},{"v":50000,"d":"R 50,000.00"}]
[]
[null,"(b)","Handling cost and profit in respect of ",null,null,"%",null,{"v":50000,"d":"R 50,000.00"}]
[null,null,"subitem C10.01(a) "]
{"$rows_empty":50}
["Section A","TOTAL SECTION A CARRIED TO SUMMARY"]

{"sheet":"Summary of_Schedule","index":12,"n_rows":24,"n_cols":3,"rows_kept":24,"merged":[[22,0,22,1],[23,0,24,0],[23,1,24,2]],"flags":["formulas_cached_only"]}
{"$rows_empty":8}
["SECTION","DESCRIPTION","AMOUNT"]
["CHAPTER 1","GENERAL REQUIREMENTS AND PROVISIONS "]
["CHAPTER 2","SERVICES"]
["CHAPTER 3","DRAINAGE"]
["CHAPTER 4","EARTHWORKS AND PAVEMTN LAYERS: MATERIALS"]
["CHAPTER 5","EARTHWORKS AND PAVEMTN LAYERS: CONSTRUCTION"]
["CHAPTER 6","CONCRETE LAYERS"]
["CHAPTER 11","ANCILLARY ROAD WORKS"]
["CHAPTER 20","QUALITY ASSURANCE"]
["SECTION A","SOCIO-ECONOMIC REQUIREMENTS"]
[null,"SUB TOTAL"]
[null,"CONTINGENCIES (10%)"]
[null,"SUB TOTAL (EXCL. VAT)"]
[null,"15% VALUE ADDED TAX (VAT)                                        "]
["TOTAL (INCL VAT) "]
["AMOUNT IN WORDS"]