{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Annexure A"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Annexure A","index":0,"n_rows":53,"n_cols":34,"rows_kept":53,"merged":[[6,2,6,23],[7,2,7,3],[7,4,7,5],[8,2,8,15],[9,2,43,3],[44,18,44,19],[44,22,44,23],[45,2,45,8],[45,10,45,15],[45,18,45,19],[45,22,45,23],[46,2,46,7],[46,10,46,12],[46,14,46,15],[46,18,46,19],[46,22,46,23],[47,2,47,7],[47,10,47,13],[47,14,47,15],[52,2,53,8],[52,10,52,11],[52,16,53,17],[52,18,53,19],[52,20,53,21],[52,22,53,23],[52,24,53,25],[53,10,53,11],[54,14,54,15]],"flags":["formulas_cached_only"]}
[{"$nulls":3},0,"Do Not Meet",{"$nulls":22},"MAX",null,"Not applicable",{"v":0,"d":"0%"},{"v":0.69,"d":"69%"},"NOT MEET","0-69"]
[{"$nulls":3},1,"Partial Meet",{"$nulls":22},{"v":0,"d":"0%"},0,"Do Not Meet",{"v":0.7,"d":"70%"},{"v":0.79,"d":"79%"},"PARTIAL MEET","70-79"]
[{"$nulls":3},2,"Meet",{"$nulls":22},{"v":0.75,"d":"75%"},1,"Partial Meet",{"v":0.8,"d":"80%"},{"v":1,"d":"100%"},"MEET","80 - 100"]
[{"$nulls":3},3,"Exceed",{"$nulls":22},{"v":1,"d":"100%"},2,"Meet",{"v":1.01,"d":"101%"},110,"EXCEED","101-110"]
[{"$nulls":27},{"v":1.1,"d":"110%"},2,"Exceed"]
[{"$nulls":27},{"v":1,"d":"100%"},"X","Not applicable"]
[null,null,"Functional Evaluation Criteria for Plant Enquiry No: WCKBG2588AB - The Supply and Delivery of two (2) Forklifts to Koeberg Nuclear Power Station "]
[{"$nulls":4},"Requirements",null,"Compliant/Non Compliant","Deliverables","Weighting",null," Rating","% Rating","% Score",null,"[ Supplier Name ] Response","Eskom Comments"]
[null,null,"Three (3) Ton Forklift",{"$nulls":13},{"v":0,"d":"0.0%"},{"$nulls":7},{"v":0,"d":"0.0%"}]
[null,null,"Annexure A",null," Engine Capacity","Minimum displacment 3000cc ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Engine Emision Category   (97/68EC stage II)","Tier 3",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," kW output","Minimum  of 40kW ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Nm output","Torque: Minimum 180nm",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Fuel driven","Diesel Powered (Normally aspirated or Turbo)",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Brakes ","Hydraulic foot pedal",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Park brake ","Parking brake lever with interlock",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Transmission "," Automatic Power Shift",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Lifting capacity in     kg","3000kg @500mm load centre",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Mast type ","Wide view mast.",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Mast lift height","4000mm  2 stage mast",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Mast lowered height","Max 2800mm",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Overhead guard height","Max 2800mm",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Fork length","1500mm",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Forks width and thickness","130mm x50mm",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Fork positioner","Hydraulic  side Shift",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Fork leveling ","Automatic control ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Tyre size ","As per manufacturers specifications.",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Tyre type","Solid tyres",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Steering ","Power assisted steering hydrostatic type",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Noise levels","Noise Level: not to exceed 85db",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Seat belts ","Seat Belts: S A B S  approved",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Colour ","Colour : Yellow",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Full Corrosion protection for West Coast conditions","Painted with Jotun mastic  90 paint to a thickness of 300 micron and a top coat of Jotun hard top flex to a thighness of 60 microns",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Reverse Buzzer","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Amber led rotaing lamp ","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Horn","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Non slip floor mat","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"  2 x rear view mirrors","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Headlights & indicators","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Rear working light","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4}," Tail & stop lights","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Rear pillar grab handle ","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Suspension seat with seat belt.","To be fitted as standard ",null,"Proof (brochures) for verification of compliance",{"v":0.0147,"d":"1.47%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"TOTAL WEIGHTING",{"$nulls":3},{"v":0.4997999999999998,"d":"50%"},null,false,{"v":0,"d":"0%"},{"v":0,"d":"0%"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":7},{"$error":"#REF!"}]
[]
[null,null,"Final Analysis"]
[null,null,"Annexure A",{"$nulls":5},{"v":0.5,"d":"50%"},null,{"v":0,"d":"0.0%"}]
[null,null,"TOTAL",{"$nulls":5},{"v":0.5,"d":"50%"},null,{"v":0,"d":"0.0%"}]
[{"$nulls":3},"RECOMMENDED"]
[{"$nulls":3},"NOT RECOMMENDED"]
[{"$nulls":3},"RE-EVALUATE",{"$nulls":6},{"$error":"#REF!"},true,null,null,{"$error":"#REF!"},true]
[]
[null,null,"The scoring of Annexure A is as follows:\n\n0 - 0% -    Non-compliant \n2 -100% - Compliant"]