{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["ANNEXURE A"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"ANNEXURE A","index":0,"n_rows":165,"n_cols":12,"rows_kept":165}
["LINE #","ITEM NUMBER","GROUP SERIES","ITEM DESCRIPTION","MEDICAL DEVICE CLASSIFICATION AS PER SAHPRA REQUIREMENTS","SAMPLE TO BE SUBMITTED/ DEMONSTARTED","NUMBER OF SAMPLES TO BE SUBMITTED","LOCAL CONTENT AND PRODUCATION % OBJECTIVE TARGET","LIST THE MATERIALS SOURCED LOCALLY","LIST THE MATERIALS IMPORTED","SHORT DESCRIPTION OF PRODUCTION PROCESS ","SPECIFY ANY DEVIATION TO SPECIFICATION"]
[1,"RT21-01-001","Not applicable","Radiation Protective aprons of 0.25mmPb equivalent: Double sided: Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. .Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[2,"RT21-01-002","Not applicable","Radiation Protective aprons of 0.25mmPb equivalent: Double sided: Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean. State your covering material. State type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. .Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[3,"RT21-01-003","Not applicable","Radiation Protective aprons of 0.25mmPb equivalent: Double sided: Sizes: Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean.State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. .Bidders to quote separately for different design","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[4,"RT21-01-004","Not applicable","Radiation Protective aprons of 0.25mmPb equivalent: Double sided: Sizes: X- Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean.State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. .Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[5,"RT21-01-005","Not applicable","Radiation Protective aprons of 0.25mmPb equivalent: Double sided: Sizes: XX- Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean.State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. .Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[6,"RT21-01-006","Not applicable","Radiation Protective aprons of 0.25mmPb equivalent: Double sided: Sizes: XXX- Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean.State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. .Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[7,"RT21-01-007","Not applicable","Radiation Protective aprons of 0.35mmPb equivalent: Double sided: Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[8,"RT21-01-008","Not applicable","Radiation Protective aprons of 0.35mmPb equivalent: Double sided: Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[9,"RT21-01-009","Not applicable","Radiation Protective aprons of 0.35mmPb equivalent: Double sided: Sizes: Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean.State your covering material, state type of fasterners used, state if you use shoulders pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. Bidders to quote separately for different design","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[10,"RT21-01-010","Not applicable","Radiation Protective aprons of 0.35mmPb equivalent: Double sided: Sizes: X-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean.State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. Bidders to quote separately for different design","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[11,"RT21-01-011","Not applicable","Radiation Protective aprons of 0.35mmPb equivalent: Double sided: Sizes: XX-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resitant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Pb-equivalent lead shielding on both front and back panels, providing 360° radiation protection. Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[12,"RT21-01-012","Not applicable","Radiation Protective aprons of 0.25mm Pb equivalent: Wrap around jacket with belt, Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[13,"RT21-01-013","Not applicable","Radiation Protective aprons of 0.25mm Pb equivalent: Wrap around jacket with belt, Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[14,"RT21-01-014","Not applicable","Radiation Protective aprons of 0.25mm Pb equivalent: Wrap around jacket with belt, Sizes: Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[15,"RT21-01-015","Not applicable","Radiation Protective aprons of 0.25mm Pb equivalent: Wrap around jacket with belt, Sizes: X-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[16,"RT21-01-016","Not applicable","Radiation Protective aprons of 0.25mm Pb equivalent: Wrap around jacket with belt, Sizes: XX-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[17,"RT21-01-017","Not applicable","Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[18,"RT21-01-018","Not applicable","Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[19,"RT21-01-019","Not applicable","Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[20,"RT21-01-020","Not applicable","Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: X-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[21,"RT21-01-021","Not applicable","Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: XX-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[22,"RT21-01-022","Not applicable","Lead free Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[23,"RT21-01-023","Not applicable","Lead free Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[24,"RT21-01-024","Not applicable","Lead free Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[25,"RT21-01-025","Not applicable","Lead free Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: X-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[26,"RT21-01-026","Not applicable","Lead free Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: XX-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[27,"RT21-01-027","Not applicable","Lead free Radiation Protective aprons of 0.35mm Pb equivalent: Wrap around jacket with belt, Sizes: XXX-Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean, state your covering material, state type of fasteners used, state if you use shoulder pads, per apron.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[28,"RT21-01-028","Not applicable","Lead -freeRadiation Protective  wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[29,"RT21-01-029","Not applicable","Lead -freeRadiation Protective  wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[30,"RT21-01-030","Not applicable","Lead -freeRadiation Protective  wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: Large(metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[31,"RT21-01-031","Not applicable","Lead -freeRadiation Protective  wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: XLarge(metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[32,"RT21-01-032","Not applicable","Lead -freeRadiation Protective  wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: XXLarge(metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[33,"RT21-01-033","Not applicable","Radiation Protective waist apron of 0.35mm Pb equivalent, size: small,  length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material. State type of fasteners used, per set.Must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[34,"RT21-01-034","Not applicable","Radiation Protective waist apron of 0.35mm Pb equivalent,  size:  medium length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material. State type of fasteners used, per set.Must be clearly labelled on the outside of each apron.Bidders to quote separately for diffent design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[35,"RT21-01-035","Not applicable","Radiation Protective waist apron of 0.35mm Pb equivalent, size:   large, length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material. State type of fasteners used, per set.Must be clearly labelled on the outside of each apron.Bidders to quote separately for diffent design.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[36,"RT21-01-036","Not applicable","Radiation Protective waist apron of 0.35mm Pb equivalent,  size:  X-large, length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material. State type of fasteners used, per set.Must be clearly labelled on the outside of each apron.Bidders to quote separately for diffent design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[37,"RT21-01-037","Not applicable","Radiation Protective waist apron of 0.35mm Pb equivalent,  size: XX-large, length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material. State type of fasteners used, per set.Must be clearly labelled on the outside of each apron.Bidders to quote separately for diffent design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[38,"RT21-01-038","Not applicable","Radiation Protective waist apron of 0.35mm Pb equivalent, size:  XXX-large length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material. State type of fasteners used, per set.Must be clearly labelled on the outside of each apron.Bidders to quote separately for diffent design.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[39,"RT21-01-039","Not applicable","Radiation Protective wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: Small (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[40,"RT21-01-040","Not applicable","Radiation Protective wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: Medium (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design. Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[41,"RT21-01-041","Not applicable","Radiation Protective wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: Large (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[42,"RT21-01-042","Not applicable","Radiation Protective wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: XLarge(metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron.Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[43,"RT21-01-043","Not applicable","Radiation Protective wrap around vest and skirt aprons of 0.35mm Pb equivalent:  Sizes: XXLarge (metric measurements to be specified by tenderer), length of the sizes to be specified, different colours to be specified, covering to be waterproof, stain resistant and easy to clean. State your covering material, state type of fasterners used, state if you use shoulders pads, per apron. Lead (Pb) equivalent must be clearly labelled on the outside of each apron. Bidders to quote separately for different design.Skirt and vest can be interchangeable. Sizes to be specified at ordering. ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[44,"RT21-01-044","Not applicable","Gonald Shields ( set of three -S,M,L) with radiation protection effect of 0.5mm Pb equivalent , covering to be waterproof, stain resistant and easy to clean. State your covering material, per set.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[45,"RT21-01-045","Not applicable","Radiation Protective screen, mobile height adjustable stand with lead equivalent shields of 0.5mm. Footrest should be stable as not to tip over, wheels to be in the range of 15-25cm diameter per device.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[46,"RT21-01-046","Not applicable","Radiation Protective Thyroid collar: For reducing radiation to the thyroid during general fluoroscopy and special procedures, lightweight, comfortable, of 0.5mm Pb equivalent, shielded area is semi-circular, 10-15cm wide, tape fasteners or Velcro to permit adjustment for shield to fit all neck sizes, covered with a easily-cleaned soft vinyl, per collar. Size in centimeters will be specified on order.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[47,"RT21-01-047","Not applicable","Radiation Protective glasses: Sturdy frame with minimum 0.5mm Pb equivalent glasses to be supplied with a protective casing. Normal lightweight frame (metal, polycarbonate,nylon), per glasses and casing.","Class A","Yes","2 Samples","N/A"]
[48,"RT21-01-048","Not applicable","Radiation Protective glasses: Sturdy frame with lead glasses with minimum 0.75mm Pb equivalent to be supplied with a protective casing 180° protection lightweight frame (metal, polycarbonate,nylon), per glasses and casing","Class A","N/A","N/A","N/A"]
[49,"RT21-01-049","Not applicable","Radiation Protective gloves: 0.35mm Pb equivalent, Different sizes: 5-6, 7-8, 9-10, different colours to be specified, covering to be waterproof, stain resistant and easy to clean,separate ordering of Right and Left gloves possible. (per glove). ","Class B","Yes","2 Samples","N/A"]
[50,"RT21-01-050","Not applicable","Radiation attenuating gloves –  anatomically correct radiation attenuating latex free surgical gloves with smooth inside and textured outside to be used for radiological and surgical procedures. Sizes 6 .  Used when performing CT guided and Fluoroscopic procedures.","Class B","N/A","N/A","N/A"]
[51,"RT21-01-051","Not applicable","Radiation attenuating gloves –  anatomically correct radiation attenuating latex free surgical gloves with smooth inside and textured outside to be used for radiological and surgical procedures. Sizes 7 .  Used when performing CT guided and Fluoroscopic procedures.","Class B","Yes","2 Samples","N/A"]
[52,"RT21-01-052","Not applicable","Radiation attenuating gloves –  anatomically correct radiation attenuating latex free surgical gloves with smooth inside and textured outside to be used for radiological and surgical procedures. Sizes 8.  Used when performing CT guided and Fluoroscopic procedures.","Class B","N/A","N/A","N/A"]
[53,"RT21-01-053","Not applicable","Radiation attenuating gloves –  anatomically correct radiation attenuating latex free surgical gloves with smooth inside and textured outside to be used for radiological and surgical procedures. Sizes 9.  Used when performing CT guided and Fluoroscopic procedures.","Class B","N/A","N/A","N/A"]
[54,"RT21-01-054","Not applicable","Lead open palm mittens: To cover back of hand and wrist, allow unrestricted use of fingers, thumb to be lead shielded, 0.5mm Pb equivalent, different colours to be specified, covering to be waterproof, stain resistant and easy to clean separate ordering of R and L mitten possible, per mitten.","Class B","Yes","2 Samples",{"v":1,"d":"100%"}]
[55,"RT21-02-001","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium: Size: 354 x 837 mm . Bidders must quote separately for available brands and sizes to fit the CR Cassettes.\n","Class B","N/A","N/A","N/A"]
[56,"RT21-02-002","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium: Size: 252 x 580 mm / 240 x 570mm. Bidders must quote separately for available brands and sizes to fit the CR Cassettes","Class B","N/A","N/A","N/A"]
[57,"RT21-02-003","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium: Size: 354 x 1245 mm . Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","N/A","N/A","N/A"]
[58,"RT21-02-004","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium: Size: 354 x 1017 mm . Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","N/A","N/A","N/A"]
[59,"RT21-02-005","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium: Size: 150 x 300 mm. Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","N/A","N/A","N/A"]
[60,"RT21-02-006","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium:Size: 180 x 240 mm. Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","N/A","N/A","N/A"]
[61,"RT21-02-007","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium: Size: 240 x 300 mm. Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","Yes","2 Samples","N/A"]
[62,"RT21-02-008","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium:Size: 350 x 350 mm. Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","N/A","N/A","N/A"]
[63,"RT21-02-009","Not applicable","Computed Radiography (CR) Imaging Plate, for use in General Radiography. Photostimulable phosphor plate as a recording medium:Size: 350 x 430 mm. Bidders must quote separately for available brands and sizes to fit the CR Cassettes.","Class B","Yes","2 Samples","N/A"]
[64,"RT21-02-010","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 180 x 240 mm/200 X 250 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[65,"RT21-02-011","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 240 x 300 mm/250 X 300mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","Yes","2 Samples","N/A"]
[66,"RT21-02-012","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium size: 350 x 350 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[67,"RT21-02-013","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 350 x 430 mm.Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","Yes","2 Samples","N/A"]
[68,"RT21-02-014","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium:Size: 240 x 570mm / 252 x 580 mm. Bidders must quote separately for  available brands.","Class B","N/A","N/A","N/A"]
[69,"RT21-02-015","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 354 x 837 mm. Bidders must quote separately for available brands.","Class B","N/A","N/A","N/A"]
[70,"RT21-02-016","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 354 x 1245 mm. Bidders to quote separately for available brands.","Class B","N/A","N/A","N/A"]
[71,"RT21-02-017","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 354 x 1017 mm. Bidders must quote separately for available brands.","Class B","N/A","N/A","N/A"]
[72,"RT21-02-018","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in Mammography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 180 x 240 mm/200 x 250mm. Bidders must quote separately for available brand.","Class B","N/A","N/A","N/A"]
[73,"RT21-02-019","Not applicable","Computed Radiography (CR) Cassette with Imaging Plate Set, for use in Mammography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 240 x 300 mm/250 x 300mm. Bidders must quote separately for available brands and sizes compatible to CR Reader.","Class B","Yes","2 Samples","N/A"]
[74,"RT21-02-020","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 180 x 240 mm/200 X 250 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[75,"RT21-02-021","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 240 x 300 mm/250 X 300mm. Bidders must quote separately for available brands and sizes for compatabilityto CR Reader.","Class B","Yes","2 Samples","N/A"]
[76,"RT21-02-022","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium size: 350 x 350 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[77,"RT21-02-023","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 350 x 430 mm.Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","Yes","2 Samples","N/A"]
[78,"RT21-02-024","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium:Size: 240 x 570mm / 252 x 580 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[79,"RT21-02-025","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 354 x 837 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[80,"RT21-02-026","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 354 x 1245 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[81,"RT21-02-027","Not applicable","Computed Radiography (CR) Cassette for use in General Radiography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 354 x 1017 mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[82,"RT21-02-028","Not applicable","Computed Radiography (CR) Cassette  for use in Mammography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 180 x 240 mm/200 x 250mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader.","Class B","N/A","N/A","N/A"]
[83,"RT21-02-029","Not applicable","Computed Radiography (CR) Cassette for use in Mammography. Light weight, heavy duty construction. Photostimulable phosphor plate as a recording medium: Size: 240 x 300 mm/250 x 300mm. Bidders must quote separately for available brands and sizes for compatability to CR Reader..","Class B","Yes","2 Samples","N/A"]
[84,"RT21-02-030","Group Series 1","Cassettes for conventional radiography, with green emitting intensifying screens, lightweight material, heavy duty construction, extended working life due to easily replaceable components, with ID window suitable for daylight markers, speed: 400: 180 x 240mm, per cassette . It must run as a series from item RT21-02-030 to RT21-02-035 will be evaluated as series ","Class B","N/A","N/A","N/A"]
[85,"RT21-02-031","Group Series 1","Cassettes for conventional radiography, with green emitting intensifying screens, lightweight material, heavy duty construction, extended working life due to easily replaceable components, with ID window suitable for daylight markers, speed: 400: 180 x 430mm, per cassette. It must run as a series from item RT21-02-030 to RT21-02-035  will be evaluated as series ","Class B","N/A","N/A","N/A"]
[86,"RT21-02-032","Group Series 1","Cassettes for conventional radiography, with green emitting intensifying screens, lightweight material, heavy duty construction, extended working life due to easily replaceable components, with ID window suitable for daylight markers, speed: 400: 240 x 300mm, per cassette. It must run as a series from item RT21-02-030 to RT21-02-035 will be evaluated as series ","Class B","Yes","2 Samples","N/A"]
[87,"RT21-02-033","Group Series 1","Cassettes for conventional radiography, with green emitting intensifying screens, lightweight material, heavy duty construction, extended working life due to easily replaceable components, with ID window suitable for daylight markers, speed: 400: 300 x 400mm, per cassette. It must run as a series from item RT21-02-030 to RT21-02-035   will be evaluated as series ","Class B","N/A","N/A","N/A"]
[88,"RT21-02-034","Group Series 1","Cassettes for conventional radiography, with green emitting intensifying screens, lightweight material, heavy duty construction, extended working life due to easily replaceable components, with ID window suitable for daylight markers, speed:  400:  350 x 350mm, per cassette.\nIt must run as a series from item RT21-02-030 to RT21-02-035   will be evaluated as series ","Class B","N/A","N/A","N/A"]
[89,"RT21-02-035","Group Series 1","Cassettes for conventional radiography, with green emitting intensifying screens, lightweight material, heavy duty construction, extended working life due to easily replaceable components, with ID window suitable for daylight markers, speed: 400: 350 x 430mm, per cassette. It must run as a series from item RT21-02-030 to RT21-02-035 ` will be evaluated as series ","Class B","Yes","2 Samples","N/A"]
[90,"RT21-02-036","Not applicable","Weight Distribution Cassette Cap should be compatable with all DR brand system · Protects DR Panel during weight-bearing exams. · Fits over the 240x300mm DR Panel· Features slip resistant grips for stability. · For non-gridded weight-bearing studies. · Portable. ","Class A","Yes","2 Samples","N/A"]
[91,"RT21-02-037","Not applicable","Weight Distribution Cassette Cap should be compatable with all DR brand system · Protects DR Panel during weight-bearing exams. · Fits over the 350x430mm DR Panel  · Features slip resistant grips for stability. · For non-gridded weight-bearing studies. · Portable. ","Class A","Yes","2 Samples","N/A"]
[92,"RT21-02-038","Not applicable","Weight Distribution Cassette Cap should be compatable with all DR brand system · Protects DR Panel during weight-bearing exams. · Fits over the 430x430mm DR Panel.  · Features slip resistant grips for stability. · For non-gridded weight-bearing studies. · Portable. ","Class A","Yes","2 Samples","N/A"]
[93,"RT21-02-039","Not applicable","CD for recording archived images with minimum storage capacity of 700MB. CD`s shall have printable face for labelling and marking purposes. CD`s shall be provided in a quantity of 100 per spindle.","N/A","N/A","N/A","N/A"]
[94,"RT21-02-040","Not applicable","DVD-R DVD disk for recording images. Shall have a printable face for labeling and marking purposes. DVD disk shall be provided in individual cases  for easy access when stored. DVD`s shall be upwards of 16 x write speed compatible. Storage capacity minimum of 4,7 GB. DVD`s shall be provided in a quantity of 100 per box.","N/A","N/A","N/A","N/A"]
[95,"RT21-02-041","Not applicable","CD and DVD sleeves - White paper sleeve with window and flap. Dimensions: 124mm x 127mm, w/ a Flap 38mm x 127mm (un-gummed), Packing Type: 100 pcs","N/A","N/A","N/A","N/A"]
[96,"RT21-02-042","Not applicable","CD cases- Single, clear, good quality cd jewel case to store single CD or DVD – Box/Pack of a 100.","N/A","N/A","N/A","N/A"]
[97,"RT21-03-001","Group Series 2","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 180 x 240mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007  will be evaluated as series ","Class A","N/A","N/A","N/A"]
[98,"RT21-03-002","Group Series 2","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 180 x 430mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[99,"RT21-03-003","Group Series 2","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 200 x 400mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[100,"RT21-03-004","Group Series 2","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 240 x 300mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[101,"RT21-03-005","Group Series 2","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 300 x 400mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[102,"RT21-03-006","Group Series 2","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 350 x 350mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[103,"RT21-03-007","Group Series 3","Film radiographic:  orthochromatic (Green Sensitive), medium to high contrast, pre-cut rounded corners and full speed; suitable for rapid processing, for general radiography, for use with green emitting screens; size 350 x 430mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer compatibility.Item numbers RT21-03-001 to RT21-03-007 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[104,"RT21-03-008","Group Series 3","Film radiographic: orthochromatic (Green Sensitive), wide exposure latitude, average contrast pre-cut rounded corners and full speed; suitable for rapid processing, for use with green emitting screens (latitude); size: 180 x 240mm, Box of 100 sheets. Bidders to quote separately for available brands and packaging sizes for printer.Item numbers RT21-03-008 to RT21-03-13 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[105,"RT21-03-009","Group Series 3","Film radiographic: orthochromatic (Green Sensitive), wide exposure latitude, average contrast pre-cut rounded corners and full speed; suitable for rapid processing, for use with green emitting screens (latitude); size: 180 x 430mm, Box of 100 sheets .Bidders to quote separately for available brands and packaging sizes for printer Item numbers  RT21-03-008 to RT21-03-13 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[106,"RT21-03-010","Group Series 3","Film radiographic: orthochromatic (Green Sensitive), wide exposure latitude, average contrast pre-cut rounded corners and full speed; suitable for rapid processing, for use with green emitting screens (latitude); size: 240 x300mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer Item numbers  RT21-03-008 to RT21-03-13 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[107,"RT21-03-011","Group Series 3","Film radiographic: orthochromatic (Green Sensitive), wide exposure latitude, average contrast pre-cut rounded corners and full speed; suitable for rapid processing, for use with green emitting screens (latitude); size: 300 x400mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer tem numbers  RT21-03-008 to RT21-03-13 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[108,"RT21-03-012","Group Series 3","Film radiographic: orthochromatic (Green Sensitive), wide exposure latitude, average contrast pre-cut rounded corners and full speed; suitable for rapid processing, for use with green emitting screens (latitude); size: 350 x 350mm, Box of 100 sheets. Bidders to quote separately for available brands and packaging sizes for printer.Item numbers  RT21-03-008 to RT21-03--13 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[109,"RT21-03-013","Group Series 3","Film radiographic: orthochromatic (green sensitive), wide exposure latitude, average contrast pre-cut rounded corners and full speed; suitable for rapid processing, for use with green emitting screens (latitude); size: 350 x 430mm, Box of 100 sheets.Bidders to quote separately for available brands and packaging sizes for printer. Item numbers  RT21-03-008 to RT21-03--13 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[110,"RT21-03-014","Not applicable","Film, for use with Dry-Printers (Dry Imager), high contrast, high definition for mammography use, black and white images, size: 180 x 240mm /200 x 250mm, per box. Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[111,"RT21-03-015","Not applicable","Film, for use with Dry-Printers (Dry Imager), high contrast, high definition for mammography use, black and white images, size: 240 x 300mm/250 x 300mm, per box.Bidders to quote separately for available brands and packaging sizes for printer compatibility. ","N/A","N/A","N/A","N/A"]
[112,"RT21-03-016","Not applicable","Film, for use with Dry-Printers (Dry Imager), high contrast, high definition for mammography use, black and white images, size: 250 x 360mm/257 x 364mm, per box.Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[113,"RT21-03-017","Not applicable","Film, for use with Dry-Printers (Dry Imager), black & white images, size: 180 x 240mm/200 x 250mm/203 x 254mm, per box.Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[114,"RT21-03-018","Not applicable","Film, for use with Dry-Printers (Dry Imager), black and white images, size: 240 x 300mm/ 250 x300mm, per box.Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[115,"RT21-03-019","Not applicable","Film, for use with Dry-Printers (Dry-Imager), black and white images, size: 350 x 430mm, per box.Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[116,"RT21-04-001","Group Series 4","Radioluscent Positioning Sponges for patient support/immobilization/positioning. Sponges to be covered with non-absorbable rubberised radioluscent high quality material. Shape: Cylindrical Size: Height: 31 cm Width: 20 cm Circumference: 64 cm Item numbers RT21-04-001 to RT21-04-006 will be evaluated as series ","Class A","Yes","2 Samples","N/A"]
[117,"RT21-04-002","Group Series 4","Radioluscent Positioning Sponges for patient support/immobilization/positioning. Sponges to be covered with non-absorbable rubberised radioluscent high quality material. Shape: Round Size: Height: 7 cm Width: 20 cm Circumference: 64 cm Item numbers RT21-04-001 to RT21-04-006 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[118,"RT21-04-003","Group Series 4","Radioluscent Positioning Sponges for patient support/immobilization/positioning. Sponges to be covered with non-absorbable rubberised radioluscent high quality material. Shape: 45 degrees Wedge Size: Height: 19 cm Width: 35 cm Length: 24 cm Item numbers RT21-04-001 to RT21-04-006 will be evaluated as series ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[119,"RT21-04-004","Group Series 4","Radioluscent Positioning Sponges for patient support/immobilization/positioning. Sponges to be covered with non-absorbable rubberised radioluscent high quality material. Shape: Square Size: Height: 20 cm Width: 7 cm Length: 24 cm Item numbers RT21-04-001 to RT21-04-006 will be evaluated as series ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[120,"RT21-04-005","Group Series 4","Radioluscent Positioning Sponges for patient support/immobilization/positioning. Sponges to be covered with non-absorbable rubberised radioluscent high quality material. Shape: 30 degrees Wedge Size: Height: 7 cm Width: 35 cm Length: 27 cm Item numbers RT21-04-001 to RT21-04-006 will be evaluated as series ","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[121,"RT21-04-006","Group Series 4","Radioluscent Positioning Sponges for patient support/immobilization/positioning. Sponges to be covered with non-absorbable rubberised radioluscent high quality material. Shape: 45 degrees Wedge Size: Height: 5 cm Width: 10 cm Length: 21 cm Item numbers RT21-04-001 to RT21-04-006 will be evaluated as series ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[122,"RT21-04-007","Not applicable","Mattress : X-ray table matress:  thin radiolucent mattress, maximum lenghth±200cm x maximum width 80cm, ±5cm thick, covered with rubberised radiolucent fabric cover:  easy to clean and waterproof, per matress.  ","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[123,"RT21-04-008","Not applicable","Infant Paediatric Immobilization for X-Ray\nA specialized device designed to safely and securely position infants and small children during radiographic examinations. It minimizes movement to ensure high-quality diagnostic images while reducing the need for repeat exposures, thus lowering radiation dose.\nSpecifications:\n•\tAdjustable height: 40 cm – 75 cm\n•\tBase dimensions: approx. 60 cm (W) × 60 cm (L)\n•\tSupport cradle length: 40 cm – 55 cm, adjustable for infant size\n•\tStrap width: 5 cm padded, soft-touch restraints for comfort\n•\tWeight capacity: up to 20 kg\n•\tMaterials: Radiolucent frame with non-absorbent, wipe-clean padding\n•\tSafety features: Lockable adjustments, secure fastenings, non-slip base\n•\tCompliance: Meets paediatric imaging safety and SAHPRA standards","Class C + Hazardous Act compliance ","Yes","2 Samples","N/A"]
[124,"RT21-04-009","Not applicable","Patient slide for patient transfer to and from X-ray table: material: washable thermoplastic, non static lightweight product <=7kg and X-ray translucent, size: length: 2m x width: 60 - 80cm x thickness: 4 - 6mm, shape: rectangular with rounded corners and openings to fit man`s hand, rubber strips underneath to prevent sliding, contact area to be smooth for ease of sliding, per device to support a weight of at least 200kg","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[125,"RT21-05-001","Not applicable","Thermal paper; high quality paper for use in video graphic printers, high definition, size: 100 mm x 18m/20m/21m, per roll.Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[126,"RT21-05-002","Not applicable","Thermal paper; high quality paper for use in video graphic printers, high definition, size: 110mm x 18m/110mm x 20m/110mm x21m, per roll.Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[127,"RT21-05-003","Not applicable","Thermal paper; high quality paper for use in video graphic printers, high definition, size: 210mm x 25m, per roll,Bidders to quote separately for available brands and packaging sizes for printer compatibility.","N/A","N/A","N/A","N/A"]
[128,"RT21-05-004","Not applicable","High quality durable pocket shaped envelopes for radiographic film, in accordance with the latest issue of specifications of CKS 225 (SABS): Size 370 x 450mm (220g) with no flap opening on the long side. The paper shall consist of chemically processed wood fibre material only. CKS Colour: Khaki. Detailed printing will be specified on order and must be included in bid price, per 100 envelopes.","Class A","N/A","N/A","N/A"]
[129,"RT21-05-005","Not applicable","Self adhesive labels for X-ray film identification; Descriptions: AP, PA, Inspiration, Expiration, Sitting, Erect, Prone, Supine, Mobile Unit, Decubitus, Flexion, Extension, Tomogram, Control, Compression, Release, Post Mic, Post Evac, Follow through, Review, Min, Hours, Shoot through, Weight Bearing, Oblique, Lateral, Axial, Semi erect. Detailed printing will be specified on order according to end user requirements (Quantities and label wording) and must be included in the bid price. Size: 13 x 45 mm, per 100 stickers.","Class A","N/A","N/A","N/A"]
[130,"RT21-06-001","Not applicable","Left & Right Anatomical Markers: Round or Square. L & R must be cut out. Radio opaque. Durable material. 6mm Radius (Round) or 12 x 12 mm (Square,with rounded corners) and 2 mm thickness, per set. Provision for a ribbon to be made on each disc. Round or square with or without initials will be specified on order.","Class A","Yes","2 Samples",{"v":1,"d":"100%"}]
[131,"RT21-06-002","Not applicable","Digital thermometer for measuring processing chemicals temperature: Hand-held thermometer that is a standard battery-powered unit with a coiled cable and ±15cm probe, storage case to be included. Temperature readings to be in Centigrade from -20° to 120°, with ±0.5% accuracy and a four-digit LED display plus decimal point. Shock resistant.","Class B","N/A","N/A","N/A"]
[132,"RT21-06-003","Not applicable","Densitometer: rechargeble battery powered with AC-powered,backup lightweight, protective housing to be supplied for storage, range: 0.0 to 4.0 OD, accuracy: ±0.02 D, aperture: +-1mm, digital display: 3 digits, light source can be turned on during measurement.","Class B","N/A","N/A","N/A"]
[133,"RT21-06-004","Not applicable","Sensitometer: battery-powered or AC-powered backup, protective housing to be supplied for storage, dual colour electro-luminescent: blue/green (455nm/520nm), 21 step exposure area densities: 0.05 to 3.05 D, Buzzer and delay to prevent double exposure.","Class B","N/A","N/A","N/A"]
[134,"RT21-06-005","Not applicable","Personal Electronic Dosimeter 1. Radiation Detected - X-rays and Gamma rays in range 33KeV to 1.25MeV. 2. Units - Sieverts or Rem. 3. Dose Measurement Range - 1 mrem to 1000rem. 4. Radiation Dose rate - Digital numerical 0 Sievert to 1O Sievert. 5. Overload response - to give clear indication when above 100mSv/h. 6. Variation with temperature - 20 degree Centigrade to +50 degrees Centigrade. 7. Alarms - two alarm levels for both dose and dose rate with dedicated LEDs for either loud beep and vibrate alerts. 8. Battery - Rechargeable Lithium ion with greater than 300 hours typical battery charge. 9. Electromagnetic Compliance (EMS) - Compulsory. 10. A case material - shock, vibration and drop resistant polymers. 11. The casing of dosimeter must contain a clip. \nLoan unit must be supplied within 24 hours of a reported non functioning of the unit until a funtional unit is returned.  The unit must have a minimum of 24 months warranty period.","Class B","Yes","2 Samples","N/A"]
[135,"RT21-07-001","Not applicable","Heavy Duty Metal Hangers for Radiation Protective Apron. Per set of 3.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[136,"RT21-07-002","Not applicable","Heavy Duty Wall Mounted Metal Rack with 5 metal hangers to accomodate 5 Radiation Protective Aprons.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[137,"RT21-07-003","Not applicable","Heavy Duty Wood Hangers for Radiation Protective Apron. Per set of 3.","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[138,"RT21-07-004","Not applicable","Movable heavy duty metal rack to accommodate at least 10 aprons with a four cast iron lockable wheels, must have 2 bars to allow storage of full aprons (bottom bar) and thyroid shield (top bar), storage tray to store the lead glasses and gloves. The trolley must come with non removable apron hangers.  Size 650mmx600mmx1200mm (Width, height breadth)","Class A","N/A","N/A",{"v":1,"d":"100%"}]
[139,"RT21-08-001","Group Series 5","Grid channel with a suitable radioluscent material to protect the grid. Grid to be a 8:1 parallel choice of opening along short side to house CR and conventional cassettes, size: 240 x 300mm. Items numbers RT21-08-001 to RT21-08-002 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[140,"RT21-08-002","Group Series 5","Grid channel with a suitable radioluscent material to protect the grid. Grid to be a 8:1 parallel choice of opening along long side to house CR and conventional cassettes, size: 240 x 300mm. Items numbers RT21-08-001 to RT21-08-002 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[141,"RT21-08-003","Group Series 6","Grid channel with a suitable radioluscent material to protect the grid. Grid to be a 8:1 parallel. Choice of opening: along short side to house CR and conventional cassettes, size: 350 x 430mm. Items numbers RT21-08-003 to RT21-08-004 will be evaluated as series ","Class A","Yes","2 Samples","N/A"]
[142,"RT21-08-004","Group Series 6","Grid channel with a suitable radioluscent material to protect the grid. Grid to be a 8:1 parallel. Choice of opening along long side to house CR and conventional cassetess, size: 350 x 430mm. Items numbers RT21-08-003 to RT21-08-004 will be evaluated as series ","Class A","Yes","2 Samples","N/A"]
[143,"RT21-08-005","Not applicable","MOBILE DR PANEL HOLDER - Mobile Digtal Radiography (DR) light weight detector Holder should be compatable with all DR brand system. Encases grid to protect against damage. Holds DR Panel during exams. Provides additional protection for DR detector. ","Class A","Yes","2 Samples","N/A"]
[144,"RT21-08-006","Not applicable","GRID FOR DR DETECTOR Grid channel with a suitable radioluscent material to protect the grid. Grid to have an opening along long side. To fit DR detector size 240x300mm. To be compatable with different detector brands.   ","Class A","N/A","N/A","N/A"]
[145,"RT21-08-007","Not applicable","GRID FOR DR DETECTOR Grid channel with a suitable radioluscent material to protect the grid. Grid to have an opening along long side. To fit DR detector size 350x430mm. To be compatable with different detector brands.   ","Class A","N/A","N/A","N/A"]
[146,"RT21-08-008","Not applicable","GRID FOR DR DETECTOR Grid channel with a suitable radioluscent material to protect the grid. To fit DR detector size 430x430mm. To be compatable with different detector brands.   ","Class A","N/A","N/A","N/A"]
[147,"RT21-08-009","Not applicable","GRID FOR DR DETECTOR Grid channel with a suitable radioluscent material to protect the grid. Grid to have an opening along short side. To fit DR detector size 240x300mm. To be compatable with different detector brands.   ","Class A","N/A","N/A","N/A"]
[148,"RT21-08-010","Not applicable","GRID FOR DR DETECTOR Grid channel with a suitable radioluscent material to protect the grid. Grid to have an opening along short side. To fit DR detector size 350x430mm. To be compatable with different detector brands.   ","Class A","N/A","N/A","N/A"]
[149,"RT21-08-011","Not applicable","DETECTOR PROTECTION RESEALABLE BAG bags to cover detectors or CR cassettes  – Sealable radio translucent plastic bag with a two-part strip along the opening that can be pressed together and readily reopened. Plastic resealable bags to cover detectors or CR cassettes act as a barrier between fluids and detectors or CR cassette. Should be compatable with all DR brands.","Class A","Yes","2 Samples","N/A"]
[150,"RT21-08-012","Not applicable","Plastic protective caps for C-arm - Disposable transparent polyethylene protective covers, size 350mmx460mm, suitable for covering and protecting C-arm components during procedures. Must be completely see-through to allow unobstructed imaging and must not produce artefacts on images. Latex-free, non sterile or sterile as specified and compatible with infection prevention protocols. Supplied in sealed packaging, minimum 100 units per pack. ","N/A","Yes","2 Samples","N/A"]
[151,"RT21-09-001","Group Series 7","Chemical for automatic processing. Fixer, ready mixed, contained in a 10 litre rigid plastic leak free container. To be clearly marked with Proprietary name, size of the product, date of manufacture, expiry date and batch number.  Item numbers RT21-09-001 to RT21-09-002 will be evaluated as series. ","Class A","N/A","N/A","N/A"]
[152,"RT21-09-002","Group Series 7","Chemical for automatic processing. Developer, ready mixed, contained in a 10 Litre rigid plastic leak free container. To be clearly marked with Proprietary name, size of the product, date of manufacture, expiry date and batch number. Item numbers RT21-09-001 to RT21-09-002 will be evaluated as series ","Class A","N/A","N/A","N/A"]
[153,"RT21-10-001","Not applicable","Screen cleaner, anti-static, compatible with intensifying screens, per supplying unit of 500ml","N/A","Yes","2 Samples","N/A"]
[154,"RT21-10-002","Not applicable","Cleaning solution compatible with CR imaging plates. Size- 250ml. Bidders to quote separately for available brands","Class A","Yes","2 Samples","N/A"]
[155,"RT21-10-003","Not applicable","Cleaning solution compatible with DR detectors. Size- 250ml. Must be medical grade surface disinfectant , alcohol phenol and aldehyde free. Bidders to quote separately for available brands","Class A","Yes","2 Samples","N/A"]
[156,"RT21-10-004","Not applicable","Lint free cloths compatible with CR imaging plates. Size - 230x230mm. Bidders to quote separately for available brands. Box of 50.","Class A","Yes","2 Samples","N/A"]
[157,"RT21-10-005","Not applicable","Disinfectant Cleaning solution compatible with ultrasound probes. Must be medical grade surface disinfectant , alcohol phenol and aldehyde free. Size - 250ml. Bidders to quote separately for available brands ","Class A","Yes","2 Samples","N/A"]
[158,"RT21-10-006","Not applicable","Disinfectant lint free wipes compatible with ultrasound probes. Must be medical grade surface disinfectant , alcohol phenol and aldehyde free. Size - 230x230mm. Bidders to quote separately for available brands.","Class A","Yes","2 Samples","N/A"]
[159,"RT21-11-001","Not applicable","QC Tool for assessment of beam alignment / collimation congruency and centering point for general x ray machines\nUsed to:\n•\tTo verify the correct alignment of the collimator light field with the X-Ray field\n•\tTo verify central beam alignment to the image receptors\nPerspex Cylindrical with 6-7 cm diameter and height of 15-18cm\n\n","N/A","Yes","2 Samples","N/A"]
[160,"RT21-11-002","Not applicable","Collimator Test Plate\nUsed for : (1) To test parameters for Collimator Congruency Plate  (2) To check the alignment of light and X-Ray field, Stainless steel, 18 X 14 cm, 5-10 mm graduations,\nTotal size to be approximately: 25x20 cm’s.","Class A","Yes","2 Samples","N/A"]
[161,"RT21-11-003","Not applicable","QC Cu Filter\nTest for AEC tests and Dose Consistency \nCu Plate\n1mm Thick\n17-18 cm in size","N/A","Yes","2 Samples","N/A"]
[162,"RT21-11-004","Not applicable","QC Cu Filter\nTest for AEC tests and Dose Consistency \nCu Plate\n1,5mm Thick\n17-18 cm in size","N/A","Yes","2 Samples","N/A"]
[163,"RT21-11-005","Not applicable","QC Cu Filter\nTest for AEC tests and Dose Consistency \nCu Plate\n2mm Thick\nsize 10cmx10cm","N/A","Yes","2 Samples","N/A"]
[164,"RT21-12-001","Not applicable","Ultrasound Transmission Gel - Acoustically Perfect, Non-Corrosive, High viscosity Highly Conductive, Water Soluble, Non-Flaky, Non-Greasy, Hypo Allergenic, Non-Toxic, Bacteriostatic and provided in 250 ml bottles.","Class B","Yes","2 Samples","N/A"]