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PART C1:
AGREEMENTS & CONTRACT DATA

	Contents:


	
	No of pages

	C1.1
	Form of Offer and Acceptance 

[to be inserted from Returnable Documents at award stage]
	5

	C1.2a
	Contract Data provided by the Employer
	11

	C1.2b
	Contract Data provided by the 

[to be inserted from Returnable Documents at award stage]
	2

	C1.3
	Pro forma Guarantees
	N/A


C1.1 Form of Offer & Acceptance

Section 1.1 Offer

The Employer, identified in the Acceptance signature block, has solicited offers to enter into a contract for the procurement of:

Article II. Supply of Fire and Rescue Services for Kriel Power Station 
The tenderer, identified in the Offer signature block, has examined the documents listed in the Tender Data and addenda thereto and by submitting this Offer has accepted the Conditions of Tender.

By the representative of the tenderer, deemed to be duly authorised, signing this part of this Form of Offer and Acceptance the tenderer offers to perform all of the obligations and liabilities of the Contractor under the contract including compliance with all its terms and conditions according to their true intent and meaning for an amount to be determined in accordance with the conditions of contract identified in the Contract Data. 

	Options A or C
	The offered total of the Prices exclusive of VAT is 
	R 

	
	Sub total
	R 

	
	Value Added Tax @ 14% is
	R 

	
	The offered total of the amount due inclusive of VAT is

	R 

	
	(in words) 



This Offer may be accepted by the Employer by signing the Acceptance part of this Form of Offer and Acceptance and returning one copy of this document including the Schedule of Deviations (if any) to the tenderer before the end of the period of validity stated in the Tender Data, or other period as agreed, whereupon the tenderer becomes the party named as the Contractor in the conditions of contract identified in the Contract Data.

	Signature(s)


	
	
	

	Name(s)


	
	
	

	Capacity


	
	
	

	For the tenderer:


	

	Name & signature of witness
	(Insert name and address of organisation)
	
	Date
	

	Tenderer’s CIDB registration number: 
	N/A


Section 2.1 Acceptance

By signing this part of this Form of Offer and Acceptance, the Employer identified below accepts the tenderer’s Offer.  In consideration thereof, the Employer shall pay the Contractor the amount due in accordance with the conditions of contract identified in the Contract Data.  Acceptance of the tenderer’s Offer shall form an agreement between the Employer and the tenderer upon the terms and conditions contained in this agreement and in the contract that is the subject of this agreement.

The terms of the contract, are contained in: 

Part C1

Agreements and Contract Data, (which includes this Form of Offer and Acceptance)

Part C2

Pricing Data

Part C3

Scope of Work: Service Information

and drawings and documents (or parts thereof), which may be incorporated by reference into the above listed Parts.

Deviations from and amendments to the documents listed in the Tender Data and any addenda thereto listed in the Returnable Schedules as well as any changes to the terms of the Offer agreed by the tenderer and the Employer during this process of offer and acceptance, are contained in the Schedule of Deviations attached to and forming part of this Form of Offer and Acceptance.  No amendments to or deviations from said documents are valid unless contained in this Schedule.

The tenderer shall within two weeks of receiving a completed copy of this agreement, including the Schedule of Deviations (if any), contact the Employer’s agent (whose details are given in the Contract Data) to arrange the delivery of any securities, bonds, guarantees, proof of insurance and any other documentation to be provided in terms of the conditions of contract identified in the Contract Data at, or just after, the date this agreement comes into effect.  Failure to fulfil any of these obligations in accordance with those terms shall constitute a repudiation of this agreement.

Notwithstanding anything contained herein, this agreement comes into effect on the date when the tenderer receives one fully completed original copy of this document, including the Schedule of Deviations (if any).  

	Signature(s)


	
	
	

	Name(s)
	Morongwe Raphasha
	
	

	Capacity


	General Manager Kriel Power Station
	
	

	for the Employer

	Eskom Holdings SOC Ltd (Reg No. 2002/015527/30), KRIEL POWER STATION, Bethal-Ogies Road, Kriel, 2271, Mpumalanga

	Name & signature of witness
	
	
	Date
	


Note: If a tenderer wishes to submit alternative tenders, use another copy of this Form of Offer and Acceptance.
Section 2.2 Schedule of Deviations to be completed by the Employer prior to contract award

Note:

1. This part of the Offer & Acceptance would not be required if the contract has been developed by negotiation between the Parties and is not the result of a process of competitive tendering.

2. The extent of deviations from the tender documents issued by the Employer prior to the tender closing date is limited to those permitted in terms of the Conditions of Tender.

3. A tenderer’s covering letter must not be included in the final contract document.  Should any matter in such letter, which constitutes a deviation as aforesaid be the subject of agreement reached during the process of Offer and Acceptance, the outcome of such agreement shall be recorded here and the final draft of the contract documents shall be revised to incorporate the effect of it.

	No.
	Subject
	Details

	1
	[●]
	[●]

	2
	[●]
	[●]

	3
	[●]
	[●]

	4
	[●]
	[●]

	5
	[●]
	[●]

	6
	[●]
	[●]

	7
	[●]
	[●]

	
	
	


By the duly authorised representatives signing this Schedule of Deviations below, the Employer and the tenderer agree to and accept this Schedule of Deviations as the only deviations from and amendments to the documents listed in the Tender Data and any addenda thereto listed in the Tender Schedules, as well as any confirmation, clarification or changes to the terms of the Offer agreed by the tenderer and the Employer during this process of Offer and Acceptance.  

It is expressly agreed that no other matter whether in writing, oral communication or implied during the period between the issue of the tender documents and the receipt by the tenderer of a completed signed copy of this Form shall have any meaning or effect in the contract between the parties arising from this Agreement. 

	
	(i) For the tenderer:


	
	(ii) For the Employer


	Signature


	
	
	Morongwe Raphasha

	Name
	
	
	General Manager Kriel Power Station

	Capacity


	
	
	Eskom Holdings SOC Ltd (Reg No. 2002/015527/30), KRIEL POWER STATION, Bethal-Ogies Road, Kriel, 2271, Mpumalanga

	On behalf of
	(Insert name and address of organisation)


	
	Morongwe Raphasha

	Name & signature of witness
	
	
	

	Date
	
	
	


C1.2 TSC3 Contract Data

Article III. Part one - Data provided by the Employer
	Clause
	Section 3.1 Statement
	Section 3.2 Data

	1
	Section 3.3 General
	Section 3.4 

	
	The conditions of contract are the core clauses and the clauses for main Option: 
	

	
	
	A:

Priced contract with price list

	
	dispute resolution Option
	W1:
Dispute resolution procedure

	
	and secondary Options
	

	
	
	X1:

Price adjustment for inflation

	
	
	X2

Changes in the law

	
	
	X4:

Parent company guarantee

	
	
	X18:
Limitation of liability

	
	
	X19:
Task Order

	
	
	Z:

Additional conditions of contract

	
	of the NEC3 Term Service Contract (June 2005)


	

	10.1
	The Employer is (name):
	Eskom Holdings SOC Ltd (reg no: 2002/015527/30), a state owned company incorporated in terms of the company laws of the Republic of South Africa

Morongwe Raphasha

	
	Address
	Registered office at Megawatt Park, Maxwell Drive, Sandton, Johannesburg normanmathibela@mpumacare.co.za

	10.1
	The Service Manager is (name): 
	

	
	Address

The authority of the Services Manager is
	Kriel Power Station, Private Bag X5009, Kriel 2271

	11.2(2)
	The Affected Property is
	Fire and Rescue Services

	11.2(13)
	The service is 
	Supply of Fire and Rescue Services for Kriel Power Station


	11.2(14)
	The following matters will be included in the Risk Register
	As per contract Risk register

	11.2(15)
	The Service Information is in 
	Part 3: Scope of Work and all documents and drawings to which it makes reference.

	12.2
	The law of the contract is the law of 
	the Republic of South Africa

	13.1
	The language of this contract is 
	English

	13.3
	The period for reply is
	24 Hours

	Section 3.5 2
	Section 3.6 The Contractor’s main responsibilities
	

	21.1
	The Contractor submits a first plan for acceptance within
	Two weeks of the Contract Date

	Section 3.7 3
	Section 3.8 Time
	Section 3.9 

	30.1
	The starting date is.
	TBA

	30.1
	The service period is
	60 Months

	Section 3.10 4
	Section 3.11 Testing and defects
	Section 3.12 [image: image1.emf]

	Section 3.13 5
	Section 3.14 Payment
	Section 3.15 

	50.1
	The assessment interval is 
	The 25th day of each successive month.

	51.1
	The currency of this contract is the 
	South African Rand

	51.2
	The period within which payments are made is
	30 days from date of invoice

	51.4
	The interest rate is 


	CPA



	Section 3.16 6
	Section 3.17 Compensation events
	[image: image2.emf] 

	Section 3.18 7
	Section 3.19 Use of Equipment Plant and Materials
	Section 3.20 No data is required for this section of the conditions of contract.

	Section 3.21 8
	Section 3.22 Risks and insurance
	Section 3.23 

	83.1


	The Employer provides these insurances from the Insurance Table
	as stated for “Format TSC3” available on http://www.eskom.co.za/Tenders/InsurancePoliciesProcedures/Pages/EIMS_Policies_

From_1_April_2014_To_31_March_2015.aspx 
(See Annexure A for basic guidance).

	83.1  


	The Employer provides these additional insurances
	as stated for “Format TSC3” available on http://www.eskom.co.za/Tenders/InsurancePoliciesProcedures/Pages/EIMS_Policies_

From_1_April_2014_To_31_March_2015.aspx 
(See Annexure A for basic guidance).

	83.1
	The minimum amount of cover for insurance against loss and damage caused by the Contractor to the Employer’s property is
	R1 million (one million Rand) for any one occurrence or series of occurrences arising out of one event but unlimited during the service period 



	83.1
	The minimum amount of cover for loss of or damage to Plant and Materials provided by the Employer is:
	· For Plant and Materials in transit (South Africa only), temporary off-site storage, on-site storage and during on site construction, installation, testing and commissioning:

the amount of the deductible (first amount payable) relevant to the event described in the “Format B” insurance policy available on

· For Plant and Materials in trust, under assembly or manufacture or storage at the Contractor’s or the Contractor’s agent’s premises:

For a sum sufficient to provide for their replacement at such premises

	83.1
	The minimum amount of cover for insurance in respect of loss of or damage to property (except the Employer’s property, Plant and Materials and Equipment) and liability for bodily injury to or death of a person (not an employee of the Contractor) arising from or in connection with the Contractor’s Providing the Service for any one event is:
	whatever the Contractor deems necessary for any one occurrence or series of occurrences arising out of one event but unlimited during the period of insurance with “cross liability” so that the insurance applies to the Parties involved in the contract separately.



	83.1


	The minimum limit of indemnity for insurance in respect of death of or bodily injury to employees of the Contractor arising out of and in the course of their employment in connection with this contract for any one event is: 
	As prescribed by the Compensation for Occupational Injuries and Diseases Act No. 130 of 1993 and the Contractor’s common law liability for people falling outside the scope of the Act with a limit of Indemnity of not less than R500 000 (Five hundred thousand Rands) and/or

As provided by the laws of the Country in which the Contractor’s employees are domiciled

	83.1  


	The Contractor provides these additional insurances
	Section 3.24 Against failure of the Contractor to use the skill and care normally used by professionals proving services similar to the Service for amounts at the discretion of the Contractor


	Section 3.25 9
	Section 3.26 Termination
	[image: image3.emf]

	Section 3.27 10
	Section 3.28 Data for main Option clause
	Section 3.29 

	A
	Priced contract with price list
	

	20.5
	The Contractor prepares forecasts of the final total of the Prices for the whole of the service at intervals no longer than 
	As per task order

	Section 3.30 11
	Section 3.31 Data for Option W1
	

	W1.1
	The Adjudicator is (Name)
	the person selected from the ICE-SA Division (or its successor body) of the South African Institution of Civil Engineering Panel of Adjudicators by the Party intending to refer a dispute to him.  (see www.ice-sa.org.za). If the Parties do not agree on an Adjudicator the Adjudicator will be appointed by the Arbitration Foundation of Southern Africa (AFSA).

	W1.2(3)
	The Adjudicator nominating body is: 
	the Chairman of ICE-SA a joint Division of the South African Institution of Civil Engineering and the Institution of Civil Engineers (London) (see www.ice-sa.org.za ) or its successor body

	W1.4(2)
	The tribunal is: 
	Arbitration

	W1.4(5)
	The arbitration procedure is 
	the latest edition of Rules for the Conduct of Arbitrations published by The Association of Arbitrators (Southern Africa) or its successor body.

	
	The place where arbitration is to be held is
	Megawatt Park, Johannesburg, South Africa

	
	The person or organisation who will choose an arbitrator 

· if the Parties cannot agree a choice or

· if the arbitration procedure does not state who selects an arbitrator, is
	The Chairman for the time being or his nominee of the Association of Arbitrators (Southern Africa) or its successor body.



	Section 3.32 12
	Section 3.33 Data for secondary Option clauses
	Section 3.34 

	X1
	Price adjustment for inflation
	

	X1.1
	The base date for indices is 
	One month prior to tender closing date / successful negotiation date

	Proportion
	Linked To Index For
	Index Prepared By

	0.15
	Transport
	Seifsa Table L1

	0.30
	Other / Durable Goods
	Stats SA Table B1 – CPI Headline

	0.40
	Labour
	Seifsa Table C3

	0.15
	non-adjustable

	1.00
	Total

	
	

	X2
	Changes in the law
	[image: image4.emf]

	X4
	Parent company guarantee
	No data is required for this Option

	
	
	

	X12.1(1)
	The Client is (Name): 
	_________________________________________

	
	Address
	_________________________________________

	
	Contact details
	_________________________________________

	
	Telephone:
	_________________________________________

	
	Fax
	_________________________________________

	
	e-mail
	_________________________________________

	X12.1(4)
	The Partnering Information is in
	Part 3 Scope of Work, section C3. N/A

	X12.2(1)
	The Client’s objective is:
	

	X13
	Performance bond
	N/A

	
	
	

	X18
	Limitation of liability
	

	X18.1
	The Contractor’s liability to the Employer for indirect or consequential loss is limited to
	R0.0 (zero Rand)

	X18.2
	For any one event, the Contractor’s liability to the Employer for loss of or damage to the Employer’s property is limited to
	R15 million (fifteen million Rand) for any one occurrence or series of occurrences arising out of one event but unlimited during the service period

	X18.3
	The Contractor’s liability for Defects due to his design of an item of Equipment is limited to
	The greater of 

· the total of the Prices at the Contract Date

and 

· the amounts excluded and unrecoverable from the Employer’s insurances 

	X18.4
	The Contractor’s total liability to the Employer, for all matters arising under or in connection with this contract, other than the excluded matters, is limited to
	the total of the Prices other than for the additional excluded matters.

The Contractor’s total liability for the additional excluded matters is not limited. 

The additional excluded matters are amounts for which the Contractor is liable under this contract for

· Defects due to his design, plan and specification,

· Defects due to manufacture and fabrication outside the Affected Property, 

· loss of or damage to property (other than the Employer’s property, Plant and Materials),

· death of or injury to a person and

· infringement of an intellectual property right.

	X18.5
	The end of liability date is 
	Last day of contract.

	X19
	Task Order
	

	X19.5
	The Contractor submits a Task Order programme to the Service Manager within 
	24 Hours of receiving the Task Order

Urgent Task Orders : 12 hours

	Z
	The additional conditions of contract are
	Z1 to Z11 always apply.

	
	

	Z1
	Cession delegation and assignment

	Z1.1
	The Contractor does not cede, delegate or assign any of its rights or obligations to any person without the written consent of the Employer.

	Z1.2
	Notwithstanding the above, the Employer may on written notice to the Contractor cede and delegate its rights and obligations under this contract to any of its subsidiaries or any of its present divisions or operations which may be converted into separate legal entities as a result of the restructuring of the Electricity Supply Industry and the Electricity Distribution Industry. 

	Z2
	Joint ventures N/A

	Z3
	Change of Broad Based Black Economic Empowerment (B-BBEE) status

	Z3.1
	Where a change in the Contractor’s legal status, ownership or any other change to his business composition or business dealings results in a change to the Contractor’s B-BBEE status, the Contractor notifies the Employer within seven days of the change.

	Z3.2
	The Contractor is required to submit an updated verification certificate and necessary supporting documentation confirming the change in his B-BBEE status to the Service Manager within thirty days of the notification or as otherwise instructed by the Service Manager.

	Z3.3
	Where, as a result, the Contractor’s B-BBEE status has decreased since the Contract Date the Employer may either re-negotiate this contract or alternatively, terminate the Contractor’s obligation to Provide the Works.

	Z3.4
	Failure by the Contractor to notify the Employer of a change in its B-BBEE status may constitute a reason for termination. If the Employer terminates in terms of this clause, the procedures on termination are P1, P2 and P4 as stated in clause 92, and the amount due is A1 and A3 as stated in clause 93.

	Z4
	Ethics

	Z4.1
	Any offer, payment, consideration, or benefit of any kind made by the Contractor, which constitutes or could be construed either directly or indirectly as an illegal or corrupt practice, as an inducement or reward for the award or in execution of this contract constitutes grounds for terminating the Contractor’s obligation to Provide the Service or taking any other action as appropriate against the Contractor (including civil or criminal action).

	Z4.2
	The Employer may terminate the Contractor’s obligation to Provide the Service if the Contractor (or any member of the Contractor where the Contractor constitutes a joint venture, consortium or other unincorporated grouping of two or more persons or organisations) is found guilty by a competent court, administrative or regulatory body of participating in illegal or corrupt practices.   

Such practices include making of offers, payments, considerations, or benefits of any kind or otherwise, whether in connection with any procurement process or contract with the Employer or other people or organisations and including in circumstances where the Contractor or any such member is removed from an approved vendor data base of the Employer as a consequence of such practice.

	Z4.3
	Notwithstanding the provisions of core clause 90.2, the procedures on termination in terms of this clause are P1, P2 and P4 as stated in the core clause 92 and the amount due is A1 and A3 as stated in core clause 93.

	
	

	Z5
	Confidentiality

	Z5.1
	The Contractor does not disclose or make any information arising from or in connection with this contract available to Others. This undertaking does not, however, apply to information which at the time of disclosure or thereafter, without default on the part of the Contractor, enters the public domain or to information which was already in the possession of the Contractor at the time of disclosure (evidenced by written records in existence at that time).  Should the Contractor disclose information to Others in terms of clause 25.1, the Contractor ensures that the provisions of this clause are complied with by the recipient.

	Z5.2
	If the Contractor is uncertain about whether any such information is confidential, it is to be regarded as such until notified otherwise by the Service Manager.

	Z5.3
	In the event that the Contractor is, at any time, required by law to disclose any such information which is required to be kept confidential, the Contractor, to the extent permitted by law prior to disclosure, notifies the Employer so that an appropriate protection order and/or any other action can be taken if possible, prior to any disclosure.  In the event that such protective order is not, or cannot, be obtained, then the Contractor may disclose that portion of the information which it is required to be disclosed by law and uses reasonable efforts to obtain assurances that confidential treatment will be afforded to the information so disclosed.

	Z5.4
	The taking of images (whether photographs, video footage or otherwise) of the Affected Property or any portion thereof, in the course of Providing the Service and after the end of the service period, requires the prior written consent of the Service Manager.  All rights in and to all such images vests exclusively in the Employer.  

	Z5.5
	The Contractor ensures that all his sub-Contractors abide by the undertakings in this clause.

	
	

	Z6
	Waiver and estoppel: Add to core clause 12.3:

	Z6.1
	Any extension, concession, waiver or relaxation of any action stated in this contract by the Parties, the Service Manager or the Adjudicator does not constitute a waiver of rights, and does not give rise to an estoppel unless the Parties agree otherwise and confirm such agreement in writing.

	
	

	Z7
	Health, safety and the environment:  Add to core clause 27.4

	Z7.1
	The Contractor undertakes to take all reasonable precautions to maintain the health and safety of persons in and about the execution of the service. Without limitation the Contractor:

· accepts that the Employer may appoint him as the “Principal Contractor” (as defined and provided for under the Construction Regulations 2003 (promulgated under the Occupational Health & Safety Act 85 of 1993) (“the Construction Regulations”) for the Affected Property;

· warrants that the total of the Prices as at the Contract Date includes a sufficient amount for proper compliance with the Construction Regulations, all applicable health & safety laws and regulations and the health and safety rules, guidelines and procedures provided for in this contract and generally for the proper maintenance of health & safety in and about the execution of the service; and

· undertakes, in and about the execution of the service, to comply with the Construction Regulations and with all applicable health & safety laws and regulations and rules, guidelines and procedures otherwise provided for under this contract and ensures that his Sub Contractors, employees and others under the Contractor’s direction and control, likewise observe and comply with the foregoing.

	Z7.2
	The Contractor, in and about the execution of the service, complies with all applicable environmental laws and regulations and rules, guidelines and procedures otherwise provided for under this contract and ensures that his Sub Contractors, employees and others under the Contractor’s direction and control, likewise observe and comply with the foregoing. Likewise, the Contractor undertakes, in and about the execution of the service, to comply with all provisions of the Kriel Power Station ISO 14001 Environmental Management System and all subsequent revisions.

	
	

	Z8
	Provision of a Tax Invoice and interest.  Add to core clause 51

	Z8.1
	Within one week of receiving a payment certificate from the Service Manager in terms of core clause 51.1, the Contractor provides the Employer with a tax invoice in accordance with the Employer's procedures stated in the Service Information, showing the amount due for payment equal to that stated in the payment certificate.

	Z8.2
	If the Contractor does not provide a tax invoice in the form and by the time required by this contract, the time by when the Employer is to make a payment is extended by a period equal in time to the delayed submission of the correct tax invoice.  Interest due by the Employer in terms of core clause 51.2 is then calculated from the delayed date by when payment is to be made.

	Z8.3
	The Contractor (if registered in South Africa in terms of the companies Act) is required to comply with the requirements of the Value Added Tax Act, no 89 of 1991 (as amended) and to include the Employer’s VAT number 4740101508 on each invoice he submits for payment.

	
	

	Z9
	Notifying compensation events

	Z9.1
	Delete from the last sentence in core clause 61.3, “unless the Service Manager should have notified the event to the Contractor but did not”.

	
	

	Z10
	Employer’s limitation of liability

	Z10.1
	The Employer’s liability to the Contractor for the Contractor’s indirect or consequential loss is limited to R0.00 (zero Rand)

	Z10.2
	The Contractor’s entitlement under the indemnity in 82.1 is provided for in 60.1(12) and the Employer’s liability under the indemnity is limited to compensation as provided for under the compensation events stated in this contract.

	
	

	Z11
	Termination: Add to core clause 91.1, at the second main bullet point, fourth sub-bullet point, after the words "against it":  

	Z11.1
	   Or had a judicial management order granted against it.

	
	

	Z12
	Risks and insurance 

	Z12.1
	Delete 83.2 and replace with 

83.2 The insurances are in the joint names of the Parties for their respective rights and interests and provides cover for events arising out of the Contract from the starting date until the end of the service period or a termination certificate has been issued.



	Z12.2
	Delete 84.4 and replace with the following

84.4 Nothing in this Clause limits the obligations, liabilities or responsibilities of the Contractor under the other terms of the Contract or otherwise. Any amounts not insured or not recovered from insurers shall be borne by the Contractor in accordance with these obligations, liabilities or responsibilities.



	Z12.3
	Add Clause 84.5

84.5 The Contractor shall ensure that, where applicable, its sub-Contractor(s) shall take out and maintain in effect adequate Insurances for their employees and property and for work executed by them under the Contract, unless such sub-Contractor(s) are covered by the insurance policies taken out by the Contractor.



	Z12.4
	Add Clause 84.6

84.6 The insurances must be arranged with reputable insurers


Article IV. Annexure A:
Insurance provided by the Employer
These notes are provided as guidance to tendering Contractors and the Contractor about the insurance provided by the Employer. Details of the insurance itself are available from the internet web link given below. 

1. Services provided in a TSC3 contract could include some element of construction or refurbishment as well as a continuous maintenance or operational service activity.  If an event occurs which causes loss or damage, a claim could be made either against the Employer’s “works” type policy which may be in place for the Employer’s portion of the Affected Property concerned or against the Employer’s assets policy which may be in place for the Employer’s portion of the Affected Property concerned, or both.

2. The cover provided and the deductibles under the works policy are different to those under the assets policy.   Each policy has a range of applicable deductibles depending on the location of the Affected Property and the nature of the insurable event.   

3. The Contractor is required in terms of Contract Data for clause 83 to provide cover for the deductibles in the insurance provided by the Employer.  This can be provided from his own resources on a ‘self insured’ basis or obtained by him from his own insurers.   In order to assess the extent of this cover, tendering Contractors and their brokers should consult the internet web link given below and scroll to ‘Format B’ to establish both the cover and the deductibles in relation to the service provided in terms of this contract.

4. Tendering Contractors should note that cover provided by the Employer is only per the policies available on the internet web link listed below and may not be the cover required by the tendering Contractor or as intended by each of the listed insurances in the left hand column of the Insurance Table in clause 83.2.  In terms of clause 83.1 “the Contractor provides the insurances stated in the Insurance Table except any insurance which the Employer is to provide”.  Hence the Contractor provides insurance which the Employer does not provide and in cases where the Employer does provide insurance the Contractor insures for the difference between what the Insurance Table requires and what the Employer provides.

5. If Marine Insurance is required the Contractor needs to obtain a copy of the latest edition of Eskom’s Marine Policies Procedures found at internet website given below.

6. Further information and full details of contractor provided policies and procedures may be obtained from: 

7. The Contractor should generally give further consideration to providing for these additional insurance concepts:

[for Amounts and Periods of Insurance the Contractor deems fit and necessary]

a) Professional Indemnity. If this insurance is purchased on a ‘claims made’ basis this means that the claim must be lodged with Insurers within the period of insurance. Given this feature of the cover, the Consultant should consider continuing the cover for a further period in line with potential liabilities arising out of this contact

i. [Also refer website’s Professional Services Contract Guidance Notes].

b) Products Liability: A special General Liability extension for liability arising out of the Manufacturer’s/Supplier’s/Original Equipment Manufacturer’s defective:

i. production and manufacturing process (workmanship or material), or

ii. product design, or

iii. warnings, instructions, usage and maintenance manuals and specifications.

c) Products Guarantee: For the cost of replacing, reworking or recovering products that have failed to perform their intended function due to faulty design, manufacture, installation, after handover to the Employer.

d) Goods in Trust and under Manufacture or Storage at Manufacturer’s Premises:

i. Where the Contract involves manufacture, and/or fabrication of Plant and Materials, components or other goods to be incorporated into the works, at premises other than the site, the Contractor shall satisfy the Employer that such Plant and Materials, components or other goods for incorporation in the works are adequately insured during manufacture and/or fabrication. Should the Employer have an insurable interest in such items during manufacture or fabrication, such interest shall be noted by endorsement to the Contractor's relevant policies of insurance as well as those of any sub-Contractor.

8. Contract Works SASRIA insurance is subject to the terms exceptions and conditions of the SASRIA coupon policy. Cover and Indemnity is therefore within the scope and to the extent provided by the SASRIA coupon policy.

Annexure C:  Table of low service damages (X17)
	Low Service Damage Description
	Value of Low Service Damages
	Limit of Low Service Damage

	Not completing service as per agreed programme
	0.5% of task order value per day
	Limited to 10% of the Task Order value

	Any rework due to poor workmanship
	Contractor to provide a replacement during the re-do service period
	Contractor cost


C1.3 Forms of Securities 

Annexure A:
Insurance provided by the Employer
These notes are provided as guidance to tendering contractors and the Contractor about the insurance provided by the Employer. The Contractor must obtain its own advice. Details of the insurance itself are available from the internet web link given below. 

9. Services provided in a TSC3 contract could include some element of construction or refurbishment as well as a continuous maintenance or operational service activity.  If an event occurs which causes loss or damage, a claim could be made either against the Employer’s “works” type policy which may be in place for the Employer’s portion of the Affected Property concerned or against the Employer’s assets policy which may be in place for the Employer’s portion of the Affected Property concerned, or both.

10. The cover provided and the deductibles under the works policy are different to those under the assets policy.   Each policy has a range of applicable deductibles depending on the location of the Affected Property and the nature of the insurable event.   

11. The Contractor is required in terms of Contract Data for clause 83 to provide cover for the deductibles in the insurance provided by the Employer.  This can be provided from his own resources on a ‘self insured’ basis or obtained by him from his own insurers.   In order to assess the extent of this cover, tendering contractors and their brokers should consult the internet web link given below and scroll to ‘Format TSC3’ to establish both the cover and the deductibles in relation to the service provided in terms of this contract.

12. Tendering contractors should note that cover provided by the Employer is only per the policies available on the internet web link listed below and may not be the cover required by the tendering contractor or as intended by each of the listed insurances in the left hand column of the Insurance Table in clause 83.2.  In terms of clause 83.1 “the Contractor provides the insurances stated in the Insurance Table except any insurance which the Employer is to provide”.  Hence the Contractor provides insurance which the Employer does not provide and in cases where the Employer does provide insurance the Contractor insures for the difference between what the Insurance Table requires and what the Employer provides.

13. If Marine Insurance is required the Contractor needs to obtain a copy of the latest edition of Eskom’s Marine Policies Procedures found at internet website given below.

14. Further information and full details of all Eskom provided policies and procedures may be obtained from: 

http://www.eskom.co.za/Tenders/InsurancePoliciesProcedures/Pages/EIMS_Policies_

From_1_April_2014_To_31_March_2015.aspx 
C1.2 Contract Data

Article V. Part two - Data provided by the Contractor
Completion of the data in full, according to Options chosen, is essential to create a complete contract.

	Section 5.1 Clause
	Section 5.2 Statement
	Section 5.3 Data

	10.1
	The Contractor is (Name):
	_________________________________________

	
	Address
	_________________________________________

	
	Tel No.
	_________________________________________

	
	Fax No.
	_________________________________________

	11.2(8)
	The direct fee percentage is
	______%

	
	The subcontracted fee percentage is
	N/A

	11.2(14)
	The following matters will be included in the Risk Register
	_________________________________________

	11.2(15)
	The Service Information for the Contractor’s plan is in:
	Control Quality Plan

	21.1
	The plan identified in the Contract Data is contained in:
	Safety, Health & Environment Plan

	24.1
	The key persons are:
	

	
	1

Name:
	_________________________________________

	
	Job:
	_________________________________________

	
	Responsibilities:
	_________________________________________

	
	Qualifications:
	_________________________________________

	
	Experience:
	_________________________________________

	
	2

Name:
	_________________________________________

	
	Job
	_________________________________________

	
	Responsibilities:
	_________________________________________

	
	Qualifications:
	_________________________________________

	
	Experience:
	_________________________________________

	
	
	_________________________________________

	
	
	CV's (and further key person's data including CVs) are in _______________________________

	A
	Priced contract with price list
	

	11.2(12)
	The price list is in
	The document called “price list” in Part 2 C2.2 of this tender

	11.2(19)
	The tendered total of the Prices is
	This is a rates based tender


Part 2: Pricing Data

TSC3 Option A

	Document reference
	Title
	No of pages

	C2.1
	Pricing assumptions: Option A
	2

	C2.2
	The price list 
	4


C2.1 Pricing assumptions: Option A

1. The conditions of contract 

1.1. How work is priced and assessed for payment

Clause 11 in NEC3 Term Service Contract, June 2005 (TSC3) core clauses and Option A states:

	Identified and defined terms
	11

11.2
	(12) The Price List is the price list unless later changed in accordance with this contract.



	
	
	(17) The Price for Services Provided to Date is the total of 

· the Price for each lump sum item in the Price List which the Contractor has completed and

· where a quantity is stated for an item in the Price List, an amount calculated by multiplying the quantity which the Contractor has completed by the rate.



	
	
	(19) The Prices are the amounts stated in the Price column of the Price List. Where a quantity is stated for an item in the Price List, the Price is calculated by multiplying the quantity by the rate.




This confirms that Option A is a priced contract where the Prices are derived from a list of items of service which can be priced as lump sums or as expected quantities of service multiplied by a rate or a mix of both.

1.2. Function of the Price List

Clause 54.1 in Option A states: “Information in the Price List is not Service Information”.  This confirms that instructions to do work or how it is to be done are not included in the Price List but in the Service Information.  This is further confirmed by Clause 20.1 which states, “The Contractor Provides the Service in accordance with the Service Information”. Hence the Contractor does not Provide the Service in accordance with the Price List.   The Price List is only a pricing document.  

1.3. Link to the Contractor’s plan

Clause 21.4 states “The Contractor provides information which shows how each item description on the Price List relates to the operations on each plan which he submits for acceptance”.  Hence when compiling the price list, the tendering Contractor needs to develop his first clause 21.2 plan in such a way that operations shown on it can be priced in the price list  and result in a satisfactory cash flow in terms of clause 11.2(17). 

1.4. Preparing the price list

It will be assumed that the tendering Contractor has read Pages 14, 15 and 73 of the TSC3 Guidance Notes before preparing the price list.  Items in the price list may have been inserted by the Employer and the tendering Contractor should insert any additional items which he considers necessary.  Whichever party provides the items in the price list the total of the Prices is assumed to be fully inclusive of everything necessary to Provide the Service as described at the time of entering into this contract. 

1 As the Contractor has an obligation to correct Defects (core clause 42.1) and there is no compensation event for this unless the Defect was due to an Employer’s risk, the lump sum Prices and rates must also include for the correction of Defects.

2 If the Contractor has decided not to identify a particular item in the price list at the time of tender the cost to the Contractor of doing the work must be included in, or spread across, the other Prices and rates in the price list in order to fulfil the obligation to complete the service for the tendered total of the Prices.  

3 There is no adjustment to lump sum prices in the price list if the amount, or quantity, of work within that lump sum item of service later turns out to be different to that which the Contractor estimated at time of tender. The only basis for a change to the Prices is as a result of a compensation event. See Clause 60.1.

4 Hence the Prices and rates tendered by the Contractor in the price list are inclusive of everything necessary and incidental to Providing the Service in accordance with the Service Information, as it was at the time of tender, as well as correct any Defects not caused by an Employer’s risk. 
5 The Contractor does not have to allow in his Prices and rates for matters that may arise as a result of a compensation event.  It should be noted that the list of compensation events includes those arising as a result of an Employer's risk event listed in core clause 80.1.

1.5. Format of the price list

(From page 73 of the TSC3 Guidance Notes)

Entries in the first four columns in the price list in section C2.2 are made either by the Employer or the tendering Contractor. 

If the Contractor is to be paid an amount for the item which is not adjusted if the quantity of work in the item changes, the tendering Contractor enters the amount in the Price column only, the Unit, Expected Quantity and Rate columns being left blank.

If the Contractor is to be paid an amount for an item of work which is the rate for the work multiplied by the quantity completed, the tendering Contractor enters the rate which is then multiplied by the Expected Quantity to produce the Price, which is also entered.

If the Contractor is to be paid a Price for an item proportional to the length of time for which a service is provided, a unit of time is stated in the Unit column and the expected length of time (as a quantity of the stated units of time) is stated in the Expected Quantity column.

C2.2 the price list
	Maintenance of Fire and Emergency Equipment at Kriel Power Station for a period of Five years

	Item no.
	Description
	Frequency
	Unit
	Qty
	 Rate 
	 Total 

	100
	Preliminary & General
	 
	 
	 
	 
	 

	101
	Medicals / Safety File / Quality File / Induction/Employees Police Clearance 
	Annually
	Each
	5
	 
	 

	102
	Personal Protective Equipment
	Annually
	Each
	5
	 
	 

	103
	Transport (Limited To 100 Km Return Trip Per Day) (Once A Month-Collection)
	As And When Required
	KM
	20400
	 
	 

	104
	Accomodation allowance with annual services
	As And When Required
	Yearly
	5
	 
	 

	105
	Station Wear for Fire & Emergency Risk Personnel
	Yearly
	EA
	5
	 
	 

	106
	Station Wear for Fire & Emergency ERT Members
	Yearly
	EA
	5
	 
	 

	107
	Fire Fighting PPE For Fire Fighters (Complete sets as per 32-128
	As And When Required Basis
	Sum
	1
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	Sub-Total (100)
	 
	 
	 
	 
	 

	 
	Fire Extinguishers
	 
	 
	 
	 
	 

	200
	Fire Extinguisher Service
	 
	 
	 
	 
	 

	201
	9kg DCP Fire Extinguishers
	Once A Year
	EA
	620
	 
	 

	202
	5kg Co2 Fire Extinguishers
	Once A Year
	EA
	480
	 
	 

	203
	2.5kg DCP Fire Extinguishers
	Once A Year
	EA
	40
	 
	 

	204
	1.5kg DCP Fire Extinguishers
	Once A Year
	EA
	60
	 
	 

	205
	50kg DCP Fire Extinguishers
	Once A Year
	EA
	40
	 
	 

	206
	9 Litre Foam Fire Extinguishers
	Once A Year
	EA
	10
	 
	 

	207
	50 Kg Trolley Foam Fire Extinguishers
	Once A Year
	EA
	20
	 
	 

	300
	Extinguishers Redundant to Replace (New)
	 
	 
	 
	 
	 

	301
	9kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	200
	 
	 

	302
	5kg Co2 Fire Extinguishers
	As And When Required Basis
	EA
	200
	 
	 

	303
	2.5kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	75
	 
	 

	304
	1.5kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	50
	 
	 

	305
	50kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	15
	 
	 

	306
	9 Litre Foam Fire Extinguishers
	As And When Required Basis
	EA
	15
	 
	 

	307
	50 Kg Trolley Foam Fire Extinguishers
	As And When Required Basis
	EA
	15
	 
	 

	400
	Pressure Testing of Fire Extinguisher
	 
	 
	 
	 
	 

	401
	9kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	620
	 
	 

	402
	2.5kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	480
	 
	 

	403
	1.5kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	40
	 
	 

	404
	5kg Co2 Fire Extinguishers
	As And When Required Basis
	EA
	60
	 
	 

	405
	50kg DCP Fire Extinguishers
	As And When Required Basis
	EA
	40
	 
	 

	406
	9 Litre Foam Fire Extinguishers
	As And When Required Basis
	EA
	10
	 
	 

	407
	50 Kg Trolley Foam Fire Extinguishers
	As And When Required Basis
	EA
	20
	 
	 

	500
	Refill And Part of Fire Extinguishers
	 
	 
	 
	 
	 

	501
	Refill Fire Extinguishers With 40 % Map Powder
	As And When Required Basis
	Kg
	1800
	 
	 

	502
	Refill Fire Extinguishers with Co2
	As And When Required Basis
	Kg
	1800
	 
	 

	503
	Refill Fire Extinguishers with Foam Concentrate
	As And When Required Basis
	Lt
	500
	 
	 

	504
	Replacements Of Extinguisher Parts e.g. Hoses
	As And When Required Basis
	EA
	200
	 
	 

	505
	Lead Seals and Wire
	As And When Required Basis
	EA
	120
	 
	 

	 
	Sub-Total (200-500)
	 
	 
	 
	 
	 

	600
	Hose Reels
	 
	 
	 
	 
	 

	601
	Service Of Fire Hose Reels
	Once A Year
	EA
	75
	 
	 

	602
	Replace Of Complete Fire Hose Reel 
	As And When Required Basis
	EA
	35
	 
	 

	603
	CP Valve
	As And When Required Basis
	EA
	75
	 
	 

	604
	30 Meter Hose reel Hose
	As And When Required Basis
	EA
	75
	 
	 

	605
	Replacement Of Hose Reel Nozzles
	As And When Required Basis
	 
	1000
	 
	 

	606
	Monthly inspection of Hose Reels
	Monthly
	EA
	75
	 
	 

	700
	Hydrants
	 
	 
	 
	 
	 

	701
	Hydrants Service
	Once A Year
	EA
	70
	 
	 

	702
	Hydrants Heads to Replace
	As And When Required Basis
	EA
	150
	 
	 

	703
	Fire Hydrant Washers
	As And When Required Basis
	EA
	500
	 
	 

	704
	Fire Hydrant Blank Couplings
	As And When Required Basis
	EA
	1000
	 
	 

	705
	Flow And Pressure Readings of Fire Hydrants
	Once A Year
	EA
	75
	 
	 

	706
	Lux Valve for Hydrant Heads
	As And When Required Basis
	EA
	1000
	 
	 

	 
	Sub-Total (600-700)
	 
	 
	 
	 
	 

	 
	Fire Hoses
	 
	 
	 
	 
	 

	800
	Service Of Fire Hoses
	 
	 
	 
	 
	 

	801
	60mm X 30 Meters Hose
	Once A Year
	EA
	140
	 
	 

	802
	45mm X 30 Meters Hose
	Once A Year
	EA
	50
	 
	 

	803
	Pressure Testing of Fire Hoses
	 
	 
	 
	 
	 

	804
	60mm X 30 Meters Hose
	Once A Year
	EA
	140
	 
	 

	805
	45mm X 30 Meters Hose
	Once A Year
	EA
	40
	 
	 

	900
	Fire Hoses Redundant to Replace (New)
	 
	 
	 
	 
	 

	901
	60mm X 30 Meters Hose  (Duraline Type)
	As And When Required Basis
	EA
	150
	 
	 

	902
	45mm X 30 Meters Hose (Duraline Type)
	As And When Required Basis
	EA
	150
	 
	 

	 
	Sub-Total (900-1000)
	 
	 
	 
	 
	 

	1000
	Self-Containing Breathing Apparatus (Serviced and Certification By OEM)
	 
	 
	 
	 
	 

	1001
	Self-Containing Breathing Apparatus Cylinders Service
	Once A Year
	EA
	85
	 
	 

	1002
	Self-Containing Breathing Apparatus Cylinder Compressor Unit (Fixed)
	Once A Year
	EA
	1
	 
	 

	1003
	Self-Containing Breathing Apparatus Service of Backpacks
	Once A Year
	EA
	45
	 
	 

	1004
	Self-Containing Breathing Apparatus of Face Masks
	Once A Year
	EA
	85
	 
	 

	1100
	Hydraulic Equipment (Serviced and Certification By OEM)
	 
	 
	 
	 
	 

	1101
	Service Holmatro Pump
	Once A Year
	EA
	2
	 
	 

	1102
	Service Holmatro Cutters
	Once A Year
	EA
	2
	 
	 

	1103
	Service Holmatro Spreaders
	Once A Year
	EA
	2
	 
	 

	1104
	Service Holmatro Rams
	Once A Year
	EA
	3
	 
	 

	1105
	Service Of Hydraulic Hoses
	Once A Year
	EA
	5
	 
	 

	1106
	Service Of Vetter Bag Equipment With 2 Bags
	Once A Year
	EA
	2
	 
	 

	1200
	Pneumatic Equipment 
	 
	 
	 
	 
	 

	1201
	Vetter Bag (Small)
	Once A Year
	EA
	1
	 
	 

	1202
	Vetter Bag (Medium)
	Once A Year
	EA
	1
	 
	 

	1203
	Vetter Bag Gauge
	Once A Year
	EA
	3
	 
	 

	1204
	High Pressure Hoses
	Once A Year
	EA
	3
	 
	 

	1300
	Pneumatic Equipment Redundant to be replaced
	 
	 
	 
	 
	 

	1301
	Vetter Bag (Small)
	As And When Required Basis
	EA
	1
	 
	 

	1302
	Vetter Bag (Medium)
	As And When Required Basis
	EA
	1
	 
	 

	1303
	Vetter Bag Gauge
	As And When Required Basis
	EA
	1
	 
	 

	1304
	High Pressure Hoses
	As And When Required Basis
	EA
	1
	 
	 

	1400
	Service Of Small Fire Fighting Gear
	 
	 
	 
	 
	 

	1401
	Adjustable Fire Nozzles
	Once A Year
	EA
	50
	 
	 

	1402
	Lockable Fire Lockers
	Once A Year
	EA
	75
	 
	 

	1403
	Wildfire Trailer & Pump Unit Service
	Once A Year
	EA
	1
	 
	 

	1404
	Angus 2200 Portable Pump
	Once A Year
	EA
	1
	 
	 

	1405
	Portable Generator
	Once A Year
	EA
	1
	 
	 

	1406
	Foam Trolleys
	Once A Year
	EA
	20
	 
	 

	1407
	Ground Monitors Complete
	Once A Year
	EA
	10
	 
	 

	1408
	Suction Hoses 
	Once A Year
	EA
	5
	 
	 

	1409
	Foam Branches
	Once A Year
	EA
	30
	 
	 

	1410
	Inline Inductors
	Once A Year
	EA
	20
	 
	 

	1500
	Small Gear Redundant to Replace (New)
	 
	 
	 
	 
	 

	1501
	Lockable Fire Lockers
	As And When Required Basis
	EA
	40
	 
	 

	1502
	Foam Trolleys
	As And When Required Basis
	EA
	5
	 
	 

	1503
	Ground Monitors Complete
	As And When Required Basis
	EA
	2
	 
	 

	1504
	Suction Hoses 
	As And When Required Basis
	EA
	2
	 
	 

	1505
	Adjustable Fire Nozzles
	As And When Required Basis
	EA
	15
	 
	 

	1506
	Safety Signs
	As And When Required Basis
	EA
	750
	 
	 

	1507
	Replenish of 6% Aqueous Film Forming Foam (AFFF) (700 x 25 l Drums)
	As And When Required Basis
	EA
	700
	 
	 

	1508
	Replacement of Old and Obsolete BA Sets (Complete)
	As And When Required Basis
	EA
	35
	 
	 

	1509
	Hydrant Blank Caps
	As And When Required Basis
	EA
	750
	 
	 

	1510
	Inspection Stickers 
	As And When Required Basis
	EA
	10 000
	 
	 

	 
	Sub-Total(1100-1500)
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	Section
	 
	 
	 
	 
	 
	 

	100
	Preliminary & Generals 
	 
	 
	 
	 
	 

	200-500
	Fire Extinguishers 
	 
	 
	 
	 
	 

	600-700
	Horse Reels & Hydrants
	 
	 
	 
	 
	 

	800-900
	Servicing 
	 
	 
	 
	 
	 

	1000-1500
	Replace and Service 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	Total Rand Value excluding VAT and CPA
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1. Introduction

Maintenance and servicing contract is required to keep all fire and emergency equipment at Eskom Kriel Power Station Generation division, Mpumalanga, at an acceptable standard and condition as required by Occupational Health and Safety act 85 of 1993, National Building Regulation no.103 of 1977, Fire Brigade Services Act 99 of 1987 and SANS 1475 Production of Reconditioned Fire Fighting Equipment.

Maintenance and Inspections performed shall be monthly service and inspected to confirm visual operational status of fire equipment. This schedule establishes preventative maintenance of Fire Equipment to minimize the likelihood of breakdowns and constantly ensuring readiness.

2. Supporting Clauses

2.1 Maintenance of Fire Emergency Equipment

2.1.1 Applicability
This document applies to all the Fire & Emergency equipment maintenance at Eskom Kriel Power Station Generation division.
2.1.2 Effective date
This document will be effective from the authorisation date.
2.2 Normative/Informative References

2.2.1 Normative

[1] 
ISO 9001 Quality Management Systems

[2]
OHSAS 18001, Occupational Health and Safety Management Systems, Requirements OHSAS 18001
2007

[3] ISO 14001, Environmental Management Systems, Requirements with guidance for use
  ISO 14001
2004
[4] Eskom Health, Safety, Environmental Management and Quality Policy 32-727

[5] Eskom Standard for Emergency Planning 32-123

[6] Fire Brigade Services Act 99 of 1987
[7] National Environmental Management Act 107/1998 107/1998
[8] NFPA 25, Standard for the Inspection, Testing, and Maintenance of Water-Based Fire Protection Systems.

[9] SANS 1475 Production of Reconditioned Fire Fighting Equipment
2.2.2 Informative
[10] SHE requirements for tender enquiries

[11] SHE tender evaluation and scoring card.

2.3 SHE tender evaluation and scoring card Definitions.

	Term
	Description

	Fire Truck/Engine 
	Fire Fighting Vehicle

	Hazmat Vehicle
	Hazardous Equipment Vehicle for First Responder

	Skid Unit
	Wild Land Fire Fighting Vehicle / Unit

	Small Gear
	Is referred as Circular Saw, Chain Saw, Reciprocating Saw, Cordless Drill, Positive Pressure Ventilator and Electrical Generator


2.3.1 Document:

2.4 
Abbreviations
	Abbreviation
	Description

	CO2
	Carbon Dioxide

	DCP
	Dry Chemical Powder

	OEM
	Original Equipment Manufacturer

	PPV
	Positive Pressure Ventilator

	PVC
	Poly Vinyl Chloride

	SAQCC
	South African Qualification and Certification Committee

	SCBA
	Self-Contained Breathing Apparatus


2.5 
Roles and Responsibilities

2.5.1 Procurement Department

The procurement department to ensure that the successful contractor is accredited and or registered with the following institutions:

· 
South African Bureau of Standards in terms of SABS 1475.

· 
The South African Qualification & Certification Committee for the Fire Industry (SAQCC).

· 
South African Bureau of Standards in terms of SABS 1737:2001.

2.5.2 Service Provider/Partner

a. 
The service provider/partner shall ensure that this scope of work is executed accordingly.

2.5.3 Contract’s Manager / Operations Controller
a. Contract’s Manager shall ensure that the technical evaluation score sheet is supplied to the tender evaluation committee.

b. Contract’s Manager shall verify that the service provider/partner executes this scope of work accordingly.

c. Contract’s Manager shall conduct a quarterly inspection at the service provider/partner off site Workshop to ensure SAQCC Certification validity.

2.6 
Process for Monitoring

a. The service provider will do inspections on fire emergency equipment as in accordance with section 3.3; and submit an inspection report to the contract’s manager.

b. The contract’s manager will conduct a monthly assessment to monitor work progress.

2.7 
Related/Supporting Documents

        
Not Applicable
3. 

Document Content

Scope of work for the maintenance / replacement of fire emergency equipment

The scope comprises the following but is not limited to:

a. Servicing and Maintenance of Fire Extinguishers

b. Periodically repair and replacement of Fire Extinguishers

c. De-rusting, Pressure / Hydrostatic Tests of Fire Extinguishers

d. Service and periodically repair or replacement of Fire Hose Reels and Hydrants in conjunction with Eskom Kriel Maintenance Department  

e. Service, Maintenance, and certification of Hydraulic Rescue equipment

f. Service, Maintenance, and certification of Pneumatic Rescue equipment

g. Maintenance and replacement of Stabilising equipment

h. Maintenance and replacement on Adjustable Fire Fighting Nozzles
i. Service and Maintenance of PPV fans

j. Service and Maintenance of Fire Department Generators 

k. Servicing and Maintenance of complete sets of SCBA 

l. Periodically repair and replacement of complete sets of SCBA

m. Service and Maintenance of SCBA Compressors

n. De-Rust, Chemical Treatment and Hydrostatic Pressure Test on all SCBA Cylinders (Composite/Steel See 3.3)

o. Servicing and Maintenance of Fire Engine Pump and portable Fire Pumps

p. Servicing, Repair and Replacements on Skid Units & Skid Unit Trailers

q. Servicing and Maintenance on hand tools and small gear

r. Maintenance of Fire Fighting Hoses and Replacements

s. Pressure and vacuum test of suction hoses
t. Servicing, Maintenance, and replacement of Foam Trolleys

u. Replacement of Expired Foam Concentrate

v. Ladder Inspection and Load Testing

w. Maintenance and replacement of Portable Lighting equipment

x. Daily, Weekly & Monthly inspections of portable fire equipment

3.1 Inspections


When Inspection date is reached the following is to be done on fire equipment.
· Fire Extinguishers

· Fire Hose Reels

· Fire Hydrants


A Signed comprehensive monthly report to be submitted to Fire Risk Management indicating all work done according to this scope.

3.2 
Services



When service date is reached the following is to be done on fire equipment.

A Signed comprehensive monthly report to be submitted to Fire Risk Management indicating all work done according to this scope.

A. Extinguishers

i. Extinguisher is to be removed from its position and replaced with a serviceable unit. 
ii. Extinguisher to be stripped.

iii. Extinguisher is to be inspected for any defects, such as rust, cracks and any deformities rendering it inoperable.
iv. Extinguisher hoses deteriorated from exposure to the elements are to be replaced.

v. Extinguisher gauges to be checked and calibrated.

vi. Extinguishers that are faded or slightly rusted must be sandblasted and repainted and all decals replaced.

vii. Extinguishers to be pressure tested (See 3.3)
viii. Extinguishers to be supplied with Pressure Test Certificates post service.

ix. Ensure Hydrostatic testing of CO2 extinguishers with Certification when required (See 3.3)
x. Inspection sticker to be added indicating next Service Date

xi. Information / Instruction Stickers to be present on all units. 
xii. PVC covers for extinguishers are in place.

xiii. Ensure Fire extinguisher bracket mountings are in place.
xiv. Ensure that the fire bank has symbolic signs for Extinguishers.

xv. Disposable Certificate supplied when Extinguisher exceeds lifespan.

xvi. Lockable Fire Extinguisher Cabinets to be available at identified locations. 

B. 

Hose Reels
i. Hose Reels to be inspected monthly and indicated on a monthly inspection sticker. 
ii. Nozzles to be inspected and replaced when defective.  
iii. Inspect Isolation Valve’s functionality and repair or replace when defective.

iv. Inspect drum functionality and repair or replace when defective.

v. Inspect waterways for leaks and repair or replace when defective.

vi. Ensure that the fire bank has a symbolic sign for Hose Reels
vii. PVC covers for hose reels.

viii. Next Service date sticker to be supplied on the outside as well on the inside of the drum.

ix. Ensure that all spares are readily available at the Fire Station Storeroom 

C. Hydrants
i. Hydrants to be checked monthly for leaks etc. and any deformities rendering it inoperable.

ii. Monthly Inspection sticker needs to be placed on all units.

iii. Inspection sticker to be placed indicating next Service Date on all units.   
iv. Hydrants to be flushed monthly.

v. Hydrants seals to be in place and replaced if necessary. 
vi. Ensure that the fire Hydrants  Lugs are in good condition, if not load a defect

vii. Ensure that the fire bank has a symbolic sign for hydrants.
viii. Ensure that damaged fire hydrants are reported, and defect are loaded.
ix. Ensure that spares are readily available at the Fire Station Storeroom
D. 

Fire Fighting Equipment
i. Hydraulic / Pneumatic Rescue Equipment
· Replace with spare set of Hydraulic / Pneumatic Equipment at onset of Service.

· Place Service Label and date of next Service on each equipment Serviced.

· Service as per OEM requirements

· Service or replace affected moving parts and critical components.
ii. 
Small Gear and Hand Tools
· All small gear and hand tools should be replaced by a spare set if equipment is 
sent 
away for prolonged period for OEM Servicing

· Replacement of Hand tools and Small Gear

· Service or replace affected moving parts and critical components. 

iii. 
SCBA 
· Cylinders to be Hydrostatic Pressure Tested

· Replacement of redundant Cylinders

· Replacement of redundant Back-Plates

· Replacement of redundant Masks and Harnesses

· Replacement of redundant Demand Valves

· Hydrostatic Pressure Test of cylinders of Fixed Charging Unit

· Replace old & Obsolete Breathing Apparatus (Complete Sets)

iv. 

Wildfire Trailer and Grass Fire Unit
· Wildfire trailer / unit services according to OEM

· Replacement of redundant pump

· Replacement of redundant water tank

· Replacement of redundant piping

· Replacement of redundant high-pressure nozzle

· Redundant Battery Replacement

· Repair or replace Grass Beaters

v. Adjustable Fire Nozzles
· Fire nozzles service

· Replace redundant fire nozzle.

· Repair fixable nozzle with correct parts.

· Service or replace affected moving parts and critical components.
vi. Fire Fighting Hoses (38mm-100mm)
· Replace Male coupling if defective.

· Replace Female coupling if defective.

· Hoses Binding if necessary.

· Replace missing Seals.

· Lug Replacement if damaged

· Replace redundant Fire Fighting Hoses.

vii. Inline Inductors
· Replacement of irreparable inductor 225
· Replacement of irreparable inductor 450
· Service or replace affected moving parts and critical components.
viii. 
Foam Trolleys
· Repair or Replacement of Foam Trolleys if defective
· Replenishment of Foam Concentrate
ix. 
Pressure and vacuum test of suction hoses 75mm to 200mm
· Replacement of Suction Hoses if inoperable

x. Fire Fighting Gear & Office Uniform
· Provide approved Fire Fighting Gear and Office Wear as per Eskom Standard.
· Fire Fighting PPE must comply with NFPA Standards.

xi. 
SCBA mobile and fixed refilling Compressors
· OEM specific service required.

· One set at a time to be send for Servicing.

· Service or replace affected moving parts and critical components.
3.3 Frequency
	DESCRIPTION
	FREQUENCY
	RESPONSIBLE PERSON

	A Signed comprehensive  report to be submitted to Fire Risk Management indicating all work done according to this scope
	Monthly
	Competent person

	All Serviceable Equipment to be allocated a Serviceable sticker to indicate next Service Due Date
	When required
	Competent person

	Service and maintain all 1 - 50kg DCP extinguisher
	Annual
	Competent person

	Service and maintain all 2 – 5kg co2 extinguishers
	Annual
	Competent person

	Service and maintain all 1 - 50kg Foam extinguisher
	Annual
	Competent person

	Pressure test 1 – 50kg DCP extinguishers
	Annual
	Competent person

	Pressure test 1 – 50kg Foam extinguishers
	Annual
	Competent person

	Hydrostatic Pressure test 2 – 5kg co2 extinguishers
	10 Yearly
	OEM

	Recharge 1 – 50kg DCP extinguishers
	Annual
	Competent person

	Recharge 2 – 5kg co2 extinguishers
	Annual
	Competent person

	Recharge 1 – 50kg Foam extinguishers
	Annual
	Competent person

	Reconditioning of all DCP extinguishers 1 – 50kg
	When required
	Competent person

	Reconditioning of all Foam extinguishers 1 – 50kg
	When required
	Competent person

	Reconditioning of all co2 extinguishers 2 – 5kg 
	When required
	Competent person

	Testing and reconditioning of all inline foam inductors
	Annual
	Competent person

	Test and service of fire hose reels
	Annual
	Competent person

	Pressure test of delivery hoses 38 mm to 65mm
	Annual
	Competent person

	Pressure and vacuum test of suction hoses 75mm to 200mm
	Annual
	Competent person

	Hydrostatic Pressure test of SCBA cylinders (Steel / Composite)
	10 Yearly
	OEM

	Refill 300 bar SCBA cylinders
	When required
	Competent person

	De-rusting/chemical treatment of SCBA cylinders
	When required
	OEM

	Test and service of hydrants
	Annual
	Competent person

	Service of portable and floatable fire pump
	Annual
	OEM

	Service of hydraulic rescue set (Dye pen test)
	Annual
	OEM

	Inspection and service of Vetter bags
	Annual
	OEM

	Vacuum pressure and delivery test of vehicle pump
	Annual
	OEM

	SERVICE OF SMALL GEAR. 

· Circular Saw

· Portable Generator

· PPV 

· Chain Saw
	Annual
	OEM

	SCBA. 

· Replacement of redundant Cylinders (Steel / Composite)

· Replacement of redundant Back-Plates
· Replacement of redundant Masks and Harnesses
· Replacement of redundant Demand Valves
·  Replace old & Obsolete Breathing Apparatus (Complete Sets)
	When required
	OEM

	SCBA compressor service (Mobile and Fixed)
	Annual
	OEM

	Ladder Inspection (Dye pen testing)
	Annual
	Competent person

	Service skid units
	Bi-Annual
	OEM

	Service skid units’ trailers
	Bi-Annual
	OEM

	Fire equipment boxes/ PVC cover
	When required
	Competent person

	Service and Replacement of adjustable Fire Nozzles
	When required
	Competent person

	Winch to be Load Tested
	Annual
	Competent person

	Safety signs for emergency equipment
	When required
	Competent person

	3.4 Description of Critical Spares


	
	

	DESCRIPTION
	FREQUENCY
	RESPONSIBLE PERSON



	EXTINGUISHERS SPARES

	A. Valve assembly complete
	As & when required
	Competent person

	B. Pressure gauge
	As & when required
	Competent person

	C. Syphon tube 
	As & when required
	Competent person

	D. Discharge hose
	As & when required
	Competent person

	E. Valve seat
	As & when required
	Competent person

	F. Seal ring
	As & when required
	Competent person

	G. Instruction label
	As & when required
	Competent person

	H. Monthly inspection sticker
	As & when required
	Competent person

	I. Replacement of foam concentrate
	As & when required
	Competent person

	J. Replacement of all scrapped extinguisher
	As & when required
	Competent person

	CO2 EXTINGUISHERS SPARES

	A. Valve assembly complete
	As & when required
	Competent person

	B. Safety disc
	As & when required
	Competent person

	C. Syphon tube
	As & when required
	Competent person

	D. Discharge horn
	As & when required
	Competent person

	E. Discharge hose
	As & when required
	Competent person

	F. Instruction label
	As & when required
	Competent person

	G. Monthly inspection label
	As & when required
	Competent person

	H. Replacement of all scrapped extinguisher
	As & when required
	Competent person

	FIRE HOSE REELS SPARES

	A. Stop valve
	As & when required
	Competent person

	B. 30m PVC hose
	As & when required
	Competent person

	C. Gland packing
	As & when required
	Competent person

	D. Nozzle
	As & when required
	Competent person

	E. Clamps
	As & when required
	Competent person

	F. Instruction label
	As & when required
	Competent person

	G. Monthly inspection sticker
	As & when required
	Competent person

	H. Replacement reel
	As & when required
	Competent person

	I. Replacement on waterways
	As & when required
	Competent person

	FIRE FIGHTING HOSE SPARES 

	A. Male coupling
	As & when required
	Competent person

	B. Female coupling
	As & when required
	Competent person

	C. Binding
	As & when required
	Competent person

	D. Seal
	As & when required
	Competent person

	E. Replacement lug
	As & when required
	Competent person

	F. Replacement hose 45 mm
	As & when required
	Competent person

	G. Replacement hose 65mm
	As & when required
	Competent person

	H. Replacement hose 38mm
	As & when required
	Competent person

	I. Replacement hose 100mm
	As & when required
	Competent person

	J. Suction hose spares
	As & when required
	Competent person

	K. Seal
	As & when required
	Competent person

	L. Coupling
	As & when required
	Competent person

	M. Binding
	As & when required
	Competent person

	N. Replacement hoses
	As & when required
	Competent person

	SCBA CYLINDERS SPARES

	A. Valve assembly complete
	As & when required
	Competent person

	B. Seals
	As & when required
	Competent person

	C. Replacement of scrapped SCBA cylinder
	As & when required
	Competent person

	INLINE INDUCTORS SPARES

	A. Siphon tube
	As & when required
	Competent person

	B. Induction valve assembly
	As & when required
	Competent person

	C. Male coupling 
	As & when required
	Competent person

	D. Female coupling
	As & when required
	Competent person

	E. Separate lug for instantaneous coupling
	As & when required
	Competent person

	F. Seal for 65mm instantaneous coupling
	As & when required
	Competent person

	G. Seal for induction valve assembly
	As & when required
	Competent person

	H. Replacement of irreparable inductor 225
	As & when required
	Competent person

	I. Replacement of irreparable inductor 450
	As & when required
	Competent person

	HYDRAULIC RESCUE EQUIPMENT SET SPARES

	A. Spreader tips 
	As & when required
	Competent person

	B. Spreader arms 
	As & when required
	Competent person

	C. Cutter blades 
	As & when required
	Competent person

	D. Hydraulic oil
	As & when required
	Competent person

	E. Carburettor kit
	As & when required
	Competent person

	F. Pull start mechanism
	As & when required
	Competent person

	G. Internal piston
	As & when required
	Competent person

	H. Oil seal
	As & when required
	Competent person

	I. Quick release coupling
	As & when required
	Competent person

	J. High pressure pipe
	As & when required
	Competent person

	K. Spark plug
	As & when required
	Competent person

	PORTABLE PUMP SPARES

	A. Gland packing
	As & when required
	Competent person

	B. Gauges
	As & when required
	Competent person

	C. Primer oil
	As & when required
	Competent person

	D. Primer
	As & when required
	Competent person

	E. Primer belies.
	As & when required
	Competent person

	F. Spark plug
	As & when required
	Competent person

	G. Discharge valve
	As & when required
	Competent person

	AIRBAGS SPARES (VETTERBAG)

	A. O rings
	As & when required
	Competent person

	B. Airbag replacement 16 ton
	As & when required
	Competent person

	C. Airbag replacement 32 ton
	As & when required
	Competent person

	D. Airbag replacement 64 ton
	As & when required
	Competent person

	E. Gauges
	As & when required
	Competent person

	F. High pressure air pipe with quick release coupling
	As & when required
	Competent person

	G. Screw in connection to connect to SCBA cylinder
	As & when required
	Competent person
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7.1 
Roles and Responsibilities

7.1.1 Procurement Department

The procurement department to ensure that the successful contractor is accredited and / or registered as an Emergency Services service company actively involved in the provision of fire and emergency services in the industrial environment. 

7.1.2 Service Provider

The Service Provider is required to provide onsite Maintenance Services 0f all Fire Fighting equipment as indicated in the Scope of Work through professionally trained contract employees at Kriel Power Station. 
It is expected that the Service Provider shall adhere to the staff requirements set out in Annexure 1 of this scope of work.  The Service Provider must comply with the OSH Act and Eskom Health Safety and Environmental Policies, SHE specifications and Generation Operational Standards.  To that end, the Service Provider must appoint a suitably qualified safety officer who shall visit the Kriel Power Station at regular intervals but not less than monthly to review the Contractor safety file, conduct Job Observations and safety meetings.  
7.1.3 Contract’s Manager / Operations Controller
· Contract’s Manager shall ensure that the technical evaluation score sheet is supplied to the tender evaluation committee.

· Contract’s Manager shall verify that the Service Provider executes this scope of work accordingly. 

7.2 
Process for Monitoring


The Employer through the Service Provider Base Manager will hold formal weekly meetings to 
measure performance on an ongoing basis.  Regular reviews and audits shall be conducted for the 
compliance of the content of this document.  The SAP Plant Equipment Maintenance Management 
System shall be used to track or assess the scheduled inspection of equipment.
7.3 Related/Supporting Documents

* RIR0113 
- Kriel Emergency Preparedness Plan 
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C3.1: Employer’s service Information

1 Management strategy and start up.

1.1 The Contractor’s plan for the service
The Contractor to submit a mobilisation plan to Service Manager within two weeks, after contract award.

1.2 Management meetings

Regular meetings:

	Title and purpose
	Approximate time & interval
	Location
	Attendance by:

	Risk register and Safety events
	Monthly on 25th or Friday before the 25 if on a weekend or public holiday of the month
	On site
	 Contractors Representative and the Contracts Manager on shift 

Service Manager and safety officer

	Overall contract progress, Assessment and feedback session
	Monthly on 25th or Friday before the 25 if on a weekend or public holiday of the month
	On site
	Employer Rep, Contractor Rep and the contract Manager on shift, Cost engineer

	Emergency Preparedness Meeting
	 Ad-hoc basis
	On Site
	Employers Rep and Contracts Manager

	Contractors SHE meeting site
	Once a month on notification Usually a Tuesday morning
	Off site
	Contracts Manager and SHE officer


Meetings of a specialist nature may be convened as specified elsewhere in this Service Information or if not so specified by persons and at times and locations to suit the Parties, the nature and the progress of the service.  Records of these meetings shall be submitted to the Service Manager by the person convening the meeting within five days of the meeting.  

All meetings shall be recorded using minutes or a register prepared and circulated by the person who convened the meeting. Such minutes or register shall not be used for the purpose of confirming actions or instructions under the contract as these shall be done separately by the person identified in the conditions of contract to carry out such actions or instructions.  

1.3 Contractor’s management, supervision and key people

The Contractor to supply organograms, showing his personal and their lines of authority and communication.

Please also supply CV, of the managers and key personal including the SHE officer
Please supply proof of HPCSA registration of the entire group of employees.  

Prior to contract start the Contractor must provide the following information to the satisfaction of the Employer:

· Provide a list of all the potential fire fighters/ medics you wish to employ on the MpumaCare site with certified copies of their identity documents.  

· Cv’s of the officers to be submitted with reference to any previous sites worked on

· Statement confirming that the medical service business complies with the minimum wage requirements in terms of Sectorial determination 6

· Submit fingerprint screening classification by the criminal-record centre of the Saps for all medics/ fire fighters as proof that they have not been found guilty of a criminal offence specified in the schedule (in previous 10 years) 

· Psychological and physiological reports for all fire fighters/ medics that will be employed for this project (fit and proper person)

· Confirmation that the fire fighters/ medics have not been found guilty of improper conduct in terms of the private security industry regulation act 2001 (act no. 56 of 2001) (in previous 5 years)

1.4 Provision of bonds and guarantees

N/A

1.5 Documentation control

All communication will be in writing as per the contract. Please state the clause that is used, with reference to the communication.

· All documents are to be filled in date order in a durable PVC lever ach file with boxing.

· A file indexing is to be adhere too, the Contracts file structure procedure

· Reports are to be in word, excel power point format compatible with office 2010 these may be emailed to the Service Manager and a hard copy placed on file.

· Contractual communications will be in the form of properly compiled letters or forms attached to e mails and not as a message in the e mail itself.

· On emailing, please send a copy to The Contractors address (to be issued on contract award)

· All instructions are to be from the Service Manager only.
1.6 Invoicing and payment

The invoice needs to have all supporting documentation attached to the invoice, posting sheets, equipment registers and signed off by both parties.

Within one week of receiving a payment certificate from the Service Manager in terms of core clause 51.1, the Contractor provides the Employer with a tax invoice showing the amount due for payment equal to that stated in the Service Manager’s payment certificate.  

The Contractor shall address the tax invoice to:

and include on each invoice the following information:

· Name and address of the Contractor and the Service Manager; 

· The contract number and title;

· Contractor’s VAT registration number;

· The Employer’s VAT registration number 4740101508;

· Description of service provided for each item invoiced based on the Price List;

· Total amount invoiced excluding VAT, the VAT and the invoiced amount including VAT;

· (add other as required)

Add procedures for invoice submission and payment (e. g. electronic payment instructions)

1.7 Contract change management 

N/A

1.8 Records of Defined Cost to be kept by the Contractor
All actual costs relating to the Price list need to be copied and the original forwarded to the Services Manager on the assessment for the months works.

So that payments can be verified to the invoice.

1.9 Insurance provided by the Employer
First read TSC3 Core Clause 86.1 and then add anything necessary for the management of insurance related issues such as a cross reference to where procedures for making claims can be found.  Also provide contact details for persons capable of being able to answer any insurance related queries the Contractor may have, as well as to whom the information required by Marine Insurance (if any) may be addressed.  

1.10 Training workshops and technology transfer

Staffs are required to be trained on carrying out the procedure on first aid level testing on a regular basis. 

Supervisors or shift leader are to be evaluated on the procedure for incident command control and the sequence of events 

Staff is also required to be checked on the procedure for treating patients.

BLS and ILS need regular refresher training.

Emergency medical staff is to be tested on map reading and dispatching to a gridlines regular.

Training on customer interfacing.

Awareness training on Kriel OSHAS 18001 and ISO 14001 management system requirements

1.11 Design and supply of Equipment

N/A.

1.12 Things provided at the end of the service period for the Employer’s

1.12.1 Equipment

All equipment and vehicles that has been purchased by the Employer will remain the property of the Employer.

1.12.2 Information and other things

All data files and computer data needs to be handed over to the Service Manager on termination or expiry of the contract.
1.13 Management of work done by Task Order

Task order to be issued on a monthly base for routine work and for ad hoc requests.

Many considerations can apply to Task Orders, such as availability of resources, arrangements for emergency work, Task Order reporting (work carried out and service results), assessment of additional Prices for service not included in the Price List etc.

	
	Engineering and Construction Short Contract

Task Order
	Contract Nr:


	TITLE OF THE CONTRACT:
	Supply of Fire and Emergency Medical Services and Emergency Medical 

Service Consumables for Kriel Power Station 


	CONTRACTOR:
	EMPLOYER:

	Contact Person:
	Contact Person: 

	Address:


	Address: 



	Telephone No.:
	Telephone No.: 

	Fax No.:
	Fax No.: 

	THE TASK IS:
	Problem area


	The Employer is represented for this Task by:
	Contact Person: 

	
	Address: 



	
	Telephone No.:

	
	Fax No.: 


Please carry out the Task in accordance with the above referenced contract, which includes the Data, stated in this Task Order 

	Activities selected from the Price List for this Task 
	Unit
	Qty
	Rate
	Price

	Item
	Description
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	Total for this Task Order 
	

	


Start date: …………………………                                 End date:               

Amplify the Works and Site Information, if necessary, regarding anything to be provided by either Party to the other and any particular plans or interfaces for this Task. 

	.................................................................................................................................................................................................................................................................................................................................................................................................................................................................................................................

	Accepted by the Contractor:
......................................................
PRINT NAME
	..........................................................
SIGNATURE
	....................................................
DATE

	Employer:
......................................................
PRINT NAME
	..........................................................
SIGNATURE
	....................................................
DATE


2 Health and safety, the environment and quality assurance

2.1 Health and safety risk management

3.1.1
HEALTH AND SAFETY REQUIREMENTS

Contractors and their sub-Contractors shall at all times ensure compliance with all relevant Occupational Health and Safety Act 85 of 1993 and any regulations or by-laws of any local or statutory authority.

The Contractor acts in accordance with the health and safety requirements stated in the Works Information.

In carrying out its obligations to the Employer in terms of this contract; in providing the Works; in using Plant, Materials and Equipment; and while at the Site for any reason, the Contractor complies and procures and ensures the compliance by its employees, agents, Sub Contractors and mandatories with:

· the provisions of the Occupational Health and Safety Act 85 of 1993 (as amended) and all regulations in force from time to time in terms of that Act (“the OHSA”) 

•
the MpumaCare “Health, Safety and Environmental specifications for Contractors” document attached to the Works Information (as amended from time to time) and such other MpumaCare Safety Regulations as are applicable to the Works and are provided in writing to the Contractor . The MpumaCare Regulations may be amended from time to time by the Employer and all amendments will be provided in writing to the Contractor. The Contractor complies with the provisions of the latest written version of the Regulations with which it has been provided 

•
the health and safety and Environmental plan prepared by the Contractor in accordance with the SHEQ Requirements

(The OHSA and the MpumaCare Regulations are collectively referred to as the “SHEQ Requirements”).

The Contractor, at all times, considers itself to be the “Employer” for the purposes of the OHSA and shall not consider itself under the supervision or management of the Employer with regard to compliance with the SHEQ Requirements, the Contractor shall furthermore not consider itself to be a subordinate or under the supervision of the Employer in respect of these matters. The Contractor is at all times responsible for the supervision of its employees, agents, Sub Contractors and mandataries and takes full responsibility and accountability for ensuring they are competent, aware of the SHEQ Requirements and execute the Works in accordance with the SHEQ Requirements.

The Contractor acknowledges that it is fully aware of the requirements of all the above and undertakes to employ only people who have been duly authorized in terms thereof and who have received sufficient training to ensure that they can comply therewith.

The Contractor ensures that all statutory appointments and appointments required by any MpumaCare Regulations are made and that all appointees fully understand their responsibilities and is trained and competent to execute their duties. The Contractor supervises the execution of their duties by all such appointees.

The Contractor shall appoint a person who will liaise with the MpumaCare Safety/ Environmental Officer responsible for the premises relevant to this contract. The person so appointed shall, on request:

•
supply the Safety/ Environmental Officer with copies of minutes of all Health and Safety Committee meetings, whenever they are required to do so.

•
supply the Safety/Environmental Officer with copies of all appointments in respect of employees employed on this contract, in terms of the Act and Regulations and shall advise the MpumaCare Safety Officer of any changes thereto.

The Employer, or any person appointed by the Employer, may at any stage during the period of this contract:

•
conduct health and safety and Environmental audits regarding all aspects of compliance with the SHEQ Requirements, at any off-site place of work, or the site establishment of the Contractor;

•
refuse any employee, Sub Contractor or agent of the Contractor access to the premises if such person has been found to commit an unsafe act or any unsafe working practice or is found not to be qualified or authorised in terms of the SHEQ Requirements;

•
Issue the Contractor with a stop order should the Employer become aware of any unsafe working procedure or condition or any non-compliance with any provision of the SHEQ Requirements.

The Contractor immediately reports any disabling injury as well as any threat to health or safety of which it becomes aware at the Works or on the Site to the Employer’s Representative. 
The Contractor immediately reports any environmental incident as well as any threat to the environment of which it becomes aware at the Works or on the Site to the Employer’s Representative
The Contractor undertakes not to do, or not to allow anything to be done which will contravene any of the provisions of the Act, Regulations or Safety and Operating Procedures as well as provisions in the Kriel Power Station Environmental Management System.

.

The Contractor appoints a person, qualified in accordance with the SHEQ Requirements, as the liaison with the MpumaCare Safety/Environmental Officer for all matters related to health and safety, this person shall be contactable 24 hours a day.

The Contractor confirms that it has been provided with sufficient written information regarding the health and safety as well as Environmental arrangements and procedures applicable to the Works to ensure compliance by it and all employees, agents, Sub Contractors or mandataries with the SHEQ Requirements while providing the Works in terms of this contract.  As such, the Contractor confirms that this contract and the relevant Regulations referred to in this contract constitute written arrangements and procedures between the Contractor and the Employer regarding health and safety for the purposes of section 37(2) of the OHSA.

The Contractor agrees that the Employer is relieved of any and all of its responsibilities and liabilities in terms of Section 37(1) of OHSA in respect of any acts or omissions of the Contractor, and the Contractor’s employees, agents or Sub-Contractors, to the extent permitted by the OHSA.

The Contractor hereby indemnifies the Employer and holds the Employer harmless in respect of any and all loss, costs, claims, demands, liabilities, damage, penalties or expenses that may be made against the Employer and/or suffered or incurred by the Employer (as the case may be) as a result of, any failure of the Contractor, its employees, agents, Sub Contractors and/or mandataries to comply with their obligations in terms of this clause 18, and/or the failure of the Employer to procure the compliance by the Contractor , its employees, agents, Sub Contractors and/or mandataries with their responsibilities and/or obligations in terms of or arising from the OHSA.

In carrying out their obligation as the mandatory to the Employer for this contract in terms of the Kriel Power Station ISO 14001 Environmental Management System and applicable legal and other requirements associated with the Works, the Contractor ensures that they comply with the System requirements when Providing the Services or using plant, materials or equipment.  
3.1.2 TRANSPORTATION OF PASSENGERS:

It is a legal requirement to provide safe transportation of Eskom and Contractor employees – therefore the following will be enforced:

•
All passengers must be transported in a closed vehicle with proper and adequate seating, fitted with safety belts for the number of passengers to be transported.  No passengers may be transported on the back of a light delivery vehicle (ldv) whether open or closed.
•
Tools and equipment must be properly secured.

•
Only authorised drivers that comply with the road transport act, may transport passengers.
•
Proof must be submitted on request in terms of valid roadworthiness of the vehicle/s.

•
The above must apply to on site and off site transportation of passengers.

3.1.4    SHEQ INDUCTION COURSE
•
All the employees of the Contractor must attend a SHEQ induction course before they will be allowed to work on the emergency Site and vehicles. It is the responsibility of the Contractor to ensure that all employees have attended the safety induction. 

3.1.5     LOCAL SAFETY PROCEDURES
•
The Contractor adheres to all local procedures. A list of local procedures are available on request from the Employer
3.1.6
INCIDENTS / ACCIDENTS
•
Incidents and accidents must be reported and investigated.  All incidents must also be reported to the Employer within 4 hours. 

•
First aid must be made available by the Contractor.  The availability of the Contractor’s own first aid or environmental response does not relieve the Contractor of his obligation to report and investigate the incident.

3.1.7
FIRE PREVENTION
•
Fire prevention and protection requirements to which the Contractor must comply.

Please ensure that there are personal trained to use fire equipment and all vehicles to have an extinguisher.
3.1.8
PROTECTIVE EQUIPMENT AND CLOTHING
•
The Contractor supplies his own personal protective equipment and uniform necessary to carry out the Emergency medical rescue and fire fighting work. 

•
The Contractor is also responsible to inspect and maintain such equipment as required in terms of the OHS Act/ NFPA/ and Eskom SHEQ procedures.

3.1.9
INSPECTION OF EQUIPMENT
•
The Contractor’s equipment is inspected by the Service Manager on arrival at the site.

•
The following documentation is required to accompany the equipment where applicable:  copies of all test certificates and maintenance records.

•
If the equipment is found to be in an unsatisfactory condition or if insufficient maintenance has been carried out on the equipment then it will not be approved for use on Site. A list of all emergency medical equipment and description of the equipment must be submitted to the Service Manager at least 2 days prior to the occupation date. 




All vehicles will be maintained so as to prevent any leakage or spillage of fluids
•
Training of working at heights operators must comply with the Works Information and statutory requirements.

3.1.10
DOCUMENTATION
The Contractor is responsible to have the following documentation available on site in accordance 

· A copy of the OHS Act.

· Copies of all site accident report forms as required by the OHS Act.

· Copies of minutes of health and safety meetings held on site.

· Copies of inspection reports produced by the accident prevention officer
· Copies of all relevant SHEQ procedures and associated documents

The Contractor shall comply with the health and safety requirements contained in Scope Of Work Pg 9 3.1 this Service Information. 
3.1.11
RISK REGISTER

	Category
	Hazard Identification
	What is the Root Cause of the Hazard?
	What are the Consequences?

	Threats and Intimidation of employees and Contractors by striking groups
	Threats and Intimidation of employees and Contractors by striking groups
	Striking groups/ labour force
	Death/Injury/Damage 

	Community Actions towards Kriel PS
	Community
	Unhappy community due to site rules or strikes
	Death/Injury/Damage 

	Labour Unrest
	Unrest
	un happy labour due to IR issues or payments
	Death/Injury/Damage 

	Militant Groups                   (Trade unions, youth league, striking work force, local community members)
	Militant groups of people
	Political issues
	Death/Injury/Damage 

	Malicious damage to plant and property on site
	people
	Un happy labour due to IR issues or payments
	Damage property and loss of production

	Stone throwing
	people
	Un happy labour due to IR issues or payments
	Damage / Injury / Death

	Vehicle Driving
	Vehicle accident
	Recklessness/Poor judgement/human error
	Death/Injury/Damage 

	Capabilities of Emergency medical Contractor on site
	Capabilities of Emergency staff
	not fully trained staff  lack of knowledge
	losses of life / equipment and materials

	Procedures not been adhered too
	understanding of procedures
	Not sharing information or lack of training 
	losses of life/ equipment and materials 

	Arson
	people
	un happy labour due to IR issues or payments
	Death/Injury/Damage 

	Assault
	people
	 
	Death/Injury/Damage 

	Bomb and threats
	people
	 
	Death/Injury/Damage 

	Working with Hazardous substances
	Suffocation/poisoning/Fire/explosion
	Poor judgement/control/human error
	Death/Injury/Damage 

	Theft of equipment and materials (including copper)
	Equipment and materials un attended
	un attended or not secure  plant
	losses of plant and equipment and materials 

	Environmental
	Air/water/ground pollution/waste/spills/destruction
	No PTW/Poor judgement/human error/EMP non-compliant
	Disease/Injury/Pollution 

	Loading/unloading trucks
	Sprain, Fall/trip/caught between
	Poor judgement/human error
	Injury/damage 

	Cigarette Smoking
	Inhale smoke/fire/pollution
	Human behaviour/human error/ignore smoking Policy
	Disease/death

	Explosions
	Fire/explosion/leaks
	Poor judgement/human error/poor storage practice
	Death/Injury/Damage 

	Structural failure
	Falling/struck by/breaking/caught between
	No PTW/Poor judgement/Supervision/human error
	Death/Injury/Damage 

	Radiation exposure
	Exposure to passer-by/employees/operators
	No PTW/Poor judgement/Supervision/human error
	Death/Injury

	Ergonomics
	Manual handling/poor posture/lifting/pulling/computer work
	Poor judgement/Supervision/human error/haste
	Injury

	Crushing
	Falling/struck by/breaking/caught between
	No PTW/Poor judgement/Supervision/human error
	Death/Injury/Damage 

	Gas escape
	Leak/fire/explosion
	Mech. Failure/cracks/collision/corrosion/maintenance/Human error
	Fire/explosion/ Death/Injury/Damage 

	Liquid escape
	Leak/fire/explosion
	Mech. Failure/cracks/collision/corrosion/maintenance/Human error
	Fire/explosion/ Death/Injury/Damage 

	Entanglement
	Caught by/entangled by objects
	No PTW/procedure, Poor judgement/supervision/human error
	Death/Injury/Damage 

	Cutting/stabbing/puncturing
	Construction work/maintenance/repairs
	No PPE/Poor judgement/poor supervision/human error/haste
	Death/Injury/Damage 

	Dangerous animals
	Animals
	Snakes and spider can bite
	Death/Injury

	Shootings
	Fire arms
	Fire arms on persons could be used for robbery or forced entry
	Death/Injury/Damage 

	Verbal abuse
	People
	Delays in access control
	Injury

	Traffic Control on the Construction site
	Vehicle accidents
	Human behaviour/human error/ignore procedure
	Injury/damage 

	Roadway Narrowing/Gravel Traffic Control
	Vehicle accidents
	Human behaviour/human error/ignore procedure
	Injury/damage 


2.2 Environmental constraints and management

Describe or cross refer to environmental constraints applicable to the Contractor’s plan and his activities on the Affected Property and how they should be managed.  Include here or cross refer to an Annexure to the Service Information.  

The Contractor shall comply with the environmental criteria and constraints stated in Scope Of Work 

The Contractor shall comply with all provisions stipulated in the Kriel Power Station ISO 14001 Environmental Management System and ensure sufficient funding is allocated for in the BoQ.

The following Documents are included (but may change from time to time due to review and/or operational requirements):

1. Kriel Environmental Policy (to be prominently displayed in all working areas)

2. Procedure for the Identification and Assessment of all Environmental Aspects and Impacts

3. Environmental Legal and Other Requirements (this will include all applicable Environmental Authorisations and Environmental Management Plans) 

4. MpumaCare EMS Scope and Manual

5. Environmental Training, Awareness and Competence

6. Health, Safety and Environmental Communication Procedure

7. Identification and Application of Environmental Operational Controls

8. Environmental Performance Monitoring and Measurement Procedure

9. Handling of HSE Non-conformities and Corrective and Preventative Measures

10. Health, Safety and Environmental Incident Management Procedure

11. Health, Safety and Environmental Audit Procedure

12. Management Review Procedure

2.3 Quality assurance requirements

1. The Supplier shall demonstrate, provide and maintain a Quality Management System (QMS) that is ISO 9001:2008 certified or compliant thereto. Compliance with the provisions of this clause in no way relieves the Supplier of the final responsibility to furnish acceptable services.

2. The Supplier agrees to control and professionally preserve and store appropriate documents, records and recordings for a period of 5 years after termination of the agreement to guarantee the traceability of the services rendered and inspection thereof.

3. The Supplier agrees to regularly update and implement all the latest technology available as well as the necessary improvements for the installation, production and organisation deemed necessary to meet the requirements of the agreement and in order to enhance capabilities and effectiveness to deliver high quality, cost-effective security services.

4. The delivered or services shall be uniform in Quality and condition, consistent with good industry practices and adhere to requested MpumaCare requirements, without deviation.

5. The Employer shall have the right to regularly conduct inspections, assessments , audits and surveys and perform surveillance of the Supplier’s and/or Sub-Supplier facilities, sites, premises, records and documentation ( including but not limited to data books ) to evaluate their capability to comply with the requirements necessary to conform to contractual and QMS requirements.

6. The Employer reserves the right to inspect, at reasonable times, any or all of the services performed at the Supplier’s or Sub-Supplier’s premises or elsewhere. Verification by MpumaCare shall not absolve the Supplier of the responsibility to provide acceptable product and / or services, nor shall it preclude subsequent rejection by MpumaCare.

7. 
The services must comply with the agreed specifications and requirements and the applicable directives and standards set out in the Contract. Defects notified by the Employer shall be remedied by the Supplier upon demand by the Employer without undue delay and at no extra cost. The Supplier shall continuously monitor and identify non-conformances, both internal and external, as signals of opportunities for improvement making process and other relevant changes to prevent recurrence.

8. The Supplier shall further identify potential problems before they occur by identifying deviations in patterns or trends in product, service or process performance.

9. Nothing contained in the Contract and/or purchase order and/or scope of work and /or works information shall relieve in any way the Supplier from the obligation of Quality control thereof.

10. The Supplier guarantees that the Quality of the delivered services will comply with the requirements of the contract and/or relevant specifications.

11. The Supplier shall, on request, prove its ability to relate to the proposed scope of work which establishes the manner in which the Supplier intends to perform the Contract.

12. The Supplier shall, on request, prove its organisational, logistics and support resources to ensure the requirements of the contract can and will be achieved.

13. The Employer reserves the right to assess and measure, during the existence of the agreement the qualifications, capability and competence of the key staff (assigned personnel) in relation to the scope of work and to interview any / all of them to confirm the Quality evaluation.

14. The identified professional personnel who will be managing the service will be available and accessible on a continuous basis until the conclusion of the project.

15. The Supplier shall demonstrate experience in comparable projects or specific aspects of the project and / or performance in similar projects, on request.

16. The Quality of the services and the contents thereof will always be in accordance with professional standards.

17. For the duration of the Contract, the professional staff managing the service, must be and remain a member of his/her Professional Society 

18. The Supplier must, at all relevant times, scrutinise and be aware of  MpumaCare’s requirements with specific focus on , inter alia, its  philosophy, principles, strategies, practises, mission, vision, models, policies and practises.

19. The Supplier shall exercise reasonable professional skill, care and diligence in the performance of his obligations in terms of this agreement.

20. On awarding of the Contract to the successful Supplier, such Supplier shall present to the Employer an acceptable Quality Control Plan (QCP). The QCP shall comply with the requirements of ISO 10005 and shall include, but not be limited to, the following clauses:

· A description of the type, level and frequency of inspections performed by the Supplier’s Quality Control monitors .These inspection reports shall be made available to MpumaCare, on request

· Quality Control check lists used to conduct inspections which include , as a minimum , checks of equipment , uniform , attendance and/or compliance with sign in/out procedures , knowledge of and adherence to Duty Book requirements ,knowledge of and adherence to screening equipment operating procedures , Resumes for all personnel appointed to serve as Quality Control monitors.
· Scope of a Quality Plan, Quality objectives, Management responsibility, control of documents and data , Control of records , resources , Customer communication, Audits

21. On awarding the contract, the parties will each nominate to the other their Quality representative(s), in writing.

22. The Supplier shall use all methods deemed necessary to ensure that the Supplier’s employees are in a constant state of awareness and readiness. MpumaCare employees regarding the fire fighter/ medics; professionalism , courtesy and knowledge of their assigned duties

Specify minimum requirements for the Contractor’s Quality Plan and Work Procedures or provide the Employer’s Quality Plan if that is to be used. Make sure witness and hold points are identified generally and describe any particular requirements for QA outside the Affected Property.  Indicate how the Contractor’s QA documentation is to be submitted for acceptance and any conditions that need to be imposed relating to acceptance. State whether ISO compliance is a condition and if so which ISO standard shall apply. 

3 Procurement

3.1 People

3.1.1 Minimum requirements of people employed

No foreign nationals are to be employed on this contract. Psychological Profile/Test of personnel and medicals are required prior to coming on to the site and kept valid for the duration of the contract. 

Fully trained male and female employees, Contracts Managers to be registered with SAQCC  all the employees needs to have the applicable certification/qualification.
All the Contractors personnel employed by the Supplier for deployment at the Employer’s premises shall be security cleared (criminal record clearance) and appointed according to the DOL Regulations.  

Signing of legal indemnities with regards to the services to be rendered (e.g. damage to property of third parties, loss of life or injury to be sustained by the security personnel during the execution of their duties and any other legal claims resulting from acts or omissions committed by security personnel against third parties)

3.1.2 BBBEE and preferencing scheme

The Contractor is expected to maintained or improve its’ B-BBEE rating for the duration of the contract. Should the rating be change negatively, the Contractor would be expected to rectify that within 6-months of being made aware of negative change.

The Contractor is expected to submit a valid B-BBEE Verification Certificate from a SANAS accredited Verification Agency each year. Failure to submit such a Certificate may be regarded as the breach of the contract by the Employer.

3.1.3 Accelerated Shared Growth Initiative – South Africa (ASGI-SA) 



N/A

3.2 Subcontracting


   No subcontracting unless approved by Service manager for emergency situations.

3.2.1 Preferred sub-Contractors
N/A

3.2.2 Subcontract documentation, and assessment of subcontract tenders

The NEC system is compulsory with subcontracting.

3.2.3 Limitations on subcontracting

The Employer needs to give written approval before any work is subcontracted out.  

3.2.4 Attendance on sub-Contractors
N/A

3.3 Plant and Materials

3.3.1 Specifications

Ensure that all vehicles to be used on the site comply with road safety specifications.

The vehicles need to be in good working order and not older than 24 months with less than 50 000km. These vehicles would need to be approved before been used on site by the Employer.

All vehicles to have the companies logo on both doors 

All vehicles need seat belts for all passenger’s and driver.

SPECIFICATION

	Title
	Ref number
	Rev
	if publicly available
	

	Occupational Health and Safety Act and Regulations Act 85 of 1993
	As per DOL website
	
	Yes
	


3.3.2 Correction of defects

If there is any plant or equipment that is defective or faulty this needs to be reported immediately and the items need to be repaired or replaced.

The Contractor is responsible for all loss of or damage to Eskom property in their possession.

3.3.3 Contractor’s procurement of Plant and Materials

All other items to be procured where possible from local suppliers subject to pricing.

All purchases need to be discussed with the Service Manager and approved prior to placing orders.

3.3.4 Tests and inspections before delivery

N/A

3.3.5 Plant & Materials provided “free issue” by the Employer
Testing equipment that will be supplied by the Employer:

4 Working on the Affected Property

Constraints 

There are possible strikes due to labour unrest.

The site is huge with a perimeter of more than ten kilometres. 

Reaction times need to be kept to a minimum.

Severe heat conditions during the summer months.

Rainy season (October to March) can result in flooding making access to remote areas difficult

Snakes have been found that can cause injury to people

There will be no power at the outlying areas.

Services and rules applicable 

There are various site rules that are applicable.

Site instruction are issued on a regular basis as the site changes

4.1 Employer’s site entry and security control, permits, and site regulations

The Contractor needs to adhere to all site rules.

Each employee needs to have a medical done prior to entering the site and obtaining an access permit.

Induction training needs to be carried out and all risks identified and discussed with the employees. Proof of this need to be attached to the request for access permit.

The Employer has a zero tolerance on substance abuses.

Vehicles need to be roadworthy at all times otherwise access to site is denied

Strict road rules are in place and need to be adhered to at all times under normal operation.

All staff needs to wear the appropriate PPE at all times on the site.

4.2 People restrictions, hours of work, conduct and records

No employee is to work over the allowed working hours as per the law of the land. Any contraventions will be reported to the department of labour.

All records of hours work need to be kept for audit purposes.

The Service Manager shall have access to records at any time. These records may be needed when assessing compensation events.

All personal files need to be up to date and a copy on Site showing proof of registration to HPCSA, disciplinary actions taken, attendance registers and leave taken etc.

Psychological Profile/Test of personnel and medicals are required prior to coming on to the site and kept valid for the duration of the contract. 

All access cards need to be returned once the contract is complete or if any individual leave the employment of the Contractor. A levy of One Hundred Rand per card will be deducted from the invoice if the employee does not return the card. Retain proof of returning cards, signed by both parties.

Ensure that all staff has signed a code of practice showing the penalties for breaches. This needs to be placed on personal file. Code of conduct to be displayed on notice boards at each guard house.

There needs to be a parade prior to the shift starting to give a general brief of events from the last shift and to sign on staff.

All staff has to have an access card and need to scan in for duty and off duty. Under no circumstance are EMS staff allowed to use their own cards to scan in other personal.

4.3 Health and safety facilities on the Affected Property

There are Safety and Environmental advisors on the site that can assist on safety issues.

4.4 Environmental controls, fauna & flora



Would be covered in the Environmental Management System procedures and associated documents Scope of Work Pg 13 5.4.
4.5 Cooperating with and obtaining acceptance of others
Requirements for liaison with and acceptance from statutory authorities or inspection agencies.

Note: that the Contractor needs to have contact with the local emergency services in case there are problems on the site.

4.6 Records of Contractor’s Equipment

All equipment that is brought onto the site needs to be vetted by the Service Manager before using.

This needs to be in writing and signed for. A monthly audit will be conducted on this equipment.

4.7 Equipment provided by the Employer
The Employer will conduct a monthly inspection on all equipment provided to the Contractor for the service. Inspection sheet need to be signed off by both parties. Any defects need to be reported immediately to the Service Manager.

4.8 Site services and facilities

4.8.1 Provided by the Employer
This is a mandatory cross reference form clause 25.2 in TSC3.  The Employer will provide in the way of power, water, waste disposal, ablutions, fire extinguishers and lighting at the main buildings on the affected property. There will be no power at the outlying areas
4.8.2 Provided by the Contractor
The Contractor will be required to purchase the equipment as per the price list. All items at completion of the contract belong to the Employer.

The Contractor to provide: 

· Computers and Printers for management staff and maintain these items.

· Cell phones for key personal work stations
· Stationary

· Kitchen equipment for tea and coffee

· Rations for the shift (tea coffee sugar food milk etc)

· Accommodation 
· Staff transport from home to site and back after shift

· Display board for the recognition at office 
· Uniforms for personal including admin staff minimum of three sets.

· Magnetic signage for vehicles 

· Personal protective equipment (hard hats, safety glasses clear vision, dust masks, earplugs, sun hats, safety boots, reflective jackets/vests  “all weather jackets for rainy season)


4.9 Control of noise, dust, water and waste 

Please ensure that all waste is disposed of in the supplied bins if there are not sufficient please advise, so that additional bins can be made available

When patrols are in noisy areas, ear protection needs to be worn.

Water will be supplied but Contractor to distribute.

Dust could be a problem supply all staff with safety glasses (clear view) and dust masks when required. 

If roads are an issue please advise the Service Manager for dust suppression of the roads.

4.10 Hook ups to existing works

If the Contractor requires using an existing tower for communications, it need to be arranged with the Service Manager.
4.11 Tests and inspections

4.11.1 Description of tests and inspections


The Contractor needs to carry out the following testing


Calibration certification to be done yearly on equipment  

4.11.2 Materials facilities and samples for tests and inspections 

N/A

5 List of drawings

5.1 Drawings issued by the Employer
This is the list of drawings issued by the Employer at or before the Contract Date and which apply to this contract.

	Drawing  number
	Revision
	Title

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


� This total is required by the Employer for budgeting purposes only.  Actual amounts due will be assessed in terms of the conditions of contract.










DOCUMENT C2.1
PAGE iii
PRICING DATA




Part C2: Pricing Data
PAGE 20
C2 TSC3 Cover

