{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Bills Of Quantities","Final summary","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Bills Of Quantities","index":0,"n_rows":1199,"n_cols":25,"rows_kept":1199,"flags":["formulas_cached_only"]}
["Item","Description","Uom","Quantity","Rate","Amount",null,"x","Formatted Qty","x","Abstract RecID","x","Lcode","x","x","x","x","x","x","x","x","x","x","x","x"]
[]
[null,"SECTION NO. 1 : PRELIMINARY & GENERAL"]
[]
[]
[null,"BILL NO.1 : PRELIMINARIES"]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES",{"$nulls":8},2857,null,1010]
[]
[null,"Disclaimer",{"$nulls":8},2858,null,1020]
[]
[{"$nulls":10},2858,null,1020]
[]
[null,"While the ASAQS aims to ensure that its publications represent best practice, the ASAQS does not accept or assume any liability or responsibility for any events or consequences which derive from the use of the Preliminaries Bill. Such Bill is not exhaustive and is therefore only intended to provide general guidance to those who wish to make use of it. This publication is provided 'as is' without warranty of any kind, either expressed or implied including but without limitation to warranties of merchantability, fitness for a particular purpose and non-infringement",{"$nulls":8},2858,null,1020]
[]
[null,"User note",{"$nulls":8},2859,null,1050]
[]
[null,"Delete the above 'Disclaimer' when preparing this Bill No. 1 for tender or contract purposes",{"$nulls":8},2859,null,1050]
[]
[null,"Hereinafter edit all text, etc but even more specifically text within '?...?' to ensure that such text applies to the specific building agreement",{"$nulls":8},2859,null,1050]
[]
[null,"The JBCC Principal Building Agreement (Edition 6.2 - May 2018) prepared by the Joint Building Contracts Committee shall be the applicable building agreement, amended as hereinafter described",{"$nulls":8},2860,null,1030]
[]
[null,"The JBCC Principal Building Agreement contract data form an integral part of this agreement",{"$nulls":8},2861,null,1040]
[]
[null,"The JBCC General Preliminaries (May 2018) published by the Joint Building Contracts Committee  for use with the JBCC Principal Building Agreement (Edition 6.2 - May 2018) shall be deemed to be incorporated in these bills of quantities, amended as hereinafter described",{"$nulls":8},2862,null,1060]
[]
[null,"The contractor is deemed to have referred to the abovementioned documents for the full intent and meaning of each clause",{"$nulls":8},2863,null,1070]
[]
[null,"The clauses in the abovementioned documents are hereinafter referred to by clause number and heading only",{"$nulls":8},2864,null,1080]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Where any item is not relevant to this agreement such item is marked N/A signifying 'not applicable'",{"$nulls":8},2865,null,1090]
[]
[null,"Where standard clauses or alternatives are not entirely applicable to this agreement such amendments, modifications, corrections or supplements as will apply are given under each relevant clause heading and such amendments, modifications, corrections or supplements shall take precedence notwithstanding anything to the contrary contained in the abovementioned documents ",{"$nulls":8},2866,null,1100]
[]
[null,"PREAMBLES FOR TRADES",{"$nulls":8},2867,null,1110]
[]
[null,"User note",{"$nulls":8},2868,null,1130]
[]
[null,"The General Preambles for Trades 2017 published by the Association of South African Quantity Surveyors is designed to support and extend the abbreviated descriptions utilised in these bills of quantities by inter alia referring to SANS construction standards.  Where such preambles are not applicable (eg where BS or Euro construction standards are applicable or the design consultants provide other preambles/specifications for insertion), users are to ensure that the abbreviated descriptions when read in conjunction with the Standard System of Measuring Building Work (seventh edition) for works within South Africa or the Standard Method of Measuring Building Work for Africa 2015 (first edition) for works elsewhere in Africa, represent the full description by extending the abbreviated bills of quantities descriptions and/or by inserting appropriate preambles or specifications",{"$nulls":8},2868,null,1130]
[]
[null,"Note that the text of the Standard System of Measuring Building Work (seventh edition) and that of the Standard Method of Measuring Building Work for Africa 2015 (first edition) is the same",{"$nulls":8},2869,null,1140]
[]
[null,"The latest version of the General Preambles for Trades should be referred to should the General Preambles for Trades 2017 be revised in future",{"$nulls":8},2870,null,1150]
[]
[null,"The General Preambles for Trades 2017 published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of items fully described in the said General Preambles will be entertained",{"$nulls":8},2871,null,1160]
[]
[null,"Supplementary preambles and/or specifications are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles and/or specifications shall take precedence over the provisions of the General Preambles",{"$nulls":8},2872,null,1170]
[]
["Item","Description","Uom","Quantity","Rate","Amount",{"$nulls":4},2873,null,1180]
[null,"The contractor's prices for all items throughout these bills of quantities shall take account of and include where applicable for all of the obligations, requirements and specifications given in the  General Preambles and in any supplementary preambles and/or specifications}"]
[{"$nulls":10},2874,null,1190]
[null,"STRUCTURE OF THIS PRELIMINARIES BILL"]
[{"$nulls":10},2875,null,1200]
[null,"A recital of the headings of the individual clauses in the aforementioned JBCC Principal Building Agreement"]
[null,"A recital of the headings of the individual clauses in the aforementioned JBCC General Preliminaries",{"$nulls":8},2876,null,1210]
[]
[null,"Section C : Any special clauses to meet the particular circumstances of the project",{"$nulls":8},2877,null,1220]
[]
[null,"PRICING OF PRELIMINARIES",{"$nulls":8},2878,null,1230]
[]
[null,"Should the contractor select Option A in the contract data for the adjustment of  preliminaries, the amounts entered against the relevant items in these preliminaries are to be divided into one or more of the three categories provided namely fixed (F), value related (V) and time related (T)}",{"$nulls":8},2879,null,1240]
[]
[null,"SECTION A: PRINCIPAL BUILDING AGREEMENT",{"$nulls":8},2880,null,1250]
[]
[null,"Interpretation (A1-A7)",{"$nulls":8},2881,null,1260]
[]
["1","Clause 1.0 - Definitions and interpretation",{"$nulls":8},2882,null,1270]
[]
[null,"Pricing of bills of quantities",{"$nulls":8},2882,null,1270]
[]
[null,"The contractor is to allow opposite each item for all costs in connection therewith.  All prices to include, unless otherwise stated, for all materials, fabrication, conveyance and delivery, unloading, storing, unpacking, hoisting, labour, setting, fitting and fixing in position, cutting and waste (except where to be measured in accordance with the standard system of measurement), patterns, models and templates, plant, temporary works, returning of packaging, duties, taxes (other than Value Added Tax), imposts, establishment charges, overheads, profit and all other obligations arising out of this  agreement.   Value Added Tax (VAT) is to be separately stated on the summary page of these bills of quantities",{"$nulls":8},2882,null,1270]
[]
[null,"Items left unpriced will be deemed to be covered in prices against other items throughout these bills of quantities and no claim for any extras arising out of the contractor's omission to price any item will be entertained",{"$nulls":8},2882,null,1270]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Prices for all construction equipment, temporary works, services and other items shall include for the supply, maintenance, operating cost and subsequent removal and making good as necessary",{"$nulls":8},2882,null,1270]
[]
[null,"Abbreviated descriptions",{"$nulls":8},2882,null,1270]
[]
[null,"The items in these bills of quantities utilise abbreviated descriptions.  It is the intention that the abbreviated descriptions be fully described when read with the applicable measuring system and the relevant preambles and/or specifications. However, should the full intent and meaning of any description not be clear, the contractor shall, before submission of his tender, call for a written directive from the principal agent, failing which it shall be assumed that the contractor has allowed in his pricing for materials and workmanship in terms of international best practice",{"$nulls":8},2882,null,1270]
[]
[null,"Legal status of contractor",{"$nulls":8},2882,null,1270]
[]
[null,"If the contractor constitutes a joint venture, consortium or other unincorporated grouping of two or more persons then:",{"$nulls":8},2882,null,1270]
[]
[null,"1.   These persons are deemed to be jointly and severally liable to the employer for the performance of this agreement",{"$nulls":8},2882,null,1270]
[]
[null,"2.   These persons shall notify the employer of their leader who has assigned authority to bind the contractor and each of these persons",{"$nulls":8},2882,null,1270]
[]
[null,"3.  The contractor shall not alter its composition or legal status without the prior written consent of the employer","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2882,null,1270]
[]
["2","Clause 2.0 - Law, regulations and notices",{"$nulls":8},2883,null,1280]
[]
[null,"User note",{"$nulls":8},2883,null,1280]
[]
[null,"Insert the following for residential developments only",{"$nulls":8},2883,null,1280]
[]
[null,"The cost to the employer of the NHBRC levies mentioned below is to be conveyed to the employer in order to present an overall building cost",{"$nulls":8},2883,null,1280]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"NHBRC levies",{"$nulls":8},2883,null,1280]
[]
[null,"The employer shall allow for and pay any levies required by the National Home Builders Registration Council (NHBRC). The contractor warrants that he is registered and will maintain registration with the NHBRC for the duration of this agreement [2.1] ?","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2883,null,1280]
[]
["3","Clause 3.0 - Offer and acceptance","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2884,null,1290]
[]
["4","Clause 4.0 - Cession and assignment","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2885,null,1300]
[]
["5","Clause 5.0 - Documents",{"$nulls":8},2886,null,1310]
[]
[null,"Value Added Tax",{"$nulls":8},2886,null,1310]
[]
[null,"Provision is made in the summary page of these bills of quantities for the inclusion of Value Added Tax (VAT)",{"$nulls":8},2886,null,1310]
[]
[null,"? Priced document as specification",{"$nulls":8},2886,null,1310]
[]
[null,"Clause 5.4 is deemed to be deleted",{"$nulls":8},2886,null,1310]
[]
[null,"The principal agent shall decide which portion of the priced document may be used as a specification of materials and goods or methods, if any",{"$nulls":8},2886,null,1310]
[]
[null,"User Note",{"$nulls":8},2886,null,1310]
[]
[null,"Insert the following where applicable",{"$nulls":8},2886,null,1310]
[]
[null,"Electronic issue of drawings",{"$nulls":8},2886,null,1310]
[]
[null,"All drawings for this project will be issued electronically and the contractor shall be deemed to have received such drawings on the date that such drawings have been dispatched electronically [5.}","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2886,null,1310]
[]
["6","Clause 6.0 - Employer's agents",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
[]
[null,"Delegated authority may be dealt with in B 5.0 of the contract data.",{"$nulls":8},2887,null,1320]
[]
[null,"Insert in the contract data 'Refer to Bill No. 1 (Preliminaries)' should it be dealt with in Bill No. 1",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Delegated authority",{"$nulls":8},2887,null,1320]
[]
[null,"The authority of the principal agent to issue contract instructions [17.1] and perform duties for specific aspects of the works is delegated to agents  as follows [6.2]   This does not preclude the principal agent from issuing such contract instructions.",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
[]
[null,"Add delegated authority as may be required for other relevant consultants not listed hereinafter",{"$nulls":8},2887,null,1320]
[]
[null,"1. Architect",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"Note that the contract instructions hereinafter are selected from those listed in clause 17.1 of the JBCC PBA",{"$nulls":8},2887,null,1320]
[]
[null,"1.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The architect is responsible for the architectural design, functional design and quality inspection of the work",{"$nulls":8},2887,null,1320]
[]
[null,"Contract instructions [6.2; 17.1]",{"$nulls":8},2887,null,1320]
[]
[null,"Rectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",{"$nulls":8},2887,null,1320]
[]
[null,"Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.3 The site",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.4 1033 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.5  Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"1.2.6 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.7 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.8 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.9 Protection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.10 Making good physical loss and repairing damage to the works [23.2.2]",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.11 Rectification of defects [21.2]",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.12 A list for practical completion specifying outstanding or defective work to be rectified to achieve completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.13 Expenditure of budgetary allowances, prime cost amounts and provisional sums",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.14 Appointment of a subcontractor [14.0; 15.0]",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.15 Work by direct contractors [16.0]",{"$nulls":8},2887,null,1320]
[]
[null,"1.2.16   On suspension or termination, protection of the works, removal of construction equipment and surplus materials and goods  [29.0]",{"$nulls":8},2887,null,1320]
[]
[null,"2. Quantity surveyor",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"2.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The quantity surveyor is responsible for all measurements, valuations, financial assessments and all other quantity surveying and cost control functions of the works",{"$nulls":8},2887,null,1320]
[]
[null,"2.2 Contract instructions [6.1]",{"$nulls":8},2887,null,1320]
[]
[null,"2.2.1 No contract instructions delegated to the quantity surveyor",{"$nulls":8},2887,null,1320]
[]
[null,"3. Civil and structural engineer",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"Note that the contract instructions hereinafter are selected from those listed in clause 17.1 of the JBCC PBA",{"$nulls":8},2887,null,1320]
[]
[null,"3.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The civil and structural engineer is responsible for all aspects of civil and structural engineering design and quality inspection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"Contract instructions [6.2; 17.1]",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.1 Rectification of discrepancies, errors in description quantity or omission of items in the  agreement other than in the JBCC Principal Building Agreement",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.2 Alteration to design, standards or quantity of the  works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.3 The site [13.0]",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.4 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.5 Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.6 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.7 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.8 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.9 Protection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.10 Making good physical loss and repairing damage to the works [23.2.2]",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.11 Rectification of defects [21.2]",{"$nulls":8},2887,null,1320]
[]
[null,"3.2.12 A list for practical completion} specifying outstanding or defective work to be rectified to achieve practical completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"3.2.13 Expenditure of budgetary allowances, prime cost amounts and provisional sums",{"$nulls":8},2887,null,1320]
[]
[null,"4. Mechanical engineer",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"Note that the contract instructions hereinafter are selected from those listed in clause 17.1 of the JBCC PBA",{"$nulls":8},2887,null,1320]
[]
[null,"4.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The mechanical engineer is responsible for all aspects of mechanical engineering design and quality inspection of the works and, where appointed by the  employer for quantity surveying services in respect of the mechanical installations, for all measurements, valuations, financial assessments and all other quantity surveying and cost control functions",{"$nulls":8},2887,null,1320]
[]
[null,"4.2 Contract instructions [6.2; 17.1]",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.1 Rectification of discrepancies, errors in description or quantity or omission of items in the  agreement other than in the Principal Building Agreement",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.2 Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.3 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.4 Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.5 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.6 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.7 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.8 Protection of the works",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"4.2.9 Making good physical loss and repairing damage to the works [23.2.2]",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.10 Rectification of defects [21.2]",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.11 A list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a  list for completion and a  list for final completion specifying outstanding or defective work to be rectified to achieve final completion",{"$nulls":8},2887,null,1320]
[]
[null,"4.2.12 Expenditure of budgetary allowances, prime cost amounts and provisional sums",{"$nulls":8},2887,null,1320]
[]
[null,"5. Electrical engineer",{"$nulls":8},2887,null,1320]
[]
[null,"User Note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"Note that the contract instructions hereinafter are selected from those listed in clause 17.1 of the JBCC PBA",{"$nulls":8},2887,null,1320]
[]
[null,"5.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The electrical engineer is responsible for all aspects of electrical engineering design and quality inspection of the works and, where appointed by the  employer for quantity surveying services in respect of the electrical installations, for all measurements, valuations, financial assessments and all other quantity surveying and cost control functions",{"$nulls":8},2887,null,1320]
[]
[null,"Contract instructions [6.2; 17.1]",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.1 Rectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the  JBCC Principal Building Agreement",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.2 Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.3 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.4 Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"5.2.5 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.6 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.7 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.8 Protection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.9 Making good physical loss and repairing damage to the works [23.2.2]",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.10 Rectification of defects [21.2]",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.11 A list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a  list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",{"$nulls":8},2887,null,1320]
[]
[null,"5.2.12 Expenditure of budgetary allowances, prime cost amounts and provisional sums",{"$nulls":8},2887,null,1320]
[]
[null,"6.  Wet services engineer",{"$nulls":8},2887,null,1320]
[]
[null,"User note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant  in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"Note that the contract instructions hereinafter are selected from those listed in clause 17.1 of the JBCC PBA",{"$nulls":8},2887,null,1320]
[]
[null,"6.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The wet services engineer is responsible for all  aspects of wet services engineering design and quality inspection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"6.2  Contract instructions   [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.1 Rectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.2 Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"6.2.3 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.4 Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.5 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.6 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.7 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.8 Protection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.9 Making good physical loss and repairing damage to the works [23.2.2]",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.10 Rectification of defects [21.2]",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.11 A list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a  list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",{"$nulls":8},2887,null,1320]
[]
[null,"6.2.12 Expenditure of budgetary allowances, prime cost amounts and  provisional sums",{"$nulls":8},2887,null,1320]
[]
[null,"7. Fire consultant",{"$nulls":8},2887,null,1320]
[]
[null,"User note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement. Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
[]
[null,"Note that the contract instructions hereinafter are selected from those listed in clause 17.1 of the JBCC PBA",{"$nulls":8},2887,null,1320]
[]
[null,"7.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The fire consultant is responsible for all aspects of rational fire design and quality inspection of the works",{"$nulls":8},2887,null,1320]
[]
[null,"7.2  Contract instructions [6.2; 17.1]",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.1 Rectification of discrepancies, errors in description quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"7.2.2 Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.3 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.4 Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.5 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.6 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.7 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.2 Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.3 Compliance with the law, regulations and bylaws [2.1]",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.4 Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.5 Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.6 Removal or re-execution of work",{"$nulls":8},2887,null,1320]
[]
[null,"7.2.7 Removal or substitution of any materials and goods",{"$nulls":8},2887,null,1320]
[]
[null,"8. Health and safety consultant",{"$nulls":8},2887,null,1320]
[]
[null,"User note",{"$nulls":8},2887,null,1320]
[]
[null,"Insert the following but remove where the consultant is not relevant to this agreement.  Edit both the duties and the contract instructions of the consultant in keeping with the wishes of the principal agent",{"$nulls":8},2887,null,1320]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"8.1 Duties [6.2]",{"$nulls":8},2887,null,1320]
[]
[null,"The health and safety consultant is responsible for all aspects of health and safety of the works. Without derogating from the generality thereof, the health and safety consultant will perform the following specific functions and duties in respect of the health and safety aspects of the works. He shall",{"$nulls":8},2887,null,1320]
[]
[null,"8.1.1 Act as the employer's agent  in terms of  the Construction Regulations issued in terms of the Occupational Health and Safety Act,1993 (as amended",{"$nulls":8},2887,null,1320]
[]
[null,"8.1.2 Prepare and update the health and safety specification for the  works",{"$nulls":8},2887,null,1320]
[]
[null,"8.1.3 Agree with the contractor the health and safety plan for the  works",{"$nulls":8},2887,null,1320]
[]
[null,"8.1..4 Carry out regular audits to ensure adherence to the safety plan and compliance with the Act and Regulations",{"$nulls":8},2887,null,1320]
[]
[null,"8.1.5 Stop the execution of the works where the agreed specification or plan is not adhered to","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2887,null,1320]
[]
["7","Clause 7.0 - Design responsibility","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2888,null,1330]
[]
[null,"Insurances and securities (A8-A11)",{"$nulls":8},2889,null,1340]
[]
["8","Clause 8.0 - Works risk","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2890,null,1350]
[]
["9","Clause 9.0 - Indemnities","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2891,null,1360]
[]
["10","Clause 10.0 - Insurances","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2892,null,1370]
[]
["11","Clause 11.0 - Securities",{"$nulls":8},2893,null,1380]
[]
[null,"User note",{"$nulls":8},2893,null,1380]
[]
[null,"If it is deemed advisable, the extent of any guarantee for payment may be stated and whether it is required of the contractor to waive his lien.  Edit the following clause",{"$nulls":8},2893,null,1380]
[]
[null,"? Guarantee for payment",{"$nulls":8},2893,null,1380]
[]
[null,"The employer shall provide to the contractor a guarantee for payment in the amount of ?.......................................................Rand (R...........................) ? [11.5.1].  The contractor shall consequently waive his lien or right of continuing possession of the works [11.1}",{"$nulls":8},2893,null,1380]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"User note",{"$nulls":8},2893,null,1380]
[]
[null,"Where it is expected of the contractor to waive his lien in terms of  clause 11.10, the waiver of lien may be extended to subcontracts as follows:",{"$nulls":8},2893,null,1380]
[]
[null,"Extension of waiver of lien",{"$nulls":8},2893,null,1380]
[]
[null,"The contractor shall ensure that a waiver of lien is included in all subcontracts and that the works executed on the site are kept free of all liens and other encumbrances at all times [11.10]","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2893,null,1380]
[]
[null,"Execution (A12 - A17) }",{"$nulls":8},2894,null,1390]
[]
["12","Clause 12.0 - Obligations of the parties",{"$nulls":8},2895,null,1400]
[]
[null,"Office accommodation",{"$nulls":8},2895,null,1400]
[]
[null,"The contractor shall provide, maintain and remove on practical completion air conditioned office accommodation with suitable tables and chairs for meetings to be held on the site. Such offices shall be kept clean and fit for use at all times [12.2.18]",{"$nulls":8},2895,null,1400]
[]
[null,"Notice board",{"$nulls":8},2895,null,1400]
[]
[null,"The contractor shall erect in a position approved by the principal agent, maintain and remove on practical completion a notice board recommended by the South African Institute of Architects and as approved by the principal agent listing the names and logos of the employer, the contractor and the professional consultants. No subcontractor or supplier notice boards may be erected unless permission is granted by the principal agent for such notice boards to be erected [12.2.18]",{"$nulls":8},2895,null,1400]
[]
[null,"Statutory and other notices",{"$nulls":8},2895,null,1400]
[]
[null,"The contractor shall submit and/or comply with all statutory and other notices that may be required by any local or other authority in order not to cause any delay to the commencement of the works by the contractor. The contractor shall pay all deposits or fees in this regard.",{"$nulls":8},2895,null,1400]
[]
[null,"It is, however, specifically recorded that the employer shall be responsible for the timeous approval of building plans by any local or other authorities and the payment of any fees or charges related thereto","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2895,null,1400]
[]
["13","Clause 13.0 - Setting out","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2896,null,1410]
["Item","Description","Uom","Quantity","Rate","Amount"]
["14","Clause 14.0 - Nominated subcontractors","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2897,null,1420]
[]
["15","Clause 15.0 - Selected subcontractors","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2898,null,1430]
[]
["16","Clause 16.0 - Direct contractors",{"$nulls":8},2899,null,1440]
[]
[null,"Attendance on direct contractors",{"$nulls":8},2899,null,1440]
[]
[null,"In respect of direct contractors the contractor shall:",{"$nulls":8},2899,null,1440]
[]
[null,"1. Designate an area for the direct contractor to establish a temporary office and workshop and storage of equipment and materials",{"$nulls":8},2899,null,1440]
[]
[null,"2. Allow the user of personnel welfare facilities, where provided",{"$nulls":8},2899,null,1440]
[]
[null,"3. Provide water, lighting and single phase electric power to a position within 50m of the place where the direct contract work is to be carried out, other than fuel or power for commissioning of any installation",{"$nulls":8},2899,null,1440]
[]
[null,"4. Permit the direct contractor to use erected scaffolding, hoisting facilities, etc provided by the contractor, in common with others having the like right, while it remains erected on the site  [16.1]","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2899,null,1440]
[]
["17","Clause 17.0 -  Contract instructions",{"$nulls":8},2900,null,1450]
[]
[null,"Site instructions Instructions issued on site are to be recorded in a site instruction book which is to be supplied and maintained on site by the contractor","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2900,null,1450]
[]
[null,"Completion (A18 - A24) }",{"$nulls":8},2901,null,1460]
[]
["18","Clause 18.0 - Interim completion","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2902,null,1470]
[]
["19","Clause 19.0 - Practical completion","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2903,null,1480]
[]
["20","Clause 20.0 - Completion in sections","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2904,null,1490]
[]
["21","Clause 21.0 - Defects liability period and final completion","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2905,null,1500]
[]
["22","Clause 22.0 - Latent defects liability period","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2906,null,1510]
[]
["23","Clause 23.0 - Revision of the date for practical completion",{"$nulls":8},2907,null,1520]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Substitution of materials and goods",{"$nulls":8},2907,null,1520]
[]
[null,"The removal or substitution of any materials and goods which do not conform to the specification or the contract drawings shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value [17.1.8; 23.1 & 2]","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2907,null,1520]
[]
["24","Clause 24.0 - Penalty for late or non-completion","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2908,null,1530]
[]
[null,"Payment (A25 - A27) }",{"$nulls":8},2909,null,1540]
[]
["25","Clause 25.0 - Payment",{"$nulls":8},2910,null,1550]
[]
[null,"Prices submitted",{"$nulls":8},2910,null,1550]
[]
[null,"Where prices are submitted by the contractor or subcontractor during the progress of the works in respect of contract instructions or in regard to a claim under the terms of this agreement and notwithstanding the fact that such prices may be used in an interim payment certificate, there is to be no presumption of acceptance. Should the principal agent wish to accept any such prices prior to the issue of the certificate of final completion, it shall be in writing",{"$nulls":8},2910,null,1550]
[]
[null,"Fluctuations in costs",{"$nulls":8},2910,null,1550]
[]
[null,"All fluctuations in costs, with the exception of fluctuations in the rate of Value Added Tax, shall be for the account of the contractor","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2910,null,1550]
[]
["26","Clause 26.0 - Adjustment of the contract value and final account",{"$nulls":8},2911,null,1560]
[]
[null,"?Fluctuations in costs",{"$nulls":8},2911,null,1560]
[]
[null,"All fluctuations in costs, with the exception of fluctuations in the rate of Value",{"$nulls":8},2911,null,1560]
[]
[null,"Added Tax, shall be for the account of the contractor [26.9.5] ?",{"$nulls":8},2911,null,1560]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"User note",{"$nulls":8},2911,null,1560]
[]
[null,"Insert the following or similar clause where tenant installation /user requirements may be delayed or omitted",{"$nulls":8},2911,null,1560]
[]
[null,"Tenant installation/user requirements delayed",{"$nulls":8},2911,null,1560]
[]
[null,"There is a possibility that certain works related to tenant installation/user requirements may have to be delayed and may consequently not be executed prior to practical completion",{"$nulls":8},2911,null,1560]
[]
[null,"The employer reserves the right to omit such work without compensation to the contractor for loss of profit or any other loss which the contractor may suffer as a result of such omission",{"$nulls":8},2911,null,1560]
[]
[null,"Should the contractor be instructed to do so he shall execute this work under the conditions pertaining to this agreement on the basis that a separate amount for preliminaries appurtenant to this work (if applicable) is agreed to between the contractor and the principal agent and on condition that instruction to proceed with such work is given to him within a period of three (3) calendar months after the date of practical completion of the works",{"$nulls":8},2911,null,1560]
[]
[null,"Cost of claims",{"$nulls":8},2911,null,1560]
[]
[null,"All costs incurred by the contractor in the preparation of claims shall be borne by the contractor. This provision shall not preclude an adjudicator or an arbitrator appointed in terms of this agreement [30.6 & 7] from making a determination on costs",{"$nulls":8},2911,null,1560]
[]
[null,"Claims from subcontractors",{"$nulls":8},2911,null,1560]
[]
[null,"The contractor shall review, assess and adjudicate any claims received by him from any subcontractor and thereafter submit same to the principal agent with a recommendation in order to assist the principal agent in adjudicating the claim [26.6]","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2911,null,1560]
[]
["27","Clause 27.0 - Recovery of expense and/or loss","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2912,null,1570]
[]
[null,"Suspension and termination (A28 - A29)",{"$nulls":8},2913,null,1580]
[]
["28","Clause 28.0 - Suspension by the  contractor","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2914,null,1590]
[]
["29","Clause 29.0 - Termination","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2915,null,1600]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Dispute resolution (A30)",{"$nulls":8},2916,null,1610]
[]
["30","Clause 30.0 - Dispute resolution",{"$nulls":8},2917,null,1620]
[]
[null,"Agreement",{"$nulls":8},2917,null,1620]
[]
[null,"The required information of the parties and the amount of the contract sum shall be inserted in the agreement for signature of the agreement by the parties",{"$nulls":8},2917,null,1620]
[]
[null,"Contract",{"$nulls":8},2917,null,1620]
[]
[null,"User note",{"$nulls":8},2917,null,1620]
[]
[null,"Insert under the above heading, with suitable sub-headings any amendments, modifications, corrections or supplements to the contract data",{"$nulls":8},2917,null,1620]
[]
[null,"Tenderer's selection",{"$nulls":8},2917,null,1620]
[]
[null,"Before submission of his tender the contractor is to complete the tenderer's selections in the contract data",{"$nulls":8},2917,null,1620]
[]
[null,"User note",{"$nulls":8},2917,null,1620]
[]
[null,"All information for the above requires consultation with the contractor. The principal agent should not pre-select any of the alternatives available to the contractor","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2917,null,1620]
[]
[null,"SECTION B:  GENERAL PRELIMINARIES",{"$nulls":8},2918,null,1630]
[]
[null,"User note",{"$nulls":8},2919,null,1640]
[]
[null,"Amendments, modifications, corrections or supplements to the General Preliminaries in Section B should be recorded in the contract data",{"$nulls":8},2919,null,1640]
[]
[null,"Should it be necessary to expand on any of the General Preliminaries clauses, the user should list the appropriate General Preliminary clause number and heading and insert the relevant provision under a suitable heading in bold as may be ne",{"$nulls":8},2919,null,1640]
[]
[null,"Definitions and interpretation (B1)",{"$nulls":8},2920,null,1650]
[]
["31","Clause 1.1 - Definitions","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2921,null,1660]
[]
["32","Clause 1.2 - Interpretation","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2922,null,1670]
[]
[null,"Documents (B2)",{"$nulls":8},2923,null,1680]
[]
["33","Clause 2.1 - Checking of documents","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2924,null,1690]
[]
["34","Clause 2.2 - Provisional bills of quantities",{"$nulls":8},2925,null,1700]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"User note",{"$nulls":8},2925,null,1700]
[]
[null,"Check 'wet trades' included in the bills of quantities and edit the following clause as may be necessary",{"$nulls":8},2925,null,1700]
[]
[null,"? Multiple procurement",{"$nulls":8},2925,null,1700]
[]
[null,"These bills of quantities are in multiple procurement format ie the 'wet trades' - earthworks, concrete, formwork and reinforcement, precast concrete, masonry, waterproofing and sub-surface drainage - are provisionally (fully?) measured and the subsequent trades are budgetary allowances and/or provisional sums","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2925,null,1700]
[]
["35","Clause 2.3 - Availability of construction information","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2926,null,1710]
[]
["36","Clause 2.4 - Ordering of materials and goods","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2927,null,1720]
[]
[null,"Previous work and adjoining properties (B3)",{"$nulls":8},2928,null,1730]
[]
["37","Clause 3.1 - Previous work - dimensional accuracy","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2929,null,1740]
[]
["38","Clause 3.2 - Previous work - defects","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2930,null,1750]
[]
["39","Clause 3.3 - Inspection of adjoining properties","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2931,null,1760]
[]
[null,"The site (B4)",{"$nulls":8},2932,null,1770]
[]
["40","Clause 4.1 - Handover of site in stages","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2933,null,1780]
[]
["41","Clause 4.2 - Enclosure of the works",{"$nulls":8},2934,null,1790]
[]
[null,"User note",{"$nulls":8},2934,null,1790]
[]
[null,"Describe any specific hoarding requirements, other than already described in clause 4.2 or in the contract data","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2934,null,1790]
[]
["42","Clause 4.3 - Geotechnical and other investigations","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2935,null,1800]
[]
["43","Clause 4.4 - Encroachments","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2936,null,1810]
[]
["44","Clause 4.5 - Existing premises occupied","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2937,null,1820]
[]
["45","Clause 4.6 - Services - known","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2938,null,1830]
[]
[null,"Management of contract (B5)",{"$nulls":8},2939,null,1840]
[]
["46","Clause 5.1 - Management of the works","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2940,null,1850]
[]
["47","Clause 5.2 - Progress meetings","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2941,null,1860]
["Item","Description","Uom","Quantity","Rate","Amount"]
["48","Clause 5.3 - Technical meetings","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2942,null,1870]
[]
[null,"Samples, shop drawings and manufacturer's instructions (B6)",{"$nulls":8},2943,null,1880]
[]
["49","Clause 6.1 - Samples of materials","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2944,null,1890]
[]
["50","Clause 6.2 - Workmanship samples","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2945,null,1900]
[]
["51","Clause 6.3 - Shop drawings","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2946,null,1910]
[]
["52","Clause 6.4 - Compliance with manufacturer's instructions","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2947,null,1920]
[]
[null,"Deposits and fees (B7)",{"$nulls":8},2948,null,1930]
[]
["53","Clause 7.1 - Deposits and fees","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2949,null,1940]
[]
[null,"Temporary services (B8)",{"$nulls":8},2950,null,1950]
[]
["54","Clause 8.1 - Water","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2951,null,1960]
[]
["55","Clause 8.2 - Electricity","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2952,null,1970]
[]
["56","Clause 8.3 - Ablution and welfare facilities","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2953,null,1980]
[]
["57","Clause 8.4 - Communication facilities","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2954,null,1990]
[]
[null,"Prime cost amounts (B9)",{"$nulls":8},2955,null,2000]
[]
["58","Clause 9.1 - Responsibility for prime cost amounts",{"$nulls":8},2956,null,2010]
[]
[null,"User note",{"$nulls":8},2956,null,2010]
[]
[null,"Where details of materials included in prime cost amounts are not readily",{"$nulls":8},2956,null,2010]
[]
[null,"available and it is therefore not possible for the contractor to price for waste, the",{"$nulls":8},2956,null,2010]
[]
[null,"relevant prime cost amount shall be inserted in the bills of quantities as a lump",{"$nulls":8},2956,null,2010]
[]
[null,"sum with the contractor being given the opportunity to separately price his",{"$nulls":8},2956,null,2010]
[]
[null,"overheads and profit and for taking delivery, etc as called for in this clause 9.1 of",{"$nulls":8},2956,null,2010]
[]
[null,"the preliminaries. In such case the fixing only or installation only of the relevant",{"$nulls":8},2956,null,2010]
[]
[null,"materials shall be provisionally measured for the contractor to price and shall be",{"$nulls":8},2956,null,2010]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"re-measured upon completion",{"$nulls":8},2956,null,2010]
[]
[null,"Where details of materials for which prime cost amounts are to be allowed are readily available, the quantity surveyor may elect to insert the relevant prime cost amounts in measured items, which measured items shall contain sufficient detail for the contractor to price for fixing and installation, waste, etc","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2956,null,2010]
[]
[null,"Attendance on subcontractors (B10)",{"$nulls":8},2957,null,2020]
[]
["59","Clause 10.1 - General attendance",{"$nulls":8},2958,null,2030]
[]
[null,"User note",{"$nulls":8},2958,null,2030]
[]
[null,"General attendance is defined as being the duties of the contractor in terms of clause 12.2 of the JBCC n/s subcontract agreement","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2958,null,2030]
[]
["60","Clause 10.2 - Special attendance",{"$nulls":8},2959,null,2040]
[]
[null,"User note",{"$nulls":8},2959,null,2040]
[]
[null,"Insert details after the provisional sums (nominated or selected subcontract amount for any special attendance where specifically required for each n/s subcontractor separately",{"$nulls":8},2959,null,2040]
[]
[null,"It is important to note that general attendance only requires the contractor to 'permit the subcontractor to use erected scaffolding, hoisting facilities, etc provided by the contractor, in common with others having the like right while it remains erected on the site' (refer to 12.2.13 of the JBCC n/s subcontract agreement). Many n/s subcontractors qualify their tenders to exclude scaffolding and/or hoisting facilities. Especially scaffolding could be an expensive item and it may be necessary in order to avoid claims to require the contractor to provide for the extended use of scaffolding for specific subcontracts within a description of 'special attendance' in the applicable bill","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2959,null,2040]
[]
[null,"General (B11)",{"$nulls":8},2960,null,2050]
[]
["61","Clause 11.1 - Protection of the works","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2961,null,2060]
[null,"(Protect works overnight from inclement weather e.g tarpaulin and support steel frames)"]
["62","Clause 11.2 - Protection/isolation of existing works and works occupied in sections","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2962,null,2070]
[]
["63","Clause 11.3 - Security of the works","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2963,null,2080]
[]
["64","Clause 11.4 - Notice before covering work","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2964,null,2090]
[]
["65","Clause 11.5 - Disturbance",{"$nulls":8},2965,null,2100]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"User note",{"$nulls":8},2965,null,2100]
[]
[null,"The following clause may be used should 'disturbance' [11.5] need to be extended",{"$nulls":8},2965,null,2100]
[]
[null,"Disturbance",{"$nulls":8},2965,null,2100]
[]
[null,"? All work is to be carried out in such a manner as to cause no unacceptable or unreasonable dust, noise, vibrations, nuisance, inconvenience, annoyance and the like to the public, others, other properties and traffic in so far as they exceed the permissible limitations set by government legislation or by the local authority. Any delays, stoppages and the like arising from or in order to comply with the above will not constitute grounds for an adjustment to the construction period or contract value whatsoever","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2965,null,2100]
[]
["66","Clause 11.6 - Environmental disturbance",{"$nulls":8},2966,null,2110]
[]
[null,"?Controlling all forms of pollution",{"$nulls":8},2966,null,2110]
[]
[null,"The contractor shall be responsible for and take all precautions in controlling by whatever means necessary all forms of pollution emanating from the site during the construction period due inter alia to noise, artificial light, wind-blown sand, dust, deposits of mud, etc.",{"$nulls":8},2966,null,2110]
[]
[null,"The contractor is to ensure that all roads which border the site and are used by the contractor during the execution of the works  are kept clean and free of any dirt or debris caused by the execution of the works",{"$nulls":8},2966,null,2110]
[]
[null,"User note",{"$nulls":8},2966,null,2110]
[]
[null,"Insert the following clause if an environmental management plan (EMP) is available and insert the EMP in an annexure",{"$nulls":8},2966,null,2110]
[]
[null,"Environmental management plan",{"$nulls":8},2966,null,2110]
[]
[null,"The employer has prepared an environmental management plan (EMP) (refer to Annexure ? for a copy of the relevant plan). The contractor shall price opposite this item for compliance with all the requirements of such EMP","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2966,null,2110]
[]
["67","Clause 11.7 - Works cleaning and clearing","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2967,null,2120]
[]
["68","Clause 11.8 - Vermin","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2968,null,2130]
[]
["69","Clause 11.9 - Overhand work","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2969,null,2140]
[]
["70","Clause 11.10 - Tenant installations","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2970,null,2150]
[]
["71","Clause 11.11 - Advertising","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2971,null,2160]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"User note",{"$nulls":8},2972,null,2170]
[]
[null,"Where details of materials included in prime cost amounts are readily available and it is therefore not possible for the contractor to price for waste, the relevant prime cost amount shall be inserted in the bills of quantities as a lump sum with the contractor being given the opportunity to separately price his overheads and profit and for taking delivery, etc as called for in this clause 9.1 of the preliminaries. In such case the fixing only or installation only of the relevant materials shall be provisionally measured for the contractor to price and shall be re-measured upon completion",{"$nulls":8},2972,null,2170]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"SECTION  C: SPECIFIC PRELIMINARIES",{"$nulls":8},2973,null,2180]
[]
[null,"User note",{"$nulls":8},2974,null,2190]
[]
[null,"Users shall avoid inserting in Section C items which may be construed as amending, modifying, correcting or supplementing the provisions of the JBCC Principal Building Agreement. Such amendments, modifications, corrections or supplements should be kept to the absolute minimum and should be inserted in Section A under the recited clause headings of the JBCC Principal Building Agreement in this Bill No. 1",{"$nulls":8},2974,null,2190]
[]
[null,"Selected examples of typical clauses are provided to indicate ways of describing such clauses. Users must delete, adapt or add to these examples to suit their particular circumstances",{"$nulls":8},2974,null,2190]
[]
[null,"Warranties for materials and workmanship",{"$nulls":8},2975,null,2200]
[]
[null,"Where warranties for materials and/or workmanship are called for, the contractor shall obtain a written warranty, addressed to the employer, from the entity supplying the materials and/or executing the work and shall deliver same to the principal agent on final completion of the contract",{"$nulls":8},2975,null,2200]
[]
[null,"The warranty shall state that workmanship, materials and installation are warranted for a specific period from the date of practical completion and that any defects that may arise during the specified period shall be made good at the expense of the entity supplying the materials and/or doing the work, upon written notice",{"$nulls":8},2975,null,2200]
[]
[null,"The warranty will not be enforced if the work is damaged by defects in the execution of the works, in which case the responsibility for replacement shall rest entirely with the contractor",{"$nulls":8},2975,null,2200]
[]
[null,"Specific Preliminaries",{"$nulls":8},2976,null,2380]
[]
["72","Overtime",{"$nulls":8},2977,null,2210]
[]
[null,"Should overtime be required to be worked for any reason whatsoever, the cost of such overtime is to be borne by the contractor unless the principal agent has specifically authorised, prior to execution thereof, that costs for such overtime are to be borne by the employer","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2977,null,2210]
["Item","Description","Uom","Quantity","Rate","Amount"]
["73","Cooperation of the contractor for cost management",{"$nulls":8},2978,null,2220]
[]
[null,"It is specifically agreed that the contractor accepts the obligation of assisting the principal agent in implementing proper cost management. The contractor will be advised by the principal agent of all cost management procedures which will be implemented to ensure that the contract value does not exceed the budget","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2978,null,2220]
[]
["74","Overloading",{"$nulls":8},2979,null,2230]
[]
[null,"The contractor shall take all necessary steps to ensure that no damage occurs due to overloading of any portion of the works or temporary works eg scaffolding, etc. The contractor shall submit details of his proposed loading, storage, plant erection, etc to the principal agent for approval prior to proceeding with such loading, storing or erecting and shall comply with and pay for the principal agent's requirements in connection with the provision of temporary support work, etc. Any damage caused to the works by overloading shall be made good by the contractor at his sole expense","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2979,null,2230]
[]
["75","Propping of floors below",{"$nulls":8},2980,null,2240]
[]
[null,"The contractor is advised that propping of floors below may be required if he wishes to use any areas of completed suspended reinforced concrete slabs for vehicle access, storage of materials and goods and location of plant, scaffolding, etc. The location of these areas and any necessary propping shall be approved by the principal agent and the cost thereof shall be borne by the contractor","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2980,null,2240]
[]
["76","Testing of flat roof waterproofing for watertightness",{"$nulls":8},2981,null,2250]
[]
[null,"Flat roof waterproof areas shall be flooded and kept 'ponded' for at least forty eight hours as a test to ensure the watertightness of the waterproofing and before any further construction work is carried out above the waterproofing","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2981,null,2250]
[]
[null,"User note",{"$nulls":8},2982,null,2260]
[]
[null,"Insert the following where a health and safety specification IS NOT YET available. Note that there is an obligation on the employer to ensure that the contractor has priced opposite this item for the compliance with the act and the regulations and the reasonable provisions of the health and safety specification",{"$nulls":8},2982,null,2260]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"Health and safety",{"$nulls":8},2983,null,2270]
[]
[null,"Without limiting the generality of the provisions of clause 2.0, the contractor's attention is drawn to the provisions of the Construction Regulations issued in terms of the Occupational Health and Safety Act, 1993 as amended. It is specifically stated that the employer shall prepare a documented health and safety specification for the works and that the employer shall ensure that the contractor has made provision for the cost of health and safety measures during the execution of the works. The  contractor shall price opposite this item for compliance with the act and the regulations and the reasonable provisions of the aforementioned health and safety specification [2.1]",{"$nulls":8},2983,null,2270]
[]
[null,"User note",{"$nulls":8},2984,null,2280]
[]
[null,"Insert the following where a health and safety specification IS available. Note that there is an obligation on the employer to ensure that the contractor has priced opposite this item for the compliance with the act and the regulations and the reasonable provisions of the health and safety specification",{"$nulls":8},2984,null,2280]
[]
["77","Health and safety",{"$nulls":8},2985,null,2290]
[]
[null,"Without limiting the generality of the provisions of clause 2.0, the contractor's attention is drawn to the provisions of the Construction Regulations issued in terms of the Occupational Health and Safety Act, 1993 as amended. It is specifically stated that the employer shall prepare a documented health and safety specification for the works (refer to Annexure ? for a copy of the relevant specification) and that the employer shall ensure that the contractor has made provision for the cost of health and safety measures during the execution of the works. The contractor shall price opposite this item for compliance with the act and the regulations and the provisions of the aforementioned health and safety specification [2.1]","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2985,null,2290]
[]
["78","The contractor shall",{"$nulls":8},2986,null,2300]
[]
[null,"1.   Comply with the health and safety specification for the works",{"$nulls":8},2986,null,2300]
[]
[null,"2.   Prepare and agree with the health and safety consultant the health and  safety plan for the works",{"$nulls":8},2986,null,2300]
[]
[null,"3.   Cooperate with the health and safety consultant in all respects",{"$nulls":8},2986,null,2300]
[]
[null,"4.   Manage the compliance of all subcontractors with the regulations and with the health and safety plan and specification",{"$nulls":8},2986,null,2300]
[]
[null,"5.   Conform to the conditions contained in the employer's health and safety specification","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2986,null,2300]
["Item","Description","Uom","Quantity","Rate","Amount"]
["79","Green star building certification",{"$nulls":8},2987,null,2310]
[]
[null,"User note",{"$nulls":8},2987,null,2310]
[]
[{"$nulls":10},2987,null,2310]
[]
[null,"Insert the provisions called for by the relevant green star consultant should it be a requirement that the project be submitted for green star certification","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2987,null,2310]
[]
["80","Broad based black economic empowerment (BBBEE)",{"$nulls":8},2988,null,2320]
[]
[null,"Tenders submitted will be evaluated taking into account their empowerment rating",{"$nulls":8},2988,null,2320]
[]
[null,"The employer will be monitoring the broad based black economic empowerment (BBBEE) status of the contractor throughout the execution of the works",{"$nulls":8},2988,null,2320]
[]
[null,"The contractor is to submit to the principal agent on an annual basis a schedule of spend, split into vendors engaged as subcontractors and suppliers indicating their BBBEE rating including proof of the said rating","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2988,null,2320]
[]
["81","Advertising rights",{"$nulls":8},2989,null,2330]
[]
[null,"The may elect to contract with advertising agencies for the erection of advertising hoardings, banners, wraps or the like for the duration of the contract. The contractor shall not prevent such an arrangement and will assist in the facilitation of same.  The position and type of advertising structure to be agreed with the principal agent so as not to hinder the contractor in meeting his obligations under this agreement","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2989,null,2330]
[]
["82","Confidentiality",{"$nulls":8},2990,null,2340]
[]
[null,"The contractor undertakes to maintain in confidence any and all information regarding this project and shall obtain appropriate similar undertakings from all subcontractors and suppliers. Such information shall not be used in any way except in connection with the execution of the works",{"$nulls":8},2990,null,2340]
[]
[null,"No information regarding this project shall be published or disclosed without the prior written consent of the employer","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2990,null,2340]
["Item","Description","Uom","Quantity","Rate","Amount"]
["83","Media releases",{"$nulls":8},2991,null,2350]
[]
[null,"All rights of publication of articles in the media, together with any advertising relating thereto or in any way connected with this project, shall vest with the employer",{"$nulls":8},2991,null,2350]
[]
[null,"The contractor together with his subcontractors shall not, without the prior written consent of the employer, cause any statement or advertisement connected with this project to be printed, screened or aired by the media","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2991,null,2350]
[]
[null,"SUMMARY OF CATEGORIES",{"$nulls":8},2992,null,2360]
[]
[null,"Category : Fixed   R........................................",{"$nulls":8},2993,null,2370]
[]
[null,"Category : Value  R........................................",{"$nulls":8},2993,null,2370]
[]
[null,"Category : Time    R........................................",{"$nulls":8},2993,null,2370]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"SECTION NO. 2 : BUILDINGS"]
[]
[]
[null,"BILL NO.1 : ALTERATIONS"]
[]
[null,"TEMPORARY BARRICADES, SCREENS, ETC",{"$nulls":8},2854,null,500]
[]
[null,"Temporary barricades, screens, roofs, etc including removal",{"$nulls":8},2855,null,510]
[]
["1","The Contractor to provide temporary cover to prevent any damage from water and for security. (Protect works overnight from inclement weather e.g tarpaulin and support steel frames)","m²",{"v":500,"d":"500.00"},{"$nulls":4},500,null,2856,null,530]
[]
[null,"REMOVAL OF EXISTING WORK",{"$nulls":8},2828,null,570]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc",{"$nulls":8},2835,null,1080]
[]
["2","Pitched roof 9560m high overall,  of  timber trusses and purlins, IBR sheet steel covering, eaves soffit covering, fascias, barge boards, gutters and rainwater pipes","m²",{"v":458,"d":"458.00"},{"$nulls":4},458,null,2836,null,1100]
[]
["3","Suspended ceilings, including suspension grid, hangers, etc and set aside for later refixing in a similar position","m²",{"v":455,"d":"455.00"},{"$nulls":4},455,null,2837,null,1160]
[]
[null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc",{"$nulls":8},2829,null,1500]
[]
["4","Remove 13mm of 100mm thick aggregate stone and store as directed by client on site","m²","  1 064",{"$nulls":4},1064,null,2830,null,1510]
[]
[null,"RE-FIXING OF SET ASIDE MATERIAL",{"$nulls":8},2838,null,1510]
[]
[null,"Take from where set aside and refix in similar new position as directed by the Client",{"$nulls":8},2839,null,1510]
[]
["5","Suspended ceilings including new suspension grids","m²",{"v":500,"d":"500.00"},{"$nulls":4},500,null,2840,null,1510]
[]
[null,"Budgetary allowance",{"$nulls":8},2832,null,1510]
[]
["6","Allow a Budgetary allowance of R50 000.00 (Fifty Thousand Rands) for alteration works to be dertemined on site","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2833,null,1510]
[]
["7","Allow a Budgetary allowance of R 120 000.00 (One Hundred and Twenty Thousand Rands) for temporary accomodation for the duration of 6 months","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,2834,null,1510]
[]
[]
[null,"Bill Total",{"$nulls":3},{"v":0,"d":"0.00"}]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"BILL NO.2 : MASONRY"]
[]
[null,"BRICKWORK",{"$nulls":8},3039,null,28550]
[]
[null,"Sizes in descriptions",{"$nulls":8},3040,null,28560]
[]
[null,"Where sizes in descriptions are given in brick units, one brick shall represent the length and half brick the width of a brick",{"$nulls":8},3041,null,28570]
[]
[null,"User note",{"$nulls":8},3042,null,28580]
[]
[null,"The following preamble generally applies for works in hot and humid coastal areas",{"$nulls":8},3043,null,28590]
[]
[null,"Bagged and sealed walls",{"$nulls":8},3044,null,28600]
[]
[null,"Walls in two skins described as bagged and sealed shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture and sealed with two coats   bitumen emulsion waterproofing coating",{"$nulls":8},3045,null,28610]
[]
[null,"Face bricks",{"$nulls":8},3046,null,28620]
[]
[null,"Bricks shall be ordered timeously to obtain uniformity in size and colour",{"$nulls":8},3047,null,28630]
[]
[null,"Pointing",{"$nulls":8},3048,null,28640]
[]
[null,"Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc",{"$nulls":8},3049,null,28650]
[]
[null,"BRICKWORK IN SUPERSTRUCTURE",{"$nulls":8},3051,null,28800]
[]
[null,"Brickwork of NFP bricks in class II mortar",{"$nulls":8},3052,null,90430]
[]
["1","One brick walls of two half brick skins with inner skin bagged and sealed (in gabbles)","m²",{"v":20,"d":"20.00"},{"$nulls":4},20,null,3053,null,90750]
[]
[null,"2,5mm Brickwork reinforcement",{"$nulls":8},3054,null,95200]
[]
["2","150mm Wide reinforcement built in horizontally","m",{"v":80,"d":"80.00"},{"$nulls":4},80,null,3055,null,95210]
[]
[null,"FACE BRICKWORK",{"$nulls":8},3056,null,30160]
[]
[null,"Corobrik 'Firelight Satin' or equal approved FBS clay face bricks pointed with  horizontal and vertical joints",{"$nulls":8},3057,null,30170]
[]
["3","Extra over brickwork for face brickwork in soldier courses","m²",{"v":20,"d":"20.00"},{"$nulls":4},20,null,3058,null,30310]
[]
[]
[null,"Bill Total"]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"BILL NO.3 : WATERPROOFING"]
[]
[null,"WATERPROOFING TO FLAT SCREEDED ROOFS",{"$nulls":8},2820,null,33210]
[]
[null,"One layer Derbigum SP4 waterproofing membrane, with 75mm side laps and 100mm end laps, sealed to primed surface to falls and cross falls by 'torch-fusion' finished with one coat of acrylic primer followed by two coats acrylic paint. Waterproofing to be installed by an Approved Derbigum Contractor under ten year guarantee.",{"$nulls":8},2821,null,33250]
[]
["1","On flat roof","m²","  1 064",{"$nulls":4},1064,null,2822,null,33260]
[]
[null,"One layer Derbigum SP4 waterproofing membrane, with 75mm side laps and 100mm end laps, sealed to primed surface to falls and crossfalls by 'torch-fusion' finished with two coats bituminous aluminium paint. Waterproofing to be installed by an Approved Derbigum Contractor under ten year guarantee.",{"$nulls":8},2823,null,33260]
[]
["2","on flat roof","m²","  1 064",{"$nulls":4},1064,null,2824,null,33260]
[]
[null,"WATERPROOFING TO ROOFS ETC",{"$nulls":8},2817,null,33390]
[]
[null,"Approved acrylic flashing",{"$nulls":8},2818,null,33670]
[]
["3","Headwall flashings 460mm girth to junction of roof sheeting","m",{"v":100,"d":"100.00"},{"$nulls":4},100,null,2819,null,33671]
[]
[null,"PROTECTIVE STONE DRESSING",{"$nulls":8},2825,null,33671]
[]
[null,"Clean crushed stone dressing free of pyrite or other contaminants, of 25mm stone evenly spread with larger stones around outlet",{"$nulls":8},2826,null,33671]
[]
["4","Supply and lay 50mm thick of 25mm agregates on waterproofing to flat roofs","m²","  1 064",{"$nulls":4},1064,null,2827,null,33671]
[null,"( Refer to Drawing No.5IED03-01R-A)"]
[]
[null,"Bill Total"]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"BILL NO.4 : ROOF COVERINGS"]
[]
[null,"Supply and lay Klip-Tite 700' 0,8mm thick clean Colorbond Ultra AZ200 spelter G550 with 'Global' coat finish on one side and half coat 'Shadow Grey' other side and accessories fixed to timber purlins or rails at 1200mm centres:( Refer to Drawing No.5IED03-02R-A)",{"$nulls":8},196,null,41888]
[]
["1","Roof covering with pitch not exceeding 25 degrees, in transportable lengths not exceeding 20m.","m²",{"v":458,"d":"458.00"},{"$nulls":4},458,null,197,null,41889]
[]
["2","Extra over Roof covering for bullnose to 500mm radius and edge.","m",{"v":100,"d":"100.00"},{"$nulls":4},100,null,3038,null,41889]
[]
[null,"Flashings:",{"$nulls":8},198,null,41725]
[]
["3","Ridge capping 550mm girth, three times bent along girth and notched on site to suit roof profile.","m",{"v":28,"d":"28.00"},{"$nulls":4},28,null,199,null,41728]
[]
["4","Polyclosers to suite profile of sheeting.","m",{"v":184,"d":"184.00"},{"$nulls":4},184,null,202,null,41739]
[]
["5","Ridge end cap","No",{"v":10,"d":"10.00"},{"$nulls":4},10,null,203,null,41739]
[]
[null,"ROOF AND WALL LINING AND INSULATION",{"$nulls":8},204,null,12278]
[]
[null,"Supply and lay Scrim Facing Insulationâ Heavy Industrial Grade 430 - double sided reflective foil laminate incorporating layers of natural kraft paper and fibre glass reinforcing scrim , laminated together with low density polyethylene flame retardant adhesive with R-Value not less than 1.58kw/m2 and class A/A1 fire rating in accordance with SANS 10177-5 and SANS 10177-10.",{"$nulls":8},2386,null,12278]
[]
["6","Insulation laid taut over timber rafters (at approximately 1200mm centres) and fixed concurrent with tiling battens, purlins, etc.","m²",{"v":455,"d":"455.00"},{"$nulls":4},455,null,2387,null,12278]
[]
[null,"RIBBED METAL SHEETING AND ACCESSORIES",{"$nulls":8},195,null,12196]
[]
[]
[null,"Bill Total"]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"BILL NO.5 : CARPENTRY AND JOINERY"]
[]
[null,"TRADE PREAMBLES",{"$nulls":8},2306,null,12363]
[]
[null,"Trade Preambles:",{"$nulls":8},2307,null,12363]
[]
[null,"For Trade Preambles refer to 'Specification of Materials and Methods' for the full description of materials to be used and work to be done in this Bill",{"$nulls":8},2308,null,12363]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":8},2311,null,12363]
[]
[null,"Proprietary items or materials",{"$nulls":8},2312,null,12363]
[]
[null,"Proprietary items or materials where specefied are to be of the brand specified - or other approved by the Principal Agent",{"$nulls":8},2316,null,12363]
[]
[null,"Prefabricated plate nailed timber roof truss construction:",{"$nulls":8},208,null,12363]
[]
["1","Mono pitch roof truss with a clear span of 4545mm rising 426mm to apex.","No",{"v":10,"d":"10.00"},{"$nulls":4},10,null,2466,null,12363]
[]
["2","Mono pitch roof truss with a clear span of 5190mm rising 426mm to apex.","No",{"v":5,"d":"5.00"},{"$nulls":4},5,null,212,null,12363]
[]
["3","Double pitch roof truss with a clear span of 9780mm rising 932mm to apex.","No",{"v":9,"d":"9.00"},{"$nulls":4},9,null,210,null,12363]
[]
["4","Double pitch roof truss with a clear span of 15100mm rising 956mm to apex.","No",{"v":13,"d":"13.00"},{"$nulls":4},13,null,2570,null,12363]
[]
["5","Double pitch roof truss with a clear span of 29101mm rising 956mm to apex.","No",{"v":25,"d":"25.00"},{"$nulls":4},25,null,2831,null,12363]
[]
[null,"ROOF CONSTRUCTION",{"$nulls":8},215,null,12364]
[]
[null,"Sawn softwood :",{"$nulls":8},216,null,12366]
[]
["6","38 x 114mm Wall plates.","m",{"v":72,"d":"72.00"},{"$nulls":4},72,null,217,null,12372]
[]
["7","38 x 114mm Bracings.","m",{"v":72,"d":"72.00"},{"$nulls":4},72,null,218,null,12372]
[]
["8","38 x 114mm Sprockets.","m",{"v":49,"d":"49.00"},{"$nulls":4},49,null,219,null,12372]
[]
["9","50 x 114mm Purlins.","m","  7 056",{"$nulls":4},7056,null,223,null,12372]
[]
[null,"ROOF SUNDRIES",{"$nulls":8},233,null,12452]
[]
[null,"Sundries:",{"$nulls":8},234,null,12454]
[]
["10","Two coats creosote on sawn timbers.","m²",{"v":35,"d":"35.00"},{"$nulls":4},35,null,236,null,12456]
[]
["11","Teco rafter / beam connector.","No","  3 038",{"$nulls":4},3038,null,241,null,12459]
[]
["12","2,5mm Diameter galvanised wire tie 400mm girth wrapped around rafter and purlin with ends tied together.","No","  6 076",{"$nulls":4},6076,null,242,null,12461]
[]
[]
[null,"Bill Total"]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"BILL NO.6 : STRUCTURAL STEELWORK"]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":8},2994,null,48970]
[]
[null,"Descriptions",{"$nulls":8},2995,null,49020]
[]
[null,"Descriptions of bolts shall be deemed to include nuts and washers",{"$nulls":8},2996,null,49030]
[]
[null,"Descriptions of L-shaped and U-shaped anchor bolts shall be deemed to include bending, threading, nuts and washers and embedding in concrete",{"$nulls":8},2997,null,49040]
[]
[null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete",{"$nulls":8},2998,null,49050]
[]
[null,"STEEL COLUMNS AND BEAMS",{"$nulls":8},2999,null,49060]
[]
[null,"Supply and Install Welded rafters in single lengths with flat section bearer and connection plates, bolted to concrete",{"$nulls":8},3000,null,105273]
[null,"( Refer to Drawing No.5IED03-02R-A)"]
["1","203 x 133mm x 25kg/m I-section rafter","Tonnes",{"v":2.2,"d":"2.20"},{"$nulls":4},2.2,null,3001,null,105283]
[]
[null,"STEEL PURLINS, GIRTS, BRACING, ETC",{"$nulls":8},3002,null,161313]
[]
[null,"Purlins and girts, bolted to steel",{"$nulls":8},3003,null,161323]
[]
["2","125 x 65 x 20 x 2.5mm Thick cold-formed lipped channel purlins","Tonnes",0.68,{"$nulls":4},0.68,null,3004,null,161383]
[]
[null,"Welded bracing, anti-sag rails, etc with flat connection plates, bolted to steel",{"$nulls":8},3005,null,161413]
[]
["3","40 x 40 x 6mm Angle section","Tonnes",0.28,{"$nulls":4},0.28,null,3006,null,161483]
[]
["4","50 x 50 x 5mm Angle bracing","Tonnes",0.13,{"$nulls":4},0.13,null,3010,null,161483]
[]
["5","40 x 40 x 6mm Angle section knee bracing","Tonnes",0.14,{"$nulls":4},0.14,null,3011,null,161483]
[]
[null,"BOLTS, FASTENERS, ETC",{"$nulls":8},3007,null,161953]
[]
[null,"Supply and install Hot deep galvanised grade 300W steel plate",{"$nulls":8},3008,null,161963]
[]
["6","16mm plates in brackets, end plates, stiffeners, etcHigh tensile bolts","Tonnes",0.11,{"$nulls":4},0.11,null,3009,null,161973]
[]
["7","20mm diameter high tensile bolts","Tonnes",0.05,{"$nulls":4},0.05,null,3012,null,161973]
[]
[]
[null,"Bill Total"]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"BILL NO.7 : PLASTERING"]
[]
[null,"SCREEDS",{"$nulls":8},2844,null,55090]
[]
[null,"Supply and lay screed on concrete",{"$nulls":8},2845,null,55100]
[]
["1","50mm Thick on roof slab","m²",{"v":35,"d":"35.00"},{"$nulls":4},35,null,2846,null,109603]
[]
[]
[null,"Bill Total"]
[]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"BILL NO.8 : PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL",{"$nulls":8},411,null,17852]
[]
[null,"Supply and install seamless aluminium prepainted gutters and rainwater pipes:",{"$nulls":8},412,null,17896]
[]
["1","150 x 150mm Roof gutters.","m",{"v":76,"d":"76.00"},{"$nulls":4},76,null,413,null,17899]
[]
["2","Extra over gutter for stopped end.","No",{"v":6,"d":"6.00"},{"$nulls":4},6,null,414,null,17903]
[]
["3","Extra over gutter for outlet for 150mm pipe.","No",{"v":12,"d":"12.00"},{"$nulls":4},12,null,415,null,17906]
[]
["4","150mm Rainwater pipes.","m",{"v":42,"d":"42.00"},{"$nulls":4},42,null,416,null,17908]
[]
["5","Extra over 75 x 50mm  rainwater pipe for bend.","No",{"v":22,"d":"22.00"},{"$nulls":4},22,null,417,null,17909]
[]
["6","Extra over 150mm  rainwater pipe for shoe.","No",{"v":22,"d":"22.00"},{"$nulls":4},22,null,418,null,17910]
[]
[null,"Fullbore' cast iron outlets",{"$nulls":8},2842,null,58190]
[]
["7","100mm vertical outlet & joint Upvc pipe","No",{"v":16,"d":"16.00"},{"$nulls":4},16,null,2843,null,58200]
[]
[null,"uPVC class 34  gutters and rainwater pipes",{"$nulls":8},2848,null,57680]
[]
["8","75mm Rainwater down pipes","m",{"v":48,"d":"48.00"},{"$nulls":4},48,null,2850,null,57680]
[]
["9","110mm Rainwater pipes in ducts","m",{"v":128,"d":"128.00"},{"$nulls":4},128,null,2849,null,57750]
[]
[null,"SLEEVES",{"$nulls":8},2851,null,64330]
[]
[null,"HDPE sleeves for pipes exceeding 100mm and not exceeding 200mm  diameter",{"$nulls":8},2852,null,64400]
[]
["10","Sleeve not exceeding 250mm long","No",{"v":10,"d":"10.00"},{"$nulls":4},10,null,2853,null,64410]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]
[]
["Item","Description","Uom","Quantity","Rate","Amount"]
[null,"SECTION NO. 3 : PROVISIONAL SUMS"]
[]
[]
[null,"BILL NO.1 : PROVISIONAL SUMS"]
[]
[null,"PROVISIONAL SUMS",{"$nulls":8},3013,null,75340]
[]
[null,"The following Provisional amount are Nett Amount EXCLUSIVE of commision for the Contractor. The amounts are for the work to be executed complete by Nominated /Selected Sub- Contractors.",{"$nulls":8},3016,null,75390]
[]
[null,"PROVISIONAL SUMS FOR NOMINATED/SELECTED SUBCONTRACTOR WORKS",{"$nulls":8},3017,null,75390]
[]
[null,"LIFT INSTALLATION",{"$nulls":8},3018,null,75390]
[]
["1","Provide the amount of  R 2 000 000.00 (Two Million) for Lift installation and backup battery","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,3019,null,75390]
[]
["2","Profit on the above","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,3059,null,75390]
[]
["3","Attendance on the above","Item",{"v":1,"d":"1.00"},{"$nulls":4},1,null,3060,null,75390]
[]
[null,"BUDGETARY ALLOWANCES",{"$nulls":8},1677,null,36195]
[]
[null,"ELECTRICAL WORKS",{"$nulls":8},1678,null,36185]
[]
["4","Provide the amount of  R 300 000.00 ( Three Hundred Thousand ) for electrical installation.","Item",{"$nulls":5},1,null,1679,null,36195]
[]
[null,"MECHANICAL WORKS",{"$nulls":8},1680,null,36185]
[]
["5","Provide the amount of  R 450 000.00 ( Four Hundred and Fifty Thousand ) for mechanical installation.","Item",{"$nulls":5},1,null,1681,null,36195]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]

{"sheet":"Final summary","index":1,"n_rows":62,"n_cols":3,"rows_kept":62,"merged":[[4,0,4,4],[5,0,5,4],[22,3,22,4],[23,3,23,4],[24,3,24,4],[25,3,25,4],[26,3,26,4],[28,3,28,4],[34,3,34,4],[36,3,36,4],[39,3,39,4],[46,3,46,4],[51,3,51,4]],"flags":["formulas_cached_only"]}
[]
[]
[]
["MODIFICATION OF SUPPLY CHAIN BUILDING PHASE 1"]
[]
[]
[]
[]
[]
["FINAL SUMMARY"]
[]
[]
[]
[]
[]
[]
[null,"PAGE","AMOUNT"]
[]
[]
["CONDITIONS OF CONTRACT"]
[]
[]
["SECTION 1        :  PRELIMINARY AND GENERAL","1-30"]
[]
["SECTION 2        :  BUILDINGS","2-12"]
[]
["SECTION 3        :  PROVISIONAL SUMS","3-2"]
{"$rows_empty":7}
["SUB TOTAL","R"]
[]
["ADD: CONTINGENCIES @ 10%","R"]
[]
[]
["SUB TOTAL","R"]
[]
[]
[]
[]
["VALUE ADDED TAX"]
[]
["Value added tax @ 15%","R"]
[]
[]
[]
[]
["TOTAL (FIXED PRICE) ","R"]
{"$rows_empty":9}
["FS-1"]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}