{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["0175985","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"0175985","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[19,3,19,4],[22,3,22,4],[25,2,25,4],[26,2,26,4],[27,3,27,4],[30,3,30,4],[39,1,39,3],[41,0,41,6],[43,0,43,1],[48,2,48,3]]}
[null,"Technical Schedules A and B for"]
[null,"T-OFF,MAIN 9.0-15.0 TAP 9.0-15.0 D3153"]
[null,"Eskom SAP No: 0175985"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":175985,"d":"0175985"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Supplier","Supplier Name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer","Manufacturer Name","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Product Code","Product Code","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Drawing number & Revision number","Drawing and Revision Number","xxxxxxxxxx"]
[null,"1.1.6",null,"Manufacturer's unique identifier indelibly marked on product body as per Eskom D-DT-3153","Identification Mark","xxxxxxxxxx"]
[null,"1.1.7",null,"Compliance to all dimensions and requirements of Eskom Buyer's Guide Drawings   ","Eskom D-DT-3153","YES"]
[null,"1.1.8",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Material Grade",null,"ALUMINIUM"]
[]
[null,1.3,"·","Galvanising"]
[null,"1.3.1",null,"Average minimum galvanising thickness on product body complies to SANS121","Hot Dipped","YES"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,"2.1.2",null,"Material grade certification","Certification submitted","YES"]
[null,2.2,"·","Test Reports",null,"Required","Report\nNumber"]
[null,"2.2.1",null,"Visual examination (SANS 61284)","Test Report Submitted","YES"]
[null,"2.2.2",null,"Dimensional and material verification (SANS 61284)","Test Report Submitted","YES"]
[null,"2.2.3",null,"Hot Dip Galvanising certificate for product body (SANS 61284)","Test Report Submitted","YES"]
[null,"2.2.4",null,"Non-destructive testing - Hardness Test  (SANS 61284)","Test Report Submitted","YES"]
[]
[null,3,null,"Packaging"]
[null,3.1,null,"Packaging material, method and maximum quantity, not exceeding 50 units or 800kg (as per clause 4.18 of Eskom 240-60777474)","Wooden Boxes, Crates or Pallets, Hessian / Cloth Bags ","YES"]
[]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,null,"Company Name"]
[]
[]
[]
[null,null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":45,"n_cols":5,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,2,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[37,0,37,5],[40,0,40,2],[40,4,40,5],[44,0,44,2],[44,4,44,5]]}
["Deviation schedule"]
["T-OFF,MAIN+TAP 6.3-9.0 ACA/SQUIR D3153"]
["Eskom SAP No:0175985"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":30}
["SIGNATURES"]
[]
["SUPPLIER SIGNATURES"]
[]
["         "]
["Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
["Sign",{"$nulls":3},"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":20,"n_cols":5,"rows_kept":20,"merged":[[0,1,0,4],[1,1,1,4],[2,1,2,4],[12,0,12,5],[15,0,15,2],[15,4,15,5],[19,0,19,2],[19,4,19,5]]}
[null,"Test Report Schedule"]
[null,"T-OFF,MAIN+TAP 6.3-9.0 ACA/SQUIR D3153"]
[null,"Eskom SAP No: 0175985"]
[null,1,2,3,4]
[null,"Item ","Description","Specification","Report No."]
[null,"2.2.1","Visual examination","SANS 61284"]
[null,"2.2.2","Dimensional and material verification","SANS 61284"]
[null,"2.2.3","Hot Dip Galvanising certificate for product body","SANS 61284"]
[null,"2.2.4","Non-destructive testing - Hardness Test","SANS 61284"]
[]
[]
[]
["SUPPLIER SIGNATURES"]
[]
["         "]
["Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
["Sign",{"$nulls":3},"Date"]