{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["Tender Cover Sheet","Components","Assemblies  ","CPA Formula","T & O "],"not_rendered":{"images":1,"external_links":41,"defined_names":1173},"read":"whole","date_system":"1900"}

{"sheet":"Tender Cover Sheet","index":0,"n_rows":35,"n_cols":4,"rows_kept":35}
[]
[null,"Enquiry No.","E1396NTCSAMWP"]
[null,"Package Name:","The design, manufacture, testing, supply and delievy of Line Hardware on an “as and when” required basis for a period of 5 (five) years for Transmission Division."]
[null,"Tenderer's Name:"]
[]
[]
[]
[]
[]
[]
[null,"PRICING INFORMATION"]
[]
[null,"RAND VALUE IN WORDS",null," "]
[]
[]
[null,"TENDERED PRICE:  IN ZAR",{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,"(excluding VAT)"]
[]
[null,"TENDERED PRICE:  IN ZAR"]
[null,"(including VAT)",{"$f":"#REF!","v":{"$error":"#REF!"}}]
[]
[]
[]
[null,"DATE :"]
[]
[]
[null,"FULL NAMES OF SIGNATORY:"]
[]
[]
[]
[null,"DESIGNATION OF SIGNATORY:"]
[]
[]
[null,"SIGNATURE :"]
[{"$nulls":3}," "]

{"sheet":"Components","index":1,"n_rows":185,"n_cols":7,"rows_kept":185,"merged":[[184,1,184,5]]}
[]
[null,"COMPONENTS"]
[null,"ITEM","ITEM DESCRIPTION","Conductor\neg Tern, Wolf, Bear","Configuration\nTwin/Trip\nQuad/Hex","QTY","Link CPA"]
[null,1,"2X 380 mm spacing Spacer Damper for Conductor","Goat","Twin",315,"eg: A"]
[null,2,"2X 380 mm spacing Spacer Damper for Conductor","Tern","Twin",310]
[null,3,"2X 570 mm spacing Spacer Damper for Conductor","Dinosaur","Twin",35]
[null,4,"3X 450 mm spacing Spacer Damper for Conductor","Tern","Trip",7698]
[null,5,"3X 570 mm spacing Spacer Damper for Conductor","Bersfort","Trip",1607]
[null,6,"3X 570 mm spacing Spacer Damper for Conductor","Dinosaur","Trip",153]
[null,7,"3X 570 mm spacing Spacer Damper for Conductor","IEC315","Trip",12716]
[null,8,"3X 570 mm spacing Spacer Damper for Conductor","Kingbird","Trip",45]
[null,9,"4X 380 mm spacing Spacer Damper for Conductor","Tern","Quad",1500]
[null,10,"4X 380 mm spacing Spacer Damper for Conductor","Wolf","Quad",38]
[null,11,"4X 380 mm spacing Spacer Damper for Conductor","Zebra","Quad",49]
[null,12,"4X 570 mm spacing Spacer Damper for Conductor","IEC560","Quad",1075]
[null,13,"6X 320 mm spacing Spacer Damper for Conductor","Tern","Hex",12000]
[null,14,"Spacer Damper - twin bear","Bear","Twin",10]
[null,15,"Midspan Joints for Conductor","Bear","Twin",13]
[null,16,"Midspan Joints for Conductor","Bersfort","Trip",439]
[null,17,"Midspan Joints for Conductor","Dinosaur","Trip",38]
[null,18,"Midspan Joints for Conductor","Goat","Twin",60]
[null,19,"Midspan Joints for Conductor","IEC315","Trip",2885]
[null,20,"Midspan Joints for Conductor","IEC560","Quad",212]
[null,21,"Midspan Joints for Conductor","Kingbird","Trip",4.5]
[null,22,"Midspan Joints for Conductor","Tern","Hex",13593]
[null,23,"Midspan Joints for Conductor","Wolf","Quad",13]
[null,24,"Midspan Joints for Conductor","Zebra","Quad",27]
[null,25,"Vibration damper","Bear","Twin",120]
[null,26,"Strain Clamps – Straight type 10-13,5mm",null,null,10]
[null,27,"Midspan Joints -Dino",null,null,35]
[null,28,"Midspan Joints -Zebra",null,null,35]
[null,29,"Midspan Joints - Bersfort",null,null,25]
[null,30,"Midspan Joints –Tern",null,null,35]
[null,31,"Midspan Joints –Goat",null,null,25]
[null,32,"Midspan Joints -Bear",null,null,35]
[null,33,"Midspan Joints -Wolf",null,null,35]
[null,34,"Midspan Joints – Horse",null,null,35]
[null,35,"Midspan Joints - Tiger",null,null,35]
[null,36,"Midspan Joint Compression –Earth wire 13,48mm",null,null,10]
[null,37,"Compression Repair sleeves – Dino (short)",null,null,35]
[null,38,"Compression Repair sleeves- Bersfort",null,null,38]
[null,39,"Compression Repair sleeves - Zebra",null,null,47]
[null,40,"Compression Repair sleeves – Tern",null,null,47]
[null,41,"Compression Repair sleeves – Goat",null,null,38]
[null,42,"Compression Repair sleeves - Bear",null,null,13]
[null,43,"Compression Repair sleeves – Wolf",null,null,27]
[null,44,"Compression Repair sleeves – Horse",null,null,22]
[null,45,"Compression Repair sleeves - Tiger",null,null,35]
[null,46,"Compression Repair  sleeves- IEC315",null,null,50]
[null,47,"Compression Repair  sleeves- IEC560",null,null,50]
[null,48,"Armour Rods/Helical Wraps –Dino - 36mm",null,null,35]
[null,49,"Armour Rods/Helical Wraps - Bersfort",null,null,50]
[null,50,"Armour Rods/Helical Wraps -Zebra",null,null,60]
[null,51,"Armour Rods/Helical Wraps –Tern",null,null,60]
[null,52,"Armour Rods/Helical Wraps –Goat",null,null,50]
[null,53,"Armour Rods/Helical Wraps -Bear",null,null,10]
[null,54,"Armour Rods/Helical Wraps – Wolf",null,null,35]
[null,55,"Armour Rods/Helical Wraps – Horse",null,null,35]
[null,56,"Armour Rods/Helical Wraps - Tiger",null,null,35]
[null,57,"Armour Rods/Helical Wraps - IEC315",null,null,50]
[null,58,"Armour Rods/Helical Wraps - IEC560",null,null,50]
[null,59,"Crosby clamps 19/2,70",null,null,25]
[null,60,"Bird Flight Diverters - Black",null,null,300]
[null,61,"Bird Flight Diverters - White",null,null,75]
[null,62,"Aircraft Warning spheres - Red",null,null,125]
[null,63,"Aircraft warning spheres - White",null,null,100]
[null,64,"Suspension Clamps –  16 – 24mm",null,null,25]
[null,65,"Suspension Clamps –  25 – 40mm",null,null,25]
[null,66,"Suspension Clamps – Earth wire type 11-21mm",null,null,25]
[null,67,"Compression Dead-end Clamp-Dino",null,null,25]
[null,68,"Compression Dead-end Clamp Bersfort",null,null,25]
[null,69,"Compression Dead-end Clamp-Zebra",null,null,25]
[null,70,"Compression Dead-end Clamp-Tern",null,null,25]
[null,71,"Compression Dead-end Clamp-Goat",null,null,25]
[null,72,"Compression Dead-end Clamp-Bear",null,null,25]
[null,73,"Compression Dead-end Clamp-Wolf",null,null,25]
[null,74,"Compression Dead-end Clamp - Horse",null,null,25]
[null,75,"Compression Dead-end Clamp - Tiger",null,null,25]
[null,76,"Compression Dead-end Clamp - Chicadee",null,null,25]
[null,77,"Compression Dead-end Clamp-IEC315",null,null,25]
[null,78,"Compression Dead-end Clamp-IEC560",null,null,25]
[null,79,"Strain Clamps – Straight type 10-13,5mm",null,null,25]
[null,80,"Pistol Grip/Cricket Bat Strain Clamps – 7.95 – 10.50mm",null,null,25]
[null,81,"Pistol Grip Strain/Cricket Bat Clamps – 11.50- 13.50mm",null,null,25]
[null,82,"Triangular yoke for I assembly-210kN-with 450mm spacing",null,null,25]
[null,83,"Rectangular yoke- 450kN with 450mm spacing",null,null,12]
[null,84,"765kv- suspension yoke",null,null,12]
[null,85,"765kv strain yoke-live end",null,null,12]
[null,86,"765kV strain yoke dead end",null,null,12]
[null,87,"Strain triple yoke- 600kN- 450mm spacing for 2x 300kN insulators",null,null,12]
[null,88,"Strain V yoke- 600kN- 450mm spacing for 2x 300kN insulators for dead end to connect to tower-single attachment.",null,null,12]
[null,89,"Strain rectangular yoke- 600kN- 450mm spacing for 2x 300kN insulators for dead end to connect to tower-double attachment.",null,null,25]
[null,90,"Socket Tongues –16mm, 120kN",null,null,25]
[null,91,"Socket Tongues – 20mm, 210kN",null,null,25]
[null,92,"Socket Tongues – 24mm, 300kN",null,null,25]
[null,93,"Socket Tongues – 28mm, 450kN",null,null,25]
[null,94,"Socket Clevis –16mm, 120kN",null,null,25]
[null,95,"Socket Clevis – 20mm, 120kn",null,null,25]
[null,96,"Socket Clevis – 24mm, 300kN",null,null,25]
[null,97,"Socket Clevis – 28mm, 450kN",null,null,25]
[null,98,"Ball Clevis –16mm, 120kN",null,null,25]
[null,99,"Ball Clevis – 20mm, 120kn",null,null,25]
[null,100,"BallClevis – 24mm, 300kN",null,null,25]
[null,101,"Ball Clevis-28mm-450kN",null,null,25]
[null,102,"Ball oval eyes –16mm, 120kN",null,null,25]
[null,103,"Ball oval eyes – 20mm, 120kn",null,null,25]
[null,104,"Balloval eyes – 24mm, 300kN",null,null,25]
[null,105,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin -Dinosaur",null,null,37]
[null,106,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Bersfort",null,null,37]
[null,107,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Zebra",null,null,37]
[null,108,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Tern",null,null,37]
[null,109,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Goat",null,null,37]
[null,110,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Bear",null,null,37]
[null,111,"Conductor Spacers, 570mm Spacing, Helical Wraps Trip -Dinosaur",null,null,2]
[null,112,"Conductor Spacers, 570mm Spacing, Helical Wraps Trip - Bersfort",null,null,2]
[null,113,"Conductor Spacers, 380mm Spacing, Helical Wraps Trip - Zebra",null,null,2]
[null,114,"Conductor Spacers, 450mm Spacing, Helical Wraps Trip - Tern",null,null,2]
[null,115,"Conductor Spacers, 380mm Spacing, Helical Wraps Trip - IEC315",null,null,2]
[null,116,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - Bersfort",null,null,2]
[null,117,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - Zebra",null,null,2]
[null,118,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - Tern",null,null,2]
[null,119,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - IEC560",null,null,2]
[null,120,"Conductor Spacers, 320mm Spacing, Helical Wraps Hex - Tern",null,null,25]
[null,121,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Dinosaur",null,null,25]
[null,122,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Bersfort",null,null,25]
[null,123,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Zebra",null,null,25]
[null,124,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Tern",null,null,25]
[null,125,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - IEC315",null,null,25]
[null,126,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - Bersfort",null,null,125]
[null,127,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - Zebra",null,null,50]
[null,128,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - Tern",null,null,25]
[null,129,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - IEC560",null,null,12.5]
[null,130,"Conductor Spacers, Hex Bolted Rigid Type - 380mm Spacing - Bull",null,null,25]
[null,131,"Shackles-120kN",null,null,25]
[null,132,"Shackles-210kN",null,null,125]
[null,133,"Shackles-300kN",null,null,50]
[null,134,"Shackles-450kN",null,null,1]
[null,135,"Shackles-600kN",null,null,1]
[null,136,"Shackles-900kN",null,null,25]
[null,137,"Adjustable Extension links-min 300mm-210kN",null,null,25]
[null,138,"Adjustable Extension links-min 300mm-450kN",null,null,25]
[null,139,"Chain links- 120kN",null,null,25]
[null,140,"Chain links- 210kN",null,null,50]
[null,141,"Vibration damper - Dinosaur",null,null,50]
[null,142,"Vibration damper - Bersfort",null,null,50]
[null,143,"Vibration damper - Zebra",null,null,50]
[null,144,"Vibration damper - Tern",null,null,50]
[null,145,"Vibration damper - Goat",null,null,50]
[null,146,"Vibration damper - Bear",null,null,50]
[null,147,"Vibration damper - IEC315",null,null,50]
[null,148,"Vibration damper - IEC560",null,null,75]
[null,149,"Vibration damper - 19/2,70",null,null,5]
[null,150,"Tee off Clamps (Tern bolted to Tern Compressed)",null,null,5]
[null,151,"Tee off Clamps (Bersfort bolted to  Bersfort Compressed)"]
[null,152,"Parallel groove clamps (2 Bolts al- al)",null,null,5]
[null,153,"Sag adjuster 210kN",null,null,5]
[null,154,"Sag adjuster 120kN",null,null,75]
[null,155,"Crosby clamps 19/2,70",null,null,260]
[null,156,"Preform repair for steel earth wire",null,null,50]
[null,157,"Preform Repair Aluminum Zambezi Conductor ()",null,null,150]
[null,158,"Repair Sleeves compression Zambezi conductor (Full Tension)",null,null,25]
[null,159,"Repair Sleeves compression Zambezi conductor (Non-Tension)",null,null,25]
[null,160,"Damper Spacers Quad Zambezi conductor",null,null,100]
[null,161,"Conductor Vibration Dampers - Zambezi",null,null,50]
[null,162,"Shield Wire Dampers - 533kV  Oden",null,null,1]
[null,163,"Compression Dead-end Clamp- Oden",null,null,50]
[null,164,"Compression Dead-end Clamp- Zambezi",null,null,1]
[null,165,"Midspan Joints -Oden",null,null,125]
[null,166,"Midspan Joints -Zambezi",null,null,125]
[null,167,"Midspan Joint Compression – Earth wire 17.80mm",null,null,25]
[null,168,"Compression Repair sleeves – Oden (short)",null,null,25]
[null,169,"Compression Repair sleeves- Zambezi (Long)",null,null,125]
[null,170,"Armour Rods/Helical Wraps – Oden",null,null,250]
[null,171,"Armour Rods/Helical Wraps - Zambezi",null,null,250]
[null,172,"Socket Tongues –16mm, 120kN",null,null,125]
[null,173,"Ball Clevis –16mm, 120kN",null,null,1]
[null,174,"Conductor Spacers, 380mm Spacing, Helical  Quad - Zambezi",null,null,250]
[null,175,"Earth wire  Full Tension joints ",null,null,100]
[null,176,"Vibration Dampers - Shieldwire",null,null,250]
[null,177,"Suspension Clamps ",null,null,50]
[null,178,"Strain Clamps – Straight type 10-13,5mm",null,null,250]
[null,179,"Yoke Plates- triangle, trapezoidal, service, Y and Vee types",null,null,1]
[null,180,"I assembly triple yoke -450mm spacing-210kN",null,null,25]
[null,181,"V assembly triple yoke-450mm spacing-210kN",null,null,25]
[null,"TOTAL COMPONENTS"]

{"sheet":"Assemblies  ","index":2,"n_rows":70,"n_cols":7,"rows_kept":70,"merged":[[69,1,69,5]]}
[]
[null,"132kV to 765kV ASSEMBLIES AND EARTH WIRE"]
[null,"ITEM ","ITEM DESCRIPTION","Conductor\neg Tern, Wolf, Bear","Configuration\nTwin/Trip\nQuad/Hex","QTY","Link CPA"]
[null,null,"132kV Assemblies "]
[null,1,"\"V\" Suspension assembly","Bear","Twin",{"v":1.5,"d":"2"},"eg: A"]
[null,2,"Strain Assembly","Bear","Twin",12]
[null,3,"Vibration damper","Bear","Twin",60]
[null,4,"Strain Assembly - Single attachment","Chicadee","Single",{"v":0.5,"d":"1"}]
[null,5,"\"I\" Suspension Assembly ","Tern","Trip",51]
[null,6,"\"V\" Suspension assembly","Tern","Trip",87]
[null,7,"Strain assembly-double attachment","Tern","Trip",583]
[null,8,"\"I\" Suspension Assembly ","Zebra","Single",25]
[null,9,"Cushion Grip Suspension clamp for Suspension assemblies","Zebra","Single",111]
[null,10,"Strain Assemblies for Phase Conductor (Twr 7618)","Zebra","Single",10]
[null,11,"Strain Assembly - Single attachment","Zebra","Single",25]
[null,null,"275kV Assemblies ",null,null,0]
[null,12,"\"V\" Suspension assembly","Tern","Quad",{"v":13.5,"d":"14"}]
[null,13,"Strain assembly-double attachment","Tern","Quad",60]
[null,14,"\"I\" Suspension Assembly ","Tern","Twin",48]
[null,15,"\"V\" Suspension assembly","Tern","Twin",36]
[null,16,"Strain assembly-double attachment","Tern","Twin",96]
[null,17,"\"V\" Suspension assembly","Zebra","Quad",9]
[null,18,"Strain assembly-double attachment","Zebra","Quad",30]
[null,null,"400kV Assemblies ",null,null,0]
[null,19,"\"I\" Suspension Assembly ","Bersfort","Trip",{"v":301.5,"d":"302"}]
[null,20,"\"I\" Suspension Assembly ","Dinosaur","Twin",3]
[null,21,"\"I\" Suspension Assembly ","IEC315","Trip",3927]
[null,22,"\"I\" Suspension Assembly ","Tern","Quad",192]
[null,23,"\"I\" Suspension Assembly ","Tern","Trip",1839]
[null,24,"\"I\" Suspension Assembly ","Wolf","Quad",3]
[null,25,"\"V\" Suspension assembly","Bersfort","Trip",{"v":127.5,"d":"128"}]
[null,26,"\"V\" Suspension assembly","Dinosaur","Trip",{"v":28.5,"d":"29"}]
[null,27,"\"V\" Suspension assembly","Goat","Twin",42]
[null,28,"\"V\" Suspension assembly","IEC315","Trip",1407]
[null,29,"\"V\" Suspension assembly (518 TOWER)","IEC560","Quad",{"v":142.5,"d":"143"}]
[null,30,"\"V\" Suspension assembly","Kingbird","Trip",3]
[null,31,"\"V\" Suspension assembly","Tern","Quad",{"v":308.5,"d":"309"}]
[null,32,"\"V\" Suspension assembly","Tern","Trip",{"v":841.5,"d":"842"}]
[null,33,"\"V\" Suspension assembly","Wolf","Quad",3]
[null,34,"\"V\" Suspension assembly","Zebra","Quad",{"v":1.5,"d":"2"}]
[null,35,"Strain assembly-double attachment","Bersfort","Trip",324]
[null,36,"Strain assembly-double attachment","Dinosaur","Trip",126]
[null,37,"Strain assembly-double attachment","Goat","Twin",126]
[null,38,"Strain assembly-double attachment","IEC315","Trip",2436]
[null,39,"Strain assembly-double attachment","IEC560","Quad",432]
[null,40,"Strain assembly-double attachment","Kingbird","Trip",24]
[null,41,"Strain assembly-double attachment","Tern","Quad",939]
[null,42,"Strain assembly-double attachment","Tern","Trip",2010]
[null,43,"Strain assembly-double attachment","Wolf","Quad",12]
[{"$nulls":5},0]
[null,null,"765kV Assemblies ",null,null,0]
[null,56,"\"V\" Suspension assembly","Tern","Hex",{"v":9007.5,"d":"9008"}]
[null,57,"Strain assembly-double attachment","Tern","Hex",4602]
[null,58,"Bolted slack span assembly","Tern","Hex",2]
[null,null,"Earthwire",null,null,0]
[null,59,"EW non-insulated suspension assembly","19/2,70","N/A",185]
[null,60,"EW insulated strain assembly","19/2,70","N/A",7]
[null,61,"EW non-insulated strain assembly","19/2,70","N/A",{"v":35.5,"d":"36"}]
[null,62,"EW insulated suspension assembly","19/2,70","N/A",4]
[null,63,"EW insulated suspension assembly","Panther","N/A",{"v":2.5,"d":"3"}]
[null,64,"EW insulated suspension assembly","Horse","N/A",{"v":1.5,"d":"2"}]
[null,65,"EW non-insulated suspension assembly","Panther","N/A",8]
[null,66,"EW non-insulated suspension assembly","Horse","N/A",{"v":2.5,"d":"3"}]
[null,67,"EW insulated strain assembly","Panther","N/A",{"v":76.5,"d":"77"}]
[null,68,"EW insulated strain assembly","Horse","N/A",5]
[null,69,"EW non-insulated strain assembly","Panther","N/A",81]
[null,70,"EW non-insulated strain assembly","Horse","N/A",{"v":16.5,"d":"17"}]
[null,71,"EW insulated cross rope assembly","Horse","N/A",{"v":7.5,"d":"8"}]
[null,72,"EW non-insulated cross rope assembly","Horse","N/A",{"v":124.5,"d":"125"}]
[null,"TOTAL ASSEMBLIES"]

{"sheet":"CPA Formula","index":3,"n_rows":79,"n_cols":8,"rows_kept":79,"merged":[[8,0,14,0],[16,0,22,0],[26,0,32,0],[35,0,41,0],[44,0,50,0],[53,0,59,0],[62,0,68,0],[72,0,78,0]]}
[]
["ENQUIRY N0. E1396NTCSAMWP"]
["TENDERER NAME: "]
["Name of Enquiry: The design, manufacture, testing, supply and delievy of Line Hardware on an “as and when” required basis for a period of 5 (five) years for Transmission Division."]
["PRICE ADJUSTMENT FOR INFLATION"]
["FORMULAE DETAILS"]
[]
["Description","CPA No.","Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["132kV kV assemblies",null,"a"]
[null,"\"001","b"]
[null,"\"001","c"]
[null,"\"001","d"]
[null,"\"001","e"]
[null,"\"001","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
[{"$nulls":3},{"v":0.15,"d":"0.150"},"Total (1.00)"]
["Description","CPA No.","Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["275kV assemblies",null,"a"]
[null,"002","b"]
[null,"002","c"]
[null,"002","d"]
[null,"002","e"]
[null,"002","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
[{"$nulls":3},{"v":0.15,"d":"0.150"},"Total (1.00)"]
[]
[]
["Description",null,"Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["400kV assemblies",null,"a"]
["Description of formula 2","003","b"]
["Description of formula 2","003","c"]
["Description of formula 2","003","d"]
["Description of formula 2","003","e"]
["Description of formula 2","003","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
["Description of formula 2",null,null,{"v":0.15,"d":"0.150"},"Total (1.00)"]
[]
["Description",null,"Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["765kV Assemblies",null,"a"]
["Description of formula 2","004","b"]
["Description of formula 2","004","c"]
["Description of formula 2","004","d"]
["Description of formula 2","004","e"]
["Description of formula 2","004","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
["Description of formula 2","004",null,{"v":0.15,"d":"0.150"},"Total (1.00)"]
[]
["Description",null,"Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["Earthwire","005","a"]
["Description of formula 2","005","b"]
["Description of formula 2","005","c"]
["Description of formula 2","005","d"]
["Description of formula 2","005","e"]
["Description of formula 2","005","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
["Description of formula 2",null,null,{"v":0.15,"d":"0.150"},"Total (1.00)"]
[]
["Description",null,"Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["Other Components ","006","a"]
["Description of formula 2","006","b"]
["Description of formula 2","006","c"]
["Description of formula 2","006","d"]
["Description of formula 2","006","e"]
["Description of formula 2","006","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
["Description of formula 2",null,null,{"v":0.15,"d":"0.150"},"Total (1.00)"]
[]
["Description",null,"Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["Other Components\n","007","a"]
["Description of formula 2","007","b"]
["Description of formula 2","007","c"]
["Description of formula 2","007","d"]
["Description of formula 2","007","e"]
["Description of formula 2","007","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
["Description of formula 2",null,null,{"v":0.15,"d":"0.150"},"Total (1.00)"]
[]
[]
["Description",null,"Index","Proportion / Coefficient / Weight / Base reference price","Scope of Index (eg Labour)","Title/Definition : Linked to the index, e.g., Table C3, All hourly paid employees.  Must be completely defined","Source of Index ","Base month if not Base Date as defined (See Note vi)"]
["Other Components\n","007","a"]
["Description of formula 2","007","b"]
["Description of formula 2","007","c"]
["Description of formula 2","007","d"]
["Description of formula 2","007","e"]
["Description of formula 2","007","f",{"v":0.15,"d":"0.150"},"Fixed Non-adjustable (0.15 minimum)"]
["Description of formula 2",null,null,{"v":0.15,"d":"0.150"},"Total (1.00)"]

{"sheet":"T & O ","index":4,"n_rows":32,"n_cols":12,"rows_kept":32,"merged":[[5,1,6,4],[5,5,6,11],[7,1,8,4],[7,5,8,11],[9,1,10,4],[9,5,10,11],[11,1,13,1],[11,2,11,11],[12,2,12,11],[13,2,13,11]]}
[]
[]
[null,"Transport and Off-loading "]
[]
[]
[null," ENQUIRY NO",{"$nulls":3},{"$f":"'[41]Cover Page'!C12","v":0}]
[]
[null,"COMMODITY",{"$nulls":3},{"$f":"'[41]Cover Page'!C14","v":0}]
[]
[null,"SUPPLIER",{"$nulls":3},{"$f":"'[41]Cover Page'!C16","v":0}]
[]
[null,"DISTANCE WITHIN A GIVEN RADIUS","PER UNIT PRICE IN SOUTH AFRICAN CURRENCY EXCLUDING VAT"]
[null,null,"TRANSPORT TO SITE OR GRID STORE"]
[null,null,"NUMBER OF UNITS TO BE TRANSPORTED DURING ONE SITE VISIT"]
[null,null,1,2,3,4,5,6,"7 to 9","10 to 12","13 to 18","19 or more"]
[null,"0 - 100"]
[null,"101 - 200"]
[null,"201 - 300"]
[null,"301 - 400"]
[null,"401 - 500"]
[null,"501 - 600"]
[null,"601 - 700"]
[null,"701 - 800"]
[null,"801 - 900"]
[null,"901 - 1000"]
[null,"1001 - 1100"]
[null,"1101 - 1200"]
[null,"1201 - 1300"]
[null,"1301 - 1400"]
[null,"1401 - 1500"]
[]
[null,"ADDITIONAL NOTES:"]