{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["PRICING SCHEDUL"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PRICING SCHEDUL","index":0,"n_rows":141,"n_cols":17,"rows_kept":141,"merged":[[0,0,1,0],[3,7,3,8],[3,11,3,12],[4,7,4,8],[4,11,4,12],[18,1,18,2],[21,0,21,8],[33,1,33,8],[85,1,85,8],[92,0,92,2],[101,1,101,2],[104,1,104,2],[105,1,105,8],[107,1,107,2],[110,1,110,2],[113,1,113,2],[115,1,115,8],[117,1,117,2],[118,1,118,2],[119,1,119,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[131,1,131,8],[133,1,133,2],[136,1,136,2],[138,0,138,1]],"flags":["formulas_cached_only"]}
[]
[null,"DISTRIBUTION AND STREETLIGHT POLES"]
[]
["ITEM","DESCRIPTION ","SPECIFY","SPECIFY","MANUFACTURERS","ISO 9001","MINIMUM","   PRICE PER UNIT",null,"EVALUATION","POINTS",null,null,"POINTS",null,"BID","DELIVERY IN"]
["NO","AS","DESIGNED","ACTUAL","NAME","COMPLIANT","QUANTITY","  FOR  RUSTENBURG",null,"BID","Price",null,null,"HDI","15%","PRICE","RUSTENBURG"]
[null,"SPECIFIED","KN","LENGTH",null,"YES / NO","PER TRUCK","UNIT","PRICE","PRICE","Np","BBEEE","BBEEE","Nep","VAT","(VAT INCLUDED)","(PERIOD IN)"]
[null,null,"COMPULSORY","COMPULSORY",null,null,"DELIVERY","EACH","EXCL VAT",null,null,"LOC","POINTS",{"$nulls":3},"(WEEKS)"]
[{"$nulls":10},90,null,"10"]
["DISTRIBUTION POLES : STEEL (GUIDE DRAWINGS 122/314/093 & /106)"]
[]
[1,"7.55 M : 2.4 kN GALVANIZED",{"$nulls":5},"EACH"]
[]
[2,"9.25 M : 2.4 kN GALVANIZED",{"$nulls":5},"EACH"]
[]
[3,"9.75 M : 2.6 kN GALVANIZED",{"$nulls":5},"EACH"]
[]
[4,"10.6 M : 2.8 kN GALVANIZED",{"$nulls":5},"EACH"]
[]
[5,"13.6 M : 3.0 kN (min) GALVANIZED (ROAD CROSSINGS)",{"$nulls":5},"EACH"]
[]
[]
["SPUN DISTRIBUTION POLES : CONCRETE (LITTLE SLEEVE + CLOSE TOP)"]
[]
[6,"7.5 M POLE WITH 130 mm DIA TOP   2.5 kN",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},{"$error":"#REF!"},3,8,{"$error":"#REF!"}]
[]
[{"$nulls":9},{"v":4551.7,"d":"4,551.70"}]
[7,"9.0 M POLE WITH 130 mm DIA TOP  5.5 kN",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[{"$nulls":9},5196.85]
[8,"10 M POLE WITH 130 mm DIA TOP   5.5 kN",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[{"$nulls":9},6266.35]
[9,"11 M POLE WITH 130 mm DIA TOP   8,5 kN",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[{"$nulls":9},{"v":7820,"d":"7,820.00"}]
[10,"12 M POLE WITH 130 mm DIA TOP   8,5 kN",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[11,"22 M POLE FOR 132KV DISTRIBUTION   ___ Kn",{"$nulls":5},"EACH"]
[]
["H - DISTRIBUTION POLES : CONCRETE "]
[]
[12,"7.5 M POLE",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},{"$error":"#REF!"},3,8,{"$error":"#REF!"}]
[]
[{"$nulls":9},2530]
[13,"9 M POLE",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[14,"10 M POLE",{"$nulls":5},"EACH"]
[]
[{"$nulls":9},{"v":4371.4,"d":"4,371.40"}]
[15,"11 M POLE",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[{"$nulls":9},{"v":7645,"d":"7,645.00"}]
[16,"12 M POLE",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[{"$nulls":9},{"v":7645,"d":"7,645.00"}]
[17,"13.6 M POLE",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[18,"22 M POLE FOR 132KV DISTRIBUTION   ___ kN"]
[]
["DISTRIBUTION POLES : TREATED WOOD"]
[]
[19,"8 M POLE"]
[]
[]
[20,"9 M POLE"]
[]
[]
[21,"10 M POLE"]
[]
[]
[22,"11 M POLE"]
[]
[]
[23,"12 M POLE"]
[]
[]
[25,"13 M POLE"]
[]
[]
["STREETLIGHT POLES : CONCRETE"]
[]
[26,"7,5 M WITH 130 MM TOP  2,5 kN",{"$nulls":5},"EACH",null,{"v":3294.75,"d":"3,294.75"}]
[]
[]
[27,"10 M WITH 130 MM TOP 5,5 kN",{"$nulls":5},"EACH",null,{"v":5196.85,"d":"5,196.85"}]
[]
[]
[28,"4.6 M FOR POST TOP LANTERN ",{"$nulls":5},"EACH"]
[]
["STREETLIGHT BRACKETS   (DRAWING BD3 18B)"]
[]
[29,"CONE INNER DIAMETER :  152 MM X 1.830 M",{"$nulls":5},"EACH"]
[]
[]
[30,"CONE INNER DIAMETER :  1.35 MM X 1.830 M",{"$nulls":5},"EACH"]
[]
[]
[{"$nulls":9},{"v":338,"d":"338.00"}]
[31,"CONE INNER DIAMETER :  152 MM X 0.2M X 15 DEGREES",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[32,"CONE INNER DIAMETER :  152 MM X 1 M X 15 DEGREES",{"$nulls":5},"EACH",null,{"v":439,"d":"439.00"}]
[]
[{"$nulls":9},{"v":302,"d":"302.00"}]
[33,"CONE INNER DIAMETER : 135 MM X 0.2M X 15 DEGREES",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},{"$error":"#REF!"},3,8,{"$error":"#REF!"}]
[]
[{"$nulls":9},{"v":387,"d":"387.00"}]
[34,"CONE INNER DIAMETER : 135 MM X 1M X 15 DEGREES",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[{"$nulls":9},{"v":387,"d":"387.00"}]
[35,"CONE INNER DIAMETER : 135 MM X 1M X 15 DEGREES",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[]
[36,"11.5 M STEPPED POLE WITH SINGLE  SPIGOT OF 1 M"]
[null,"11.5m pole - 10m MH (planting depth = 1.5m)",{"$nulls":7},{"v":2800,"d":"2,800.00"}]
[null,"(BOTTOM DIAMETER = 127 MM) (TOP DIAMETER = 76 MM)",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[37,"13.7 M X 11.5 M STEPPED POLE WITH SINGLE  SPIGOT OF 2 M"]
[null,"13.7m pole - 12m Mounting Height - (planting depth = 1.7m)",{"$nulls":7},{"v":3625,"d":"3,625.00"}]
[null,"(BOTTOM DIAMETER = 139 MM) (TOP DIAMETER = 76 MM)",{"$nulls":5},"EACH",null,{"v":0,"d":"0.00"},180,3,8,{"v":188,"d":"188.00"}]
[]
[]
[38,"13.7 M STEPPED POLE WITH DOUBLE SPIGOT OF 2 M"]
[null,"13.7m pole - 12m Mounting Height - (planting depth = 1.7m)"]
[null,"(BOTTOM DIAMETER = 139 MM) (TOP DIAMETER = 76 MM)",{"$nulls":5},"EACH",null,{"v":4110,"d":"4,110.00"}]
[]
[]
[]
[39,"DOUBLE  SPIGOT OF 3 M (TO FIT 76 MM POLE TOP)",{"$nulls":5},"EACH"]
[]
[]
[40,"DOUBLE  SPIGOT OF 1 M (TO FIT 76 MM POLE TOP)",{"$nulls":5},"EACH"]
[]
["30 METER HIGHMAST DISTRIBUTION BOARD"]
[]
[41,"HIGHMAST - IP STANDARD INTERNAL DISTRIBUTION BOARD (5 PIN, 16 AMP)",{"$nulls":5},"EACH"]