SPECIFICATION FOR WATER DISTILLER

Water distiller
· fully automatic operation
· supplier to quote on 4l/hr and 8l/hr models
· over temperature protector
· water float level sensor
· low water supply cut-off
· stainless steel boiling chamber
· stainless steel storage tank
· reservoir tank
· pre-filter and cartridge
· ease of maintenance, availability of spares
quote to include supply and installation
