1. [bookmark: _GoBack]SPECIFICATION FOR TRALIER FOR THE NURSERY

Tractor tipper trailer flatbed
· 5 ton trailer
· Single axil
· Load body thickness- 4mm +
· Load body size (approximate size) – 1.9m (width) x 3.4m (length)
· Drop side at ± 400mm
· Tyres 10.5/80-15.3
· Mechanical parking brake
· 4 phase telescopic cylinder
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