Specifications for the potato harvester

Supply and delivery of Small Potato harvester
Small Potato harvester to be used for sweet potatoes
Must be operated by a normal size tractor for example a Landini 8865
Working width 900-1000 cm
Working depth minimum 30 cm
Built strong to be able to work in heavy clay soil
To be connected to the 3 point system of the tractor
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