Questions and Answers for Contract No: 30849(5W); 30850(5W); 30851(5W) & 30852 (5W)

Question 1:
1. With regards to item PS-16 on page 83 of the above-mentioned tender documents, we notice that pre and post flow logging is required per zone as per the image below. We don’t see it listed as a line item on the BOQ for any of the tenders. Kindly advise how we should accommodate for this?
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1. What are the % limits of subcontracting of the total value of works for these contracts?

Answer:

Please see screenshot of PS-16 which is accounted for in the BOQ. (Pg 66) Tenderer should price according to their consideration of the project.
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Please see % for Subcontracting (Pg 61)
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Question 2:
On page 64 of each of the above documents, under item 2.2, its shows FOUR, but in brackets (5) directly after. Kindly advise on which number is to be used?
I’ve attached a screenshot below for reference purposes.
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Answer: 
The correct value is FOUR (4).



Question 3

Could you kindly advise if you are looking for a service provider for tender number 30849- 5W that has both 5CE and CO, or any between the two? 

Answer:
The service provider is required to have both 5CE and SO as the project requires expertise of both Civil Engineering and Plumbing works. 
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PS-16

Progress reporting per Reservoir Zone in line
with Leak Detection Surveys completed

Allow the following additional items which the
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CONTRACTOR PARTICIPATION GOAL (CPG)

Itis a condition of contract that the contractor must allow for a minimum of 30% of the contract
value (excluding PC Sum items and Fixed Cost allowances) to be subcontracted to contractors
who are >51% PPG (Priority Population Group) owned. Proof of payment to the subcontractors
will be required to verfy that the minimum has been achieved

The penalty for not achieving the specified CPG will be 0.5% of the contract value (excluding PC
Sum items and Fixed Cost allowances) for every 1% of CPG not achieved.
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Supply the services of Four (5) Qualfied
plumbers with a minimum of 5 years with an

extensive knowledge of industrial plumbing
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PS-16 PROGRESS REPORTING PER RESERVIOR ZONE INLINE WITH LD SURVEYS

In addition to the above reporting requirements, the Contractor is required to carry out the following activities
monthly per reservoir zone in which leak detection surveys are to be conducted:

«  Pre logging of the reservoir to establish a bench mark of the night losses
«  Complete leak detection survey of the reservoir zone

« Postlogging of the reservoir to establish impact/saving/reduction in losses





