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SOUTH AFRICAN REVENUE SERVICES

SARS Procurement Centre

	



	 REQUEST TO SUBMIT QUOTATIONS FOR THE REQUIREMENTS OF THE SOUTH AFRICAN REVENUE SERVICES

	RFQ NUMBER
	RFX 6000022329

	DESCRIPTION OF GOODS/ SERVICES
	Supply, deliver and install signages to Northern Cape 

	PUBLISH/

ADVERTISEMENT DATE
	13 June 2023

	CLOSING DATE

& TIME
	21 June 2024
At 11h00

	COMPULSORY REQUIREMENTS
	
	Tick Applicable box

	
	Acceptance of SARS conditions as well as submission of a quotation.
	

	
	Valid and original Tax Clearance Certificate  
	

	
	Valid and original or certified copy of BEE Certificate or Approval letter from the IRBA Registered Auditor.
	

	
	Complete SBD 1
	

	
	Complete SBD 4
	

	
	Complete SBD 6.1
	

	
	Complete Oath of Secrecy
	

	
	Mandatory registrations (i.e. CIDB)
	

	COMPULSORY BRIEFING  SESSION/ SITE MEETING
	NO

	ENQUIRIES
	Enquiries must be addressed to: Proc.queries@sars.gov.za

	QUOTE VALIDITY
	60 Days (commencing from the RFQ closing date)

	SUBMISSION:
	Proposals clearly marked with the RFQ number and description, must be submitted to the following email address:

e-mail: Proc.responses@sars.gov.za

	DELIVERY ADDRESS WHERE GOODS/ SERVICES/ WORKS ARE REQUIRED
	SARS – Northern Cape
Vooilsdrift Border Post and delivery at Ancorley building, Upington 
 


REQUIRED SERVICES

SARS would like to appoint a service provider to supply, deliver and install the following services: .
1. 2 x meeting rooms (only the word meeting room to be printed on signage)
a. Frame – Approved “similar or equal to” clear anodized Vista V215 x 250mm (h) profile, double sided with anodized aluminium end caps to match. Colour – pantone 2955c text / stripes. White vinyl substrate. Humanist 521BT or verdana. 2100mm AFFL to U/S frame. These will be required wall mounted (flat) and/or projecting. 
2. 2 x male toilets 

a. Wall mounted at entrance to toilet (projecting). Frame – Vista V150 x 150mm (h) light weight double sided new generation profile, with anodized aluminium end caps to match. Colour black pictogram. Pantone 2955 c strips (blue). 2100mm AFFL to U/S frame 
3. 2 x female toilets 

a. Projecting (wall mounted) at entrance to toilet. Frame Vista V150 x 150mm (h) light weight new generation profile, double sided with anodized aluminium end caps to match. Colour black pictogram. Pantone 2955 c strips (blue). 2100mm AFFL to U/S frame 
4. 4 x counter signage (2 x signages indicating numbers 1 until 2) to be hanged at various at Imports and Exportation counters 
a. Typical double sided single slat curved face “Counter XX” where “XX” is the counter number. Vista new generation 2 x clear anodized V150 x 900mm (cut to size) low weight profiles, with Vista aluminium end caps to match V150 profile. Rigid vista hanging system. Pantone 2955c logo and text on series 5 Avery 546 Gloss sliver high performance vinyl. Font – Verdana bold. 80mm high. 35mm gap top and bottom for text. 25mm gap top and bottom logo. Suspended 2200mm AFFL to U/S frame (typical) or 120mm below bulkhead or ceiling or against the wall above the window 
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Location: As per space plan.

Description: Typical double sided, single slat “Counter X” directional hanging
sign from Vista V150 lightweight new generation profiles. Rigid
Vista hanging system.
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5. To supply and deliver 2 x Airport signage (ports of entry) – Declaration signs to be manufactured as per pic indicated below (pull up banner 2200mmx850mm
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6. To supply and fit 4 x SARS CUSTOMS inspection signage at Border Post at inspection bay for Exports and Imports.  Tinted wrapped paper with SARS logo. See specification itemized 9.6 in pic below. To supply and fit for both two sides of double entrance doors at Customs building (Exports and Imports)
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7. To supply and fit SARS CUSTOMS signage to front of the building. 1000mm wide SARS brushed aluminium sign mounted on wall. See technical data specification to be provided.
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8.   Supply flat sheets gift wrapping size 1000mm x 700mm – quantity 4 for the Scanner room at the port
a. SARS logo printed in solid white pantone

b. SARS printed spot UV varnish ontop of white pantone white (Same plate)

c. Printed on paper stock (Curious metalics lustre 120g/sq mtr) 
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9. Supply and install SARS Customs Cargo Scanner signage. Height, frame and details specification to be provided on separate attachment.
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10. Supply and install 2 x disclaimer and pictogram signage ( 1 x Nakop border post and 1 x for Vooilsdrift border post). Details specification provided separately.
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The following frames to be delivered to Ancorley building, Upington 

11. 20 x aluminium (matt silver anodised) finish poster frame to suit A2 prints (portrait and landscape) 

12. 60 x aluminium (matt silver anodised) finish poster frame to suit A4 prints (portrait and landscape) 

13. 10  x aluminium (matt silver anodised) finish poster frame to suit A1 prints (portrait and landscape) 

a. Clip frame to closed position

b. 25mm snap frame with open position

c. Remove protective cover 

d. Frame to have poster backing material (firm and not flimsy)
e. Curved face to frame surround (not flat) 
f. Clear 2mm acetate sheet for poster cover
14. 90mtr x Strong 3M double sided tape to secure frames (in rolls of 30mtr each)
Notes:
· Cost to include labour, materials, transport, etc. 
· Work to be done during working hours 
· Price to include components required to secure the signages 
· Upon receipt of purchase order schedule to be provided indicating dates for the office
Bidding Structure

I/We, the undersigned, hereby acknowledge myself/ourselves fully conversant with the details and conditions set out in the Conditions of Bid General Conditions of Contract, Special Conditions, Technical Information and Specifications attached, and hereby agree to supply, render services or perform works in accordance therewith:
	BIDDER’S DETAILS

	NAME of Company/

Close Corporation or Partnership or

Sole Proprietor/Individual 
	____________________________________________(legal name) 

trading as________________________________________

	Company/Close Corporation Registration Number
	

	SARS Vendor Registration Number
	

	Postal Address
	Postal Code __________

	Physical Address
	Postal Code __________

	Contact Details of the Person Representing the Vendor
	Name: _______________________________________________

Telephone: ( ____ ) _____________ Fax: ( ____ ) _____________

Cell phone: ___________________________________________

E-mail address: ________________________________________

	Income Tax Number
	

	VAT Reference Number
	


ANNEXURE 1
Returnable Schedule: Price Schedule

	ITEM
	D E S C R I P T I O N
	UNIT
	QUANTITY
	RATE
	PRICE (Rands)

	
	Vooilsdrift border post (transport and labour to be included in cost below)
	
	
	
	

	1
	Supply and install meeting rooms signages. Detail specification provided on page 2 
	Item
	2
	
	

	2
	Supply and install male toilet signages. Detail specification provided on page 2 

	Item
	2
	
	

	3
	Supply and install female toilet signages. Detail specification provided on page 2. 
	Item
	2
	
	

	4
	Supply and install counter signages (2 x indicated counter 1 and 2 x counter 2). Details specification provided on page 2 
	Item
	4
	
	

	5
	Supply and deliver airport signages required at the port. Measurements and height provided on page 2 
	Item
	2
	
	

	6
	Supply and fit Customs inspection signages required at Exports and Imports. Detail specification provided on page 2
	Item
	4
	
	

	7
	Supply and fit Customs signage at border post. Specification to be provided 
	Item
	1
	
	

	8
	Supply flat sheet gift wrapping for Vooilsdrift border post. Details provided on page 2 
	Item
	4
	
	

	9
	Supply and install SARS Customs Scanner signage. Details specification provided separately. 
	Item 
	1
	
	

	10
	Supply and install disclaimer and pictogram signage in Vooilsdrift and Nakop border post. 1 x at each border post 
	Item 
	2
	
	

	
	Frames to be delivered to Ancorley building, Upington (delivery cost to be included)
	
	
	
	

	11
	Aluminium (matt silver anodised) finish poster frame to suit A2 prints
	Items
	20
	
	

	12
	Aluminium (matt silver anodised) finish poster frame to suit A4 prints
	Item
	60
	
	

	13
	Aluminium (matt silver anodised) finish poster frame to suit A1 prints
	Item 
	10
	
	

	14
	(Scotch guard) Strong Double sided tape required for all snapper frames 
	Mtr 
	90
	
	

	
TOTAL PRICE (INCL. VAT) CARRIED FORWARD TO FORM OF OFFER
	R


Kindly indicate delivery period in days on your quotation
All quotations must also be submitted on a formal company letterhead
Quotation to include during working hours. 

Tansport and labour to be included in final amount (INCL. VAT)
RFX 6000022329 Supply, deliver and install signages to Northern Cape
Page 2 of 4
RFX 6000022221 Supply, deliver and install signages to Northern Cape
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