{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["0013 PRICE SCHEDULE"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"0013 PRICE SCHEDULE","index":0,"n_rows":114,"n_cols":13,"rows_kept":114,"merged":[[1,7,1,8],[2,7,2,8],[59,1,59,5],[79,1,79,8],[94,1,94,8],[101,1,101,4],[107,1,107,4]],"flags":["formulas_cached_only"]}
[null,"DISTRIBUTION AND STREETLIGHT POLES"]
["ITEM","DESCRIPTION ","SPECIFY","SPECIFY","MANUFACTURERS","ISO 9001","MINIMUM","   PRICE PER UNIT",null,null,"BID","DELIVERY IN"]
["NO","AS","DESIGNED","ACTUAL","NAME","COMPLIANT","QUANTITY","  FOR  RUSTENBURG",null,"15%","PRICE","RUSTENBURG"]
[null,"SPECIFIED","KN","LENGTH",null,"YES / NO","PER TRUCK",null,null,"VAT","(VAT )","(PERIOD IN)"]
[null,null,"COMPULSORY","COMPULSORY",null,null,"DELIVERY","UNIT","PRICE",null,"INCLUDED","(WEEKS)"]
[{"$nulls":6},"COMPULSORY","EACH","EXCL VAT"]
[null,"DISTRIBUTION POLES : STEEL (GUIDE DRAWINGS 122/314/093 & /106)"]
[1,"7.55 M : 2.4 kN GALVANIZED (OR SIMILAR)",{"$nulls":5},"EACH",{"$nulls":4},"N/A"]
[]
[2,"9.25 M : 2.4 kN GALVANIZED (OR SIMILAR)",{"$nulls":5},"EACH",{"$nulls":4},"468035"]
[]
[3,"9.75 M : 2.6 kN GALVANIZED (OR SIMILAR)",{"$nulls":5},"EACH",{"$nulls":4},"468040"]
[]
[4,"10.6 M : 2.8 kN GALVANIZED (OR SIMILAR)",{"$nulls":5},"EACH",{"$nulls":4},"468030"]
[]
[5,"13.6 M : 3.0 kN GALVANIZED (ROAD CROSSINGS) (OR SIMILAR)",{"$nulls":5},"EACH",{"$nulls":4},"N/A"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"SPUN DISTRIBUTION POLES : CONCRETE (LITTLE SLEEVE + CLOSE TOP)"]
[6,"7.5 M POLE WITH 130 mm DIA TOP   2.5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468010"]
[]
[7,"9.0 M POLE WITH 130 mm DIA TOP  5.5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468015"]
[]
[8,"10 M POLE WITH 130 mm DIA TOP   5.5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468011"]
[]
[9,"11 M POLE WITH 130 mm DIA TOP   8,5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468016"]
[]
[10,"12 M POLE WITH 130 mm DIA TOP   8,5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468021"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"H - DISTRIBUTION POLES : CONCRETE "]
[11,"7 M POLE  WITH 100 X 120 mm TOP   4 kN",{"$nulls":5},"EACH",{"$nulls":4},"N/A"]
[]
[12,"9 M POLE WITH 100 X 160 mm TOP   7 kN",{"$nulls":5},"EACH",{"$nulls":4},"468003"]
[]
[13,"11 M POLE WITH 130 X 180 mm TOP   8 kN",{"$nulls":5},"EACH",{"$nulls":4},"N/A"]
[]
[14,"13 M POLE WITH 160 X 250 mm TOP   10 kN",{"$nulls":5},"EACH",{"$nulls":4},"468004"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[{"$nulls":12},"NONE"]
[]
[null,"STREETLIGHT POLES : STEEL (GUIDE DRAWINGS 122/212/075 & /128 & /085)"]
[]
[15,"4.6 M STEEL STEEL POLE : GALVANISED ",{"$nulls":5},"EACH",{"$nulls":4},"468025"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"STREETLIGHT POLES : CONCRETE"]
[16,"7,5 M WITH 130 MM TOP  2,5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468010"]
[]
[17,"10 M WITH 130 MM TOP 5,5 kN",{"$nulls":5},"EACH",{"$nulls":4},"468012"]
[]
[18,"4.6 M FOR POST TOP LANTERN ",{"$nulls":5},"EACH",{"$nulls":4},"468005"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"STREETLIGHT BRACKETS   (DRAWING BD3 18B)"]
[19,"CONE INNER DIAMETER :  152 MM X 1.830 M",{"$nulls":5},"EACH",{"$nulls":4},"364010"]
[]
[20,"CONE INNER DIAMETER :  1.35 MM X 1.830 M",{"$nulls":5},"EACH",{"$nulls":4},"NONE"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"STREETLIGHT BRACKETS - SPIGOT (DRAWING BD3 18E)"]
[21,"CONE INNER DIAMETER :  152 MM X 0.2M X 15 DEGREES",{"$nulls":5},"EACH",{"$nulls":4},"364015"]
[]
[22,"CONE INNER DIAMETER :  152 MM X 1 M X 15 DEGREES",{"$nulls":5},"EACH",{"$nulls":4},"364020"]
[]
[23,"CONE INNER DIAMETER : 135 MM X 0.2M X 15 DEGREES",{"$nulls":5},"EACH",{"$nulls":4},"364025"]
[]
[24,"CONE INNER DIAMETER : 135 MM X 1M X 15 DEGREES",{"$nulls":5},"EACH",{"$nulls":4},"364030"]
[]
[25,"CONE INNER DIAMETER : 135 MM X 1.5M X 15 DEGREES",{"$nulls":5},"EACH",{"$nulls":4},"NONE"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"SPECIAL STEEL STREETLIGHT POLES - COMPLETE WITH 15 DEGREE SPIGOT"]
[26,"11.5 M STEPPED POLE WITH SINGLE  SPIGOT OF 1 M"]
[null,"11.5m pole - 10m MH (planting depth = 1.5m)"]
[null,"(BOTTOM DIAMETER = 127 MM) (TOP DIAMETER = 76 MM)",{"$nulls":5},"EACH",{"$nulls":4},"468042"]
[]
[27,"13.7 M X 11.5 M STEPPED POLE WITH SINGLE  SPIGOT OF 2 M"]
[null,"13.7m pole - 12m Mounting Height - (planting depth = 1.7m)"]
[null,"(BOTTOM DIAMETER = 139 MM) (TOP DIAMETER = 76 MM)",{"$nulls":5},"EACH",{"$nulls":4},"468043"]
[]
[28,"13.7 M STEPPED POLE WITH DOUBLE SPIGOT OF 2 M"]
[null,"13.7m pole - 12m Mounting Height - (planting depth = 1.7m)"]
[null,"(BOTTOM DIAMETER = 139 MM) (TOP DIAMETER = 76 MM)",{"$nulls":5},"EACH",{"$nulls":4},"468044"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL"]
[]
[null,"STEEL STREETLIGHT POLES - 15 DEGREE SPIGOT "]
[29,"DOUBLE  SPIGOT OF 3 M (TO FIT 76 MM POLE TOP)",{"$nulls":5},"EACH",{"$nulls":4},"NONE"]
[]
[30,"DOUBLE  SPIGOT OF 1 M (TO FIT 76 MM POLE TOP)",{"$nulls":5},"EACH"]
[]
[null,"TOTAL",{"$nulls":5},"TOTAL",{"$nulls":4},"NONE"]
[]
[null,"HIGHMAST DISTRIBUTION BOARD"]
[31,"IP STANDARD INTERNAL DISTRIBUTION BOARD (5 PIN, 16 AMP)",{"$nulls":5},"EACH",{"$nulls":4},474025]
[null,"SECTIONAL POLES (OR SIMILAR)"]
[]
[null,"TOTAL"]
[]
[null,"132KV DOUBLE CIRCUIT KINGBIRD LINE CONCRETE POLES (OR SIMILAR)"]
[32,"21M/300MM DIA TIP/21 KN SPUN POLE – INTERMEDIATE ",{"$nulls":5},"EACH",{"$nulls":4},"NONE"]
[]
[33,"21M/300MM DIA TIP/40 KN SPUN POLE - STRAIN ",{"$nulls":5},"EACH",{"$nulls":4},"NONE"]
[]
[]
[null,"TOTAL"]