{"text_format":"3","workbook":"xls","n_sheets":23,"sheets":["Section 001","Section 002","Section 101","Section 102","Section 103","Section 105","Section 106","Section 201","Section 202","Section 203","Section 502","Section 503","Section 601","Section 602","Sheet1","Section 604","Section 605","Section 606","Section 609","Section 612","Section 613","Section 903","Summary"],"not_rendered":{"external_links":1,"defined_names":66,"comments":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Section 001","index":0,"n_rows":68,"n_cols":12,"rows_kept":68,"merged":[[65,0,65,4],[67,0,67,3],[67,4,67,5],[68,0,68,3],[68,4,68,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 0","GENERAL"]
[]
["Section 001","General Requirements and Charges"]
[]
["001.01","Preliminary and General Charges:"]
[]
["001.01.01","Fixed charges","Sum",1,null," "]
[]
["001.01.02","Time-related Charges","Month",16,null," "]
[]
["001.03","Excavate by hand to expose existing "]
[null,"services and backfill","m³",840,null," "]
[]
["B001.03.02","Relocating of existing services","Prov- sum",1,{"v":330000,"d":"R 330,000.00"},{"v":330000,"d":"R 330,000.00"}]
[null,"Services include payments for services "]
[null,"relocated by others, all carried out under the "]
[null,"direction and supervision of the Engineer"]
[]
["B001.03.03","Percentage on item B001.03.02 for"]
[null,"charges and profit","%",{"v":330000,"d":"330,000"},null,{"v":0,"d":"R 0.00"}]
[]
["001.04","Compliance with the Occupational"]
[null,"Health and Safety Act and applicable"]
[null,"regulations"]
[]
["001.04.01","Provision of a Health and Safety Plan","Lump Sum",1,null," "]
[]
["001.04.02","Provision of a Health and Safety File","Lump Sum",1,null," "]
[]
["001.04.03","Provision of construction supervisors-"]
[{"$nulls":7},{"v":6400000,"d":"R 6,400,000.00"},{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"},{"v":6400000,"d":"R 6,400,000.00"},0]
["001.04.03.02","Full time","Month",16,null," "]
[]
["001.04.04","Provision of a safety officer-"]
[]
["001.04.04.02","Full time","Month",16,null," "]
[]
["001.04.05","Health and safety training","lump sum",1,null,{"v":0,"d":"R 0.00"}]
[]
["001.04.06","Provision of personal protective"]
[null,"clothing and equipment","Lump Sum",1,null," "]
[]
["001.04.07","Provision of safety fences, signs and"]
[null,"barricades","Lump Sum",1,null," "]
[]
["B001.05","Community liaison officer"]
[]
["B001.05.01","Monthly Wage","month",16,{"v":20219.82,"d":"R 20,219.82"},{"v":323517.12,"d":"R 323,517.12"}]
[]
["001.05.02","Percentage on item B001.05.01 for"]
[null,"charges and profit","%",{"v":323517.12,"d":"R 323,517.12"},null," "]
[]
["B001.06","Contract Notice Board","no",2,null," "]
[null,"(See Drawing STD-001)"]
[]
["B001.07","Accredited Training"]
[]
["B001.07.01","Accredited training for Labourers","Prov.Sum",1,{"v":300000,"d":"R 300,000.00"},{"v":300000,"d":"R 300,000.00"}]
[]
[]
["B001.07.02","Percentage on item B001.07.01 for","%",{"v":300000,"d":"R 300,000.00"},null," "]
[null,"charges and profit"]
[]
["TOTAL CARRIED FORWARD",{"$nulls":10},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 002","index":1,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 0","GENERAL"]
[]
["Section 002","Engineer's Accommodation"]
[]
["002.01","Services"]
[]
["002.01.01","Services for offices and laboratories","Lump Sum",1,null,{"v":0,"d":"R 0.00"}]
[]
["002.02","Treatment and maintenance of areas"]
[null,"surrounding offices and "]
[null,"laboratories","Lump Sum",1,null,{"v":0,"d":"R 0.00"}]
[]
[]
["002.03","Office and laboratory accommodation"]
[]
["002.03.01","Provision of office and laboratory"]
[null,"accommodation, including fittings,"]
[null,"furniture and equipment and car ports,"]
[null,"as specified in project specifications","Lump Sum",1,null,{"v":0,"d":"R 0.00"}]
[]
["002.04","Provision of survey equipment and","Lump Sum",1,null,{"v":0,"d":"R 0.00"}]
[null,"assistants"]
[]
[]
[]
[]
[]
[]
[{"$nulls":7},92,null,null,92,0]
[]
[{"$nulls":7},92]
[]
[{"$nulls":7},92,null,null,92,0]
{"$rows_empty":13}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 101","index":2,"n_rows":52,"n_cols":12,"rows_kept":52,"merged":[[49,0,49,4],[51,0,51,3],[51,4,51,5],[52,0,52,3],[52,4,52,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 1","ANCILLARY WORK"]
[]
["Section 101","Site Clearing and Grubbing"]
[]
["101.01","Clearing and grubbing"]
[]
["LI101.01.01","Areas","m²",{"v":15679.999999999998,"d":"15,680"},null,{"v":0,"d":"R 0.00"}]
[]
["101.02","Cutting and removing large trees"]
[null,"with a girth -"]
[]
["101.02.01","exceeding 1m and up to and","no",null,null,{"v":0,"d":"R 0.00"}]
[null,"including 2m"]
[]
["101.03","Grubbing and the removal of the"]
[null,"stumps and roots of large trees with"]
[null,"girth -"]
[]
["101.03.01","exceeding 1m and up to and","no",null,null,{"v":0,"d":"R 0.00"}]
[null,"including 2m"]
[]
["101.04","Re-clearing of areas (only on the"]
[null,"written instructions of the Engineer)"]
[]
["101.04.02","Areas not classified as strips","m²",{"v":1000,"d":"1,000"},null,{"v":0,"d":"R 0.00"}]
[]
["101.05","Removal and disposal of specific"]
[null,"elements"]
[]
["101.05.01","Concrete kerbing / kerbing "]
[null,"combinations","m",175,null,{"v":0,"d":"R 0.00"}]
[]
["101.05.02","Concrete or brick elements"]
[null,"(reinforced or unreinforced)"]
[]
["LI101.05.02.01","230mm brickwork","m²",105,null,{"v":0,"d":"R 0.00"}]
[]
["101.05.02.02","Concrete elements (reinforced)","m²",10,null,{"v":0,"d":"R 0.00"}]
[]
["101.05.02.03","Interlocking / non-interlocking"]
[null,"paving blocks","m²",{"v":38.5,"d":"39"},null,{"v":0,"d":"R 0.00"}]
[]
["101.05.02.04","Boulders within Road Reserve","m3",250,null,{"v":0,"d":"R 0.00"},null,"ROAD LENGHT (m)","ROAD RESERVE MAX (m)",null,"QTY","PRICES"]
[{"$nulls":7},0,13,null,0,0]
["101.05.03","Asphalt surfacing","m²",50,null,{"v":0,"d":"R 0.00"},null,0,20,null,0,0]
[{"$nulls":10},0]
[]
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 102","index":3,"n_rows":107,"n_cols":6,"rows_kept":107,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5],[54,0,54,4],[104,0,104,4],[106,0,106,3],[106,4,106,5],[107,0,107,3],[107,4,107,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 1","ANCILLARY WORK"]
[]
["Section 102:","Accommodation of Traffic"]
[]
["102.01","Accommodation of traffic and"]
[null,"maintenance of bypasses","m²",{"v":10000,"d":"10,000"},null,{"v":0,"d":"R 0.00"}]
[]
[]
["102.02","Earthworks for bypasses"]
[]
["102.02.01","Shaping of bypasses","m",{"v":1800,"d":"1,800"},null,{"v":0,"d":"R 0.00"}]
[]
["102.02.02","Cut and borrow to fill","m³","rate only "]
[]
["102.02.03","Cut to spoil","m³",{"v":9000,"d":"9,000"}]
[]
[]
["102.03","Gravel wearing courses for"]
[null,"bypasses","m³",900,null,{"v":0,"d":"R 0.00"}]
[]
["102.04","Watering of bypasses","kℓ",{"v":503.99999999999994,"d":"504"},null,{"v":0,"d":"R 0.00"}]
[]
["102.05","Blading of bypasses by motor grader","km.pass",28,null,{"v":0,"d":"R 0.00"}]
[]
["102.07","Existing roads used as bypasses","m²",{"v":2500,"d":"2,500"}]
[]
["102.12","Provision of temporary bridges for"]
[null,"maintaining access to properties"]
[]
["102.12.02","Temporary vehicular bridges","no",null,null,{"v":0,"d":"R 0.00"}]
[]
["102.13","Moving of temporary bridges to and"]
[null,"re-erection in entirely new positions"]
[]
["102.13.02","Temporary vehicular bridges","no",null,null,{"v":0,"d":"R 0.00"}]
[]
["LI102.14","Temporary traffic-control facilities"]
[]
["102.14.01","Flagmen","Sum",1,null,{"v":0,"d":"R 0.00"}]
[]
["102.14.02","Portable Stop and Go signs","no",4,null,{"v":0,"d":"R 0.00"}]
[]
[]
[]
[]
[]
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["SERIES 1","ANCILLARY WORK"]
[]
["LI102.14","Temporary traffic-control facilities"]
[]
["102.14.04","Road signs, TR-series, 1200mm in"]
[null,"diameter or 900mm x 675mm if"]
[null,"rectangular","no",4,null,{"v":0,"d":"R 0.00"}]
[]
["102.14.05","Road signs, TW-series, 1200mm"]
[null,"sides","no",4,null,{"v":0,"d":"R 0.00"}]
[]
["102.14.06","Road signs, TG-series","m²",5,null,{"v":0,"d":"R 0.00"}]
[]
["102.14.07","Danger plates and delineators","no",25,null,{"v":0,"d":"R 0.00"}]
[]
["102.14.08","Moveable barricade / road sign"]
[null,"combination","no",10,null,{"v":0,"d":"R 0.00"}]
[]
["LI102.15","Re-use or removal of traffic-control"]
[null,"facilities"]
[]
[]
[]
["102.15.01","Amber flicker lights","no",0]
[]
["102.15.02","Road signs, TR and TW series","no",4]
[]
["102.15.03","Road signs, TG-series","no",5]
[]
["102.15.04","Danger plates and delineators","no",25,null,{"v":0,"d":"R 0.00"}]
[]
["102.15.05","Plastic New Jersey barrier","no",10,null,{"v":0,"d":"R 0.00"}]
[]
["102.16","Obliteration of bypasses","m²",{"v":10000,"d":"10,000"},null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":14}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 103","index":4,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 1","ANCILLARY WORK"]
[]
["Section 103","Overhaul"]
[]
["103.01","Overhaul on material hauled outside"]
[null,"the defined free-haul boundaries","m³.km",{"v":50400,"d":"50,400"},null,{"v":0,"d":"R 0.00"},null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},{"$error":"#REF!"}]
[]
[null,"(Free-haul boundaries will be defined",{"$nulls":5},{"v":4703.999999999999,"d":"4,704"}]
[null,"as 1km outside the indicated site ",{"$nulls":5},{"v":3000,"d":"3,000"}]
[null,"boundaries)",{"$nulls":5},{"$error":"#REF!"}]
[{"$nulls":7},{"$error":"#REF!"}]
[{"$nulls":7},{"v":5940,"d":"5,940"}]
[]
[{"$nulls":7},{"$error":"#REF!"}]
{"$rows_empty":32}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"$error":"#REF!"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 105","index":5,"n_rows":51,"n_cols":6,"rows_kept":51,"hidden":true,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 1","ANCILLARY WORK"]
[]
["Section 105","Fencing"]
[]
["105.03","Moving of existing fences and gates"]
[]
["105.03.01","Fences:"]
[]
["105.03.01.01","Ordinary Fences","m",null,{"v":450,"d":"R 450.00"},{"v":0,"d":"R 0.00"}]
[]
["105.03.02","Gates","no",null,{"v":650,"d":"R 650.00"},{"v":0,"d":"R 0.00"}]
[]
["105.04","Dismanteling of existing fences","m",null,{"v":185,"d":"R 185.00"},{"v":0,"d":"R 0.00"}]
[]
[]
["105.06","Provision of temporary fencing"]
[]
["105.06.01","Ordinary","m",null,{"v":1200,"d":"R 1,200.00"},{"v":0,"d":"R 0.00"}]
{"$rows_empty":28}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 106","index":6,"n_rows":56,"n_cols":12,"rows_kept":56,"merged":[[53,0,53,4],[55,0,55,3],[55,4,55,5],[56,0,56,3],[56,4,56,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 1","ANCILLARY WORK"]
[]
["Series 106","Service Ducts"]
[]
["LI106.01","Bedding and backfilling up to"]
[null,"300mm above pipes"]
[]
["106.01.01","Using selected excavated material","m³",30]
[]
["LI106.02","The casting of in situ concrete in"]
[null,"bedding and the encasing of pipes",{"$nulls":5},16.900000000000002]
[null,"(Class 20/19 concrete)","m³",{"v":3.5,"d":"4"},null,{"v":0,"d":"R 0.00"},null,50.699999999999996]
[{"$nulls":7},2,0.5,5,13,{"v":65,"d":"R 65.00"}]
["L106.03","Soilcrete","m³",35,null,{"v":0,"d":"R 0.00"}]
[{"$nulls":7},1150,null,null,1150,0]
["LI106.04","Service duct pipes"]
[]
["106.04.01","Ordinary pipes"]
[]
["106.04.01.01"," DN110 or similar approved","m",25,null,{"v":0,"d":"R 0.00"}]
[]
["106.04.03","Pipe fittings"]
[]
["106.04.03.01","Coupling for DN110 pipes",{"$nulls":8},0]
[null,"or similar approved","no",7,null,{"v":0,"d":"R 0.00"}]
[]
["106.04.03.01","Sealing ring for DN110 pipes"]
[null,"or similar approved","no",7,null,{"v":0,"d":"R 0.00"}]
[]
["106.04.03.01","End plug for DN110 pipes"]
[null,"or similar approved","no",7,null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":14}
[{"$nulls":7},5,null,null,5,0]
[]
[]
[]
[]
[]
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":65,"d":"R 65.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 201","index":7,"n_rows":54,"n_cols":12,"rows_kept":54,"merged":[[51,0,51,4],[53,0,53,3],[53,4,53,5],[54,0,54,3],[54,4,54,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":7},787.5]
["SERIES 2","EARTHWORKS"]
[]
["Section 201","General",{"$nulls":8},0.02]
[]
["201.02","Temporary stockpiling of material","m³",{"v":3000,"d":"3,000"},null,{"v":0,"d":"R 0.00"},null,0.3,1217,null,1825.4999999999998]
{"$rows_empty":44}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 202","index":8,"n_rows":106,"n_cols":12,"rows_kept":106,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5],[54,0,54,4],[103,0,103,4],[105,0,105,3],[105,4,105,5],[106,0,106,3],[106,4,106,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 2","EARTHWORKS"]
[]
["Section 202","Trenching"]
[]
["202.01","Trench excavation"]
[{"$nulls":7},"Overall Excavation: ",null,11520]
["202.01.01","Up to 1,0m wide",{"$nulls":5},"Pipe Network",null,1965.6]
[{"$nulls":7},"Soft 40%",null,786.24]
["202.01.01.01","Up to 1,0m deep","m³",{"v":314.49600000000004,"d":"314"},null,{"v":0,"d":"R 0.00"},null,"Intermediate 35%",null,687.9599999999999]
[{"$nulls":7},"Hard 25%",null,491.4]
["202.01.01.02","Over 1,0m deep and up to 1,5m deep","m³",{"v":471.74399999999997,"d":"472"},null,{"v":0,"d":"R 0.00"}]
[]
["202.01.01.03","Over 1,5m deep and up to 2,0m deep","m³",35,null,{"v":0,"d":"R 0.00"}]
[]
["202.01.01.04","Over 2,0m deep and up to 2,5m deep","m³","rate only"]
[]
["202.01.01.05","Over 2,5m deep and up to 3,0m deep","m³","rate only"]
[]
["202.02","Extra over items 202.01, 202.03 and"]
[null,"202.09 for excavating in -"]
[]
["202.02.01","Intermediate material","m³",950,null,{"v":0,"d":"R 0.00"}]
[]
["202.02.02","Hard material","m³",495,null,{"v":0,"d":"R 0.00"}]
[{"$nulls":7},"SUBBASE+BASE+0.03",null,"LENGTH",0,0]
[{"$nulls":7},0.33,null,1217,2008.0500000000002]
["202.03","Excavations outside the normal"]
[null,"trench profile","m³",105,null,{"v":0,"d":"R 0.00"}]
[]
["202.04","Hand excavation (extra over item"]
[null,"202.01)","m³",125,null,{"v":0,"d":"R 0.00"}]
[]
["202.06","The backfilling of trenches (excluding"]
[null,"the backfill around the pipe barrel)"]
[null,"with material obtained from"]
[null,"excavations","m³",{"v":1179.36,"d":"1,179"},null,{"v":0,"d":"R 0.00"}]
[]
["202.07","Extra over items 202.06 and 202.13"]
[null,"for using backfill material obtained -"]
[]
["202.07.01","From borrow areas","m³",{"v":393.12,"d":"393"},null,{"v":0,"d":"R 0.00"}]
[]
["202.07.02","From sources provided by the"]
[null,"contractor","m³",{"v":314.49600000000004,"d":"314"},null,{"v":0,"d":"R 0.00"}]
[]
[]
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["202.10","Removal of spoil material -"]
[]
["202.10.02","To positions indicated on the drawings or "]
[null,"by by the Engineer","m³",{"v":117.93599999999999,"d":"118"},null,{"v":0,"d":"R 0.00"}]
[]
["202.10.02","To dumping areas to be provided by","m³",{"v":589.68,"d":"590"},null,{"v":0,"d":"R 0.00"}]
[null,"Contractor"]
[]
["202.12","Extra over item 202.06 for additional"]
[null,"compaction of backfill to 93% of"]
[null,"modified AASHTO density in road"]
[null,"reserves","m³",{"v":1320,"d":"1,320"},null,{"v":0,"d":"R 0.00"}]
[]
["202.13","Backfilling trenches with soilcrete","m³",100,null,{"v":0,"d":"R 0.00"}]
[]
["202.15","Reinstatement of bitumen surfaced",{"$nulls":5},"LENGTH","WIDTH","PASS",0,0]
[null,"roads","m²",50,null,{"v":0,"d":"R 0.00"},null,1217,5,3,18255]
{"$rows_empty":10}
[{"$nulls":7},912.75,null,null,912.75,0]
[]
[]
[]
[]
[]
[]
[{"$nulls":7},1648.0500000000002,null,null,1648.0500000000002,0]
[]
[{"$nulls":7},1500,null,null,1500,0]
{"$rows_empty":10}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 203","index":9,"n_rows":99,"n_cols":12,"rows_kept":99,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5],[54,0,54,4],[98,4,98,5],[99,4,99,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 2","EARTHWORKS"]
[]
["Section 203","Mass Earthworks"]
[]
["203.01","Excavation and borrow to fill"]
[{"$nulls":7},"Overall Excavation: ",null,9900]
["203.01.01","Compaction to 90% of modified"]
[null,"AASHTO density","m³",{"v":3960,"d":"3,960"},null,{"v":0,"d":"R 0.00"},null,"Soft 40%"]
[{"$nulls":7},"Intermediate 35%"]
[{"$nulls":7},"Hard 25%"]
["203.02","Extra over item 203.01 for excavating"]
[null,"in -"]
[]
["203.02.01","Intermediate material","m³",{"v":3465,"d":"3,465"},null,{"v":0,"d":"R 0.00"}]
[]
["203.02.02","Hard material","m³",{"v":2475,"d":"2,475"},null,{"v":0,"d":"R 0.00"}]
[]
["203.02.03","Boulder material class  A","m³",null,null,{"v":0,"d":"R 0.00"}]
[]
["203.02.04","Boulder material class B","m³",null,null,{"v":0,"d":"R 0.00"}]
[]
[]
["203.03","Excavate and spoil of -"]
[]
["203.03.01","Soft material","m³",{"v":5940,"d":"5,940"},null,{"v":0,"d":"R 0.00"},null,"SUBBASE+BASE+0.03",null,"LENGTH",0,0]
[{"$nulls":7},0.33,null,2000,3300]
["203.03.02","Intermediate material","m³",{"v":1732.5,"d":"1,733"},null,{"v":0,"d":"R 0.00"}]
[]
["203.03.03","Hard material","m³",{"v":618.75,"d":"619"},null,{"v":0,"d":"R 0.00"}]
[]
["203.03.04","Boulder material class  A","m³",0,null,{"v":0,"d":"R 0.00"}]
[]
["203.03.05","Boulder material class B","m³",0,null,{"v":0,"d":"R 0.00"}]
[]
[]
["203.04","Removal of oversize material","m³",50,null,{"v":0,"d":"R 0.00"}]
[]
["203.06","Widening of cuttings (extra over"]
[null,"items 203.01 and 203.03)"]
[]
["203.06.01","In hard material","m³",null,{"v":400,"d":"R 400.00"},{"v":0,"d":"R 0.00"}]
[]
["203.06.02","In intermediate and soft material","m³",null,{"v":125,"d":"R 125.00"},{"v":0,"d":"R 0.00"}]
[]
["203.06.03","In boulder material class A or class B","m³",0,{"v":250,"d":"R 250.00"},{"v":0,"d":"R 0.00"}]
[]
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["203.08","Preparation and compaction of"]
[null,"construction bed material to 90% of"]
[null,"modified AASHTO density"]
[]
["203.08.01","For Roadworks","m³",{"v":1980,"d":"1,980"},null,{"v":0,"d":"R 0.00"}]
[]
["203.08.01","For Walkways","m³",675,null,{"v":0,"d":"R 0.00"}]
[]
["203.10","In situ treatment of the construction "]
[null,"bed"]
[]
["203.10.02","In situ treatment by blasting","m³",225,null,{"v":0,"d":"R 0.00"}]
[]
["203.11","Finishing off slopes"]
[]
["LI 203.11.01","Excavation slopes","m²",{"v":2160,"d":"2,160"},null," "]
[]
["LI 203.11.02","Fill slopes","m²",{"v":2160,"d":"2,160"},null," "]
[{"$nulls":7},"LENGTH","WIDTH","PASS",0,0]
["203.14","Extra over item 203.01 for borrow","m³",198,null,{"v":0,"d":"R 0.00"},null,1217,5,3,18255]
[null,"material from sources to be"]
[null,"supplied by the Contractor"]
[]
["203.15","Extra over item 203.03 and 203.04 for ","m³",{"v":8341.25,"d":"8,341"},null,{"v":0,"d":"R 0.00"},null,912.75,null,null,912.75,{"$error":"#REF!"}]
[null,"disposing of spoil material to sites to be"]
[null,"provided by the Contractor"]
[]
[]
[]
[]
[{"$nulls":7},1648.0500000000002,null,null,1648.0500000000002,0]
{"$rows_empty":9}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"$error":"#REF!"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 502","index":10,"n_rows":103,"n_cols":12,"rows_kept":103,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5],[54,0,54,4],[100,0,100,4],[102,0,102,3],[102,4,102,5],[103,0,103,3],[103,4,103,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 5","DRAINAGE AND EROSION"]
[null,"PROTECTION"]
[]
["Section 502","Prefabricated Culverts and"]
[null,"Stormwater Sewers"]
[]
["502.01","Backfilling with selected excavated"]
[null,"material compacted to -"]
[]
["502.01.01","90% of modified AASHTO density","m³",{"v":178.5,"d":"179"},null,{"v":0,"d":"R 0.00"}]
[]
["502.01.02","93% of modified AASHTO density","m³",{"v":325.5,"d":"326"},null,{"v":0,"d":"R 0.00"}]
[]
["502.01.03","95% of modified AASHTO density","m³",{"v":129.5,"d":"130"},null,{"v":0,"d":"R 0.00"}]
[]
[]
["502.02","Supplying and laying of concrete"]
[null,"pipe culverts (type SC-pipes)"]
[]
["502.02.01","Class B bedding / Class 50D"]
[]
["502.02.01.01","450mm Ø","m",935,null,{"v":0,"d":"R 0.00"}]
[]
["502.02.01.03","600mm Ø","m",300,null,{"v":0,"d":"R 0.00"}]
[]
["502.02.02","Class B bedding / Class 75D",{"$nulls":6},200,null,200,0]
[]
["502.02.02.01","450mm Ø","m",120,null,{"v":0,"d":"R 0.00"}]
[]
["502.02.02.03","600mm Ø","m",36,null,{"v":0,"d":"R 0.00"}]
[]
["502.10","Cast in situ concrete",{"$nulls":6},150,null,150,0]
[]
["502.10.01","In Class A bedding, blinding layers"]
[null,"and encasing of pipes, including"]
[null,"any formwork required"]
[]
["502.10.01.01","Class 20/19","m³",180,null,{"v":0,"d":"R 0.00"}]
[]
["LI502.16","Manholes, catchpits, precast inlet and",{"$nulls":9},0]
[null,"outlet structures and junction boxes"]
[null,"complete",{"$nulls":9},0]
[]
["502.16.01","Manholes (type and standard depth","No",15,null,{"v":0,"d":"R 0.00"},null,0,200,null,200,0]
[null," indicated)"]
[]
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["502.16.02","Catchpits (Sloping Kerb Both Sides as per","No",29,null,{"v":0,"d":"R 0.00"}]
[null,"Standard detail STD-003)"]
[]
[]
["502.16.05","Junction boxes (Type C)","No",6,null,{"v":0,"d":"R 0.00"},null,null,150,null,150,0]
[null,"`"]
["502.16.05","Junction boxes (Type D)","No",4,null,{"v":0,"d":"R 0.00"}]
[null,"`"]
["502.16.06","Extra over or under item 502.16.01 for ","No",3,null,{"v":0,"d":"R 0.00"}]
[null," variation in depth manholes from the"]
[null,"standard depth designated for purposes"]
[null,"of tendering (manhole type indicated0"]
[]
["LI502.23","Cleaning existing culverts","m³",45,null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":30}
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 503","index":11,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 5","DRAINAGE AND EROSION"]
[null,"PROTECTION"]
[]
["Section 503","Kerbing and Channelling"]
[]
["LI503.01","Concrete kerbing Class 20/19"]
[null,"concrete  "]
[null,"(See drawing STD007 - Sheet 1)"]
[]
["503.01.01","Edge beam","m",{"v":2200,"d":"2,200"},null,{"v":0,"d":"R 0.00"},null,1100,0,0,1100,0]
[]
["503.01.02","300mm Sloping  kerb(fig 8c)","m",{"v":2200,"d":"2,200"},null,{"v":0,"d":"R 0.00"},null,550,null,null,550,0]
[]
["LI503.03","Transition sections"]
[null,"(See drawing STD007 - Sheet 2)"]
[]
["503.03.01","Semi-vertical kerb (Fig. 7) to "]
[null,"edge beam","no",{"v":17.5,"d":"18"},null,{"v":0,"d":"R 0.00"}]
[]
["503.03.02","Semi-vertical kerb (Fig. 7) to "]
[null,"300mm sloping kerb","no",21,null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":16}
[{"$nulls":7},10,null,null,10,0]
{"$rows_empty":8}
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 601","index":12,"n_rows":50,"n_cols":12,"rows_kept":50,"merged":[[47,0,47,4],[49,0,49,3],[49,4,49,5],[50,0,50,3],[50,4,50,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 601","Gravel Pavement Layers"]
[]
["601.02","Gravel layers constructed from"]
[null,"material obtained from Borrow Pits"]
[]
["601.02.01","Subgrade ",{"$nulls":8},0,0]
[]
["601.02.01.01","150mm G5 material Compacted to 93% of modified",{"$nulls":5},1350,null,null,1350,0]
[null,"AASHTO density","m³",{"v":2160,"d":"2,160"},null,{"v":0,"d":"R 0.00"}]
[]
["601.02.01.02","Compacted to 95% of modified"]
[null,"AASHTO density","m³",{"v":2160,"d":"2,160"}]
[]
["601.02.02","Subbase"]
[]
["601.02.02.01","150mm G5 Compacted to 95% of modified"]
[null,"AASHTO density - RoadWorks","m³",{"v":2160,"d":"2,160"},null,{"v":0,"d":"R 0.00"},null,{"v":640.74,"d":"R 640.74"},null,null,640.74,0]
[]
["601.02.02.02","150mm G5 Compacted to 95% of modified"]
[null,"AASHTO density - Walkways","m³",{"v":545.9999999999999,"d":"546"},null,{"v":0,"d":"R 0.00"}]
[]
["601.02.02.02","Compacted to 97% of modified"]
[null,"AASHTO density","m³","rate only"]
[]
["601.03","Gravel layers constructed from"]
[null,"material obtained from excavations"]
[]
["601.03.01","Subgrade",{"$nulls":8},0,0]
[]
["601.03.01.02","150mm G7 Compacted to 93% of modified"]
[null,"AASHTO density","m³",864,null,{"v":0,"d":"R 0.00"}]
[]
["601.03.01.03","Compacted to 95% of modified"]
[null,"AASHTO density","m³","rate only"]
[]
["601.06","Extra over item 601.02 for borrow "]
[null,"material from sources to be supplied by"]
[null,"the Contractor",{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["601.06.01","150mm G5 material (Subgrade)","m³",{"v":2160,"d":"2,160"},null,{"v":0,"d":"R 0.00"},{"$nulls":4},0,0]
[]
["601.06.02","150mm G5 material (Subbabse)","m³",{"v":2706,"d":"2,706"},null,{"v":0,"d":"R 0.00"}]
[]
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 602","index":13,"n_rows":50,"n_cols":12,"rows_kept":50,"merged":[[47,0,47,4],[49,0,49,3],[49,4,49,5],[50,0,50,3],[50,4,50,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 602","Crushed-stone Pavement Layers"]
[]
["602.01","Crushed-stone base constructed"]
[null,"with material obtained from"]
[]
["602.01.01","Commercial sources"]
[]
["602.01.01.01","G2 material compacted to 86% of"]
[null,"Apparent density","m³",{"v":2160,"d":"2,160"},null,{"v":0,"d":"R 0.00"},null,{"v":744.1700000000001,"d":"R 744.17"}]
[]
["602.04","Additional compaction"]
[]
["602.04.01","Extra over sub items 602.01.01.01","m³",{"v":2160,"d":"2,160"},null,{"v":0,"d":"R 0.00"}]
[null,"602.01.02.01, 602.02.01.01 and"]
[null,"602.02.02.01 for compaction to"]
[null,"88% of apparent density"]
{"$rows_empty":27}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Sheet1","index":14,"n_rows":51,"n_cols":6,"rows_kept":51,"hidden":true,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 603","Unpaved areas"]
[]
["603.01","Compacted gravel shoulder or gravel"]
[null,"wearing course to 93% of modified"]
[null,"AASHTO density"]
[]
["603.01.01","Shoulder","m³",null,{"v":132,"d":"R 132.00"}," "]
[]
["603.01.02","Wearing course","m³",null,{"v":132,"d":"R 132.00"},{"v":0,"d":"R 0.00"}]
[]
[]
["603.02","Extra over Item 603.01 for borrow"]
[null,"material from sources to be"]
[null,"supplied by the Contractor","m³",null,{"v":320,"d":"R 320.00"},{"v":0,"d":"R 0.00"}]
{"$rows_empty":30}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 604","index":15,"n_rows":53,"n_cols":13,"rows_kept":53,"merged":[[50,0,50,4],[52,0,52,3],[52,4,52,5],[53,0,53,3],[53,4,53,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 604","Stabilization"]
[]
["604.01","Chemical stabilization extra over"]
[null,"unstabilized compacted layers"]
[]
["604.01.03","Subbase - RoadWorks","m³",{"v":2160,"d":"2,160"},null,{"v":0,"d":"R 0.00"}]
[]
["604.01.03","Subbase - Walkways","m³",540,null,{"v":0,"d":"R 0.00"}]
[]
["604.02","Chemical stabilizing agent"]
[]
["604.02.01","Cement","t",{"v":237.6,"d":"238"},null,{"v":0,"d":"R 0.00"},null,22.816666666666666,null,22.816666666666666,null,22.816666666666666]
[]
[{"$nulls":7},"Cement density ",null,"Cement density ",null,"Cement density "]
[{"$nulls":7},1440,"kg/m3",1441,"kg/m4",1442,"kg/m5"]
[]
[{"$nulls":7},"Stabilise",null,"Stabilise",null,"Stabilise"]
[{"$nulls":7},{"v":0.025,"d":"2.50%"},null,{"v":1.025,"d":"102.50%"},null,{"v":2.025,"d":"202.50%"}]
[{"$nulls":7},54,"m3",0,"m4",0,"m5"]
[{"$nulls":7},103.68,null,103.68,null,103.68]
{"$rows_empty":26}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":1570.5216666666668,"d":"R 1,570.52"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 605","index":16,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 605","Prime Coat"]
[{"$nulls":7},29]
["605.01","Prime coat"]
[]
["605.01.02","MC-30 cut-back bitumen","ℓ",{"v":14400,"d":"14,400"},{"$nulls":3},4868]
[]
["605.01.03","MC-70 cutback bitumen","ℓ","rate only",null,"ro"]
["605.02","Aggregate for blinding","m²",{"v":14400,"d":"14,400"}]
[]
[{"$nulls":7},7950,6853,6304,21107,0]
{"$rows_empty":34}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 606","index":17,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 606","Asphalt Base and Surfacing"]
[]
["606.02","Asphalt surfacing"]
[]
["606.02.01","30mm Continuously graded (medium)","m2",{"v":14000,"d":"14,000"},null," "]
[{"$nulls":5}," "]
["B606.02.02","Extra over or under item 606.02.01 for ","No",10,null," "]
[null,"traffic calming measures (Speed Humps)",{"$nulls":3}," "]
[null,"as per dwg STD0016",{"$nulls":3}," "]
[{"$nulls":5}," "]
["606.05","Tack coat of 30% stable grade","ℓ",{"v":14000,"d":"14,000"},null," "]
[null,"emulsion @1l/m2"]
[]
[{"$nulls":7},2.3,0.03,6085,419.86499999999995]
{"$rows_empty":30}
["TOTAL CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 609","index":18,"n_rows":54,"n_cols":6,"rows_kept":54,"merged":[[51,0,51,4],[53,0,53,3],[53,4,53,5],[54,0,54,3],[54,4,54,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 609","Segmented Paving"]
[]
["LI609.01","Construction of segmental block"]
[null,"paving made from -"]
[]
["609.01.01","60mm Type S-A, Class 25 grey "]
[null,"precast blocks","m²",{"v":4320,"d":"4,320"},null,{"v":0,"d":"R 0.00"}]
[]
["LI609.03","The construction of edge restraints"]
[null,"with"]
[]
["609.03.01","Rectangular precast concrete kerb"]
[null,"(Figure 10)","m",{"v":4000,"d":"4,000"},null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":35}
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 612","index":19,"n_rows":62,"n_cols":12,"rows_kept":62,"merged":[[59,0,59,4],[61,0,61,3],[61,4,61,5],[62,0,62,3],[62,4,62,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 612","Traffic Signs"]
[]
["612.01","Sign boards with painted back-"]
[null,"ground, symbols, lettering and"]
[null,"borders in engineering-grade retro-"]
[null,"reflective material with sign boards"]
[null,"constructed from -"]
[]
["612.01.03","Sheet steel (Chromadek) with an -"]
[]
["612.01.03.01","Area not exceeding 2m²","m²",40,null,{"v":0,"d":"R 0.00"},null,43,null,null,43,0]
[]
["612.01.03.02","Area exceeding 2m² but not 10m²","m²",10,null,{"v":0,"d":"R 0.00"}]
[]
["612.02","Extra over Item 612.01 for -"]
[]
["612.02.01","Background of retro-reflective"]
[null,"material of -"]
[]
["612.02.01.01","Super-Engineering grade","m²",15,null,{"v":0,"d":"R 0.00"}]
[]
["612.02.02","Lettering, symbols and borders of"]
[null,"retro-reflective material of -",{"$nulls":5},15,null,null,15,0]
[]
["612.02.02.01","High-intensity grade","m²",16,null,{"v":0,"d":"R 0.00"}]
[]
["612.02.02.02","Super-engineering grade","m²",5,null,{"v":0,"d":"R 0.00"}]
[]
["LI612.03","Sign supports"]
[]
["612.03.02","Steel tubing","t",2,null,{"v":0,"d":"R 0.00"}]
[]
["612.04","Extra over Items 612.03.01 and"]
[null,"612.03.02 for providing"]
[]
["612.04.01","Unpainted galvanized steel members","t",{"v":0,"d":"0.00"}]
[]
["612.04.02","Painted galvanized steel members","t",{"v":0.5,"d":"0.50"},null,{"v":0,"d":"R 0.00"}]
[]
[]
["612.05","Excavation and backfilling for"]
[null,"sign supports","m³",14,null,{"v":0,"d":"R 0.00"}]
[]
["LI612.06","Dismantling, storing and re-erecting"]
[null,"traffic signs with a surface area of -"]
[]
["612.06.01","Up to 2m²","no",35,null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":8}
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 613","index":20,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
[]
["Section 613","Traffic Markings"]
[]
["613.01","Road-marking paint"]
[]
["613.01.06","Kerb markings (any colour)","m²",null,{"v":150,"d":"R 150.00"},{"v":0,"d":"R 0.00"}]
[]
[]
["613.02","Retro-reflective road-marking paint"]
[]
["613.02.01","White lines (broken or unbroken)"]
[null,"100mm wide","km",3,null,{"v":0,"d":"R 0.00"},null,2,null,null,2,0]
[]
["613.02.03","White lettering and symbols","m²",50,null,{"v":0,"d":"R 0.00"}]
[{"$nulls":7},2,null,null,2,0]
["613.04","Variation in the rate of application"]
[{"$nulls":7},7,null,16,51]
["613.04.01","White paint","ℓ",null,null,{"v":0,"d":"R 0.00"}]
["613.06","Setting out and the premarking of "]
[null,"lines (excluding traffic-island"]
[null,"markings, lettering and symbols)","km",2]
{"$rows_empty":24}
["TOTAL CARRIED FORWARD",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Section 903","index":21,"n_rows":51,"n_cols":6,"rows_kept":51,"merged":[[48,0,48,4],[50,0,50,3],[50,4,50,5],[51,0,51,3],[51,4,51,5]],"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["SERIES 9","QUALITY CONTROL"]
[]
["Section 903","Testing"]
[]
["903.06","Other special tests requested by "]
[null,"the Engineer"]
[]
["903.06.01","Cost of Testing","PC.Sum",1,{"v":600000,"d":"R 600,000.00"},{"v":600000,"d":"R 600,000.00"}]
[]
["903.06.02","Percentage on item 903.06.01 for","%",{"v":600000,"d":"600,000.00"},null,{"v":0,"d":"R 0.00"}]
[null,"charges and profit"]
{"$rows_empty":35}
["TOTAL CARRIED FORWARD"]
[]
["Signature of person authorised to sign the tender:",{"$nulls":3},"Date"]

{"sheet":"Summary","index":22,"n_rows":82,"n_cols":3,"rows_kept":82,"merged":[[0,0,0,2],[54,0,54,1],[56,0,56,1],[57,0,57,1],[58,0,58,1],[59,0,59,1],[60,0,60,1],[61,0,61,1],[62,0,62,1],[63,0,63,1],[64,0,64,1],[65,0,65,1],[79,0,79,1],[81,0,81,1],[82,0,82,1]],"flags":["formulas_cached_only"]}
["SUMMARY OF PRICING SCHEDULE"]
["SECTION","DESCRIPTION","AMOUNT"]
[]
["SERIES 0","GENERAL   "]
["001","General Requirements and Charges",{"v":0,"d":"R 0.00"}]
["002","Engineers Accommodation",{"v":0,"d":"R 0.00"}]
[]
["SERIES 1 ","ANCILLARY WORK"]
["101","Site Clearing and Grubbing",{"v":0,"d":"R 0.00"}]
["102","Accommodation of Traffic",{"v":0,"d":"R 0.00"}]
["103","Overhaul",{"v":0,"d":"R 0.00"}]
["105","Fencing",{"v":0,"d":"R 0.00"}]
["106","Service Ducts",{"v":0,"d":"R 0.00"}]
[]
["SERIES 2","EARTHWORKS"]
["201","General",{"v":0,"d":"R 0.00"}]
["202","Trenching",{"v":0,"d":"R 0.00"}]
["203","Mass Earthworks",{"v":0,"d":"R 0.00"}]
[]
["SERIES 5","DRAINAGE AND EROSION PROTECTION"]
["502","Prefabricated Culverts and Stormwater Drainage",{"v":0,"d":"R 0.00"}]
["503","Kerbing and Channelling",{"v":0,"d":"R 0.00"}]
[]
["SERIES 6","ROADS AND PARKING AREAS"]
["601","Gravel Pavement Layers",{"v":0,"d":"R 0.00"}]
["602","Crushed-stone Pavement Layers",{"v":0,"d":"R 0.00"}]
["603","Unpaved Areas",{"v":0,"d":"R 0.00"}]
["604","Stabilization",{"v":0,"d":"R 0.00"}]
["605","Prime Coat",{"v":0,"d":"R 0.00"}]
["606","Asphalt Base and Surfacing",{"v":0,"d":"R 0.00"}]
["609","Segmented Paving",{"v":0,"d":"R 0.00"}]
["612","Traffic Signs",{"v":0,"d":"R 0.00"}]
["613","Traffic Markings",{"v":0,"d":"R 0.00"}]
[]
["SERIES 9","QUALITY CONTROL"]
["903","Testing",{"v":0,"d":"R 0.00"}]
{"$rows_empty":18}
["TOTAL SCHEDULE OF PRICES",null,{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:"]
[]
["DESCRIPTION",null,"AMOUNT"]
[]
["TOTAL OF SCHEDULED PRICES",null,{"v":0,"d":"R 0.00"}]
["Add 10% for contingencies",null,{"v":0,"d":"R 0.00"}]
["SUBTOTAL 1",null,{"v":0,"d":"R 0.00"}]
["Add 15% VAT",null,{"v":0,"d":"R 0.00"}]
["TOTAL ",null,{"v":0,"d":"R 0.00"}]
[null,null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":13}
["CONTRACT PRICE CARRIED FORWARD TO FORM OF OFFER",null,{"v":0,"d":"R 0.00"}]
[]
["Signature of person authorised to sign the tender:",null,"Date"]