{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Activity Schedule","Sheet2","Sheet3"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Activity Schedule","index":0,"n_rows":51,"n_cols":8,"rows_kept":51}
[null,null,"QUENCHING PIPELING"]
[null,null,"ACTIVITY SCHEDULE - HIGH LEVEL"]
[]
[{"$nulls":5},"Condensate Quenching Water Pipeline"]
[]
[{"$nulls":3},"ITEM","PROGRAMME REFERNCE","DESCRIPTION","UNIT","AMOUNT"]
[{"$nulls":3},1,null,"Preliminaries and General"]
[]
[{"$nulls":3},1.1,null,"Fixed Charge And Value-Related Items","Sum"]
[]
[{"$nulls":3},1.2,null,"Time-Related Items","Sum"]
[]
[{"$nulls":5},"A","Sub-Total",{"$f":"SUM(H7:H11)","v":0}]
[]
[]
[{"$nulls":5},"CARBON STEEL PIPING LINED INTERNALLY AS PER SPEC DCS1500, CPS500 EXTERNALLY FOR BUIRED PIPING AND DCS200 FOR PIPING INSTALLED ABOVE GROUND "]
[]
[{"$nulls":3},"ITEM","PROGRAMME REFERNCE","DESCRIPTION","UNIT","AMOUNT"]
[{"$nulls":3},2.1,null,"Supply, Fabricate, Erect, Flush And Test The Following SANS719/62 CARBON STEEL PIPING in earth trench or on ground level including Bends, Reducers, Tees, gaskets and all connections.","Sum"]
[]
[{"$nulls":3},2.2,null,"Supply and Install inline Valves, Instruments, etc","Sum"]
[]
[{"$nulls":3},2.3,null,"Supply and Install Pipe Supports including all relevant connections.","Sum"]
[]
[{"$nulls":3},2.4,null,"Excavate for concrete bases","Sum"]
[]
[{"$nulls":3},2.5,null,"Concrete works 30Mpa","Sum"]
[]
[{"$nulls":3},2.6,null,"KKS Coding","Sum"]
[]
[{"$nulls":3},2.7,null,"Geotechnical Investigation","Sum"]
[]
[{"$nulls":3},2.8,null,"Operators training","Sum"]
[]
[{"$nulls":3},2.9,null,"Intergrating with the existing DCS","Sum"]
[]
[{"$nulls":3},{"v":2.1,"d":"2.10"},null,"Testing and commissioning","Sum"]
[]
[{"$nulls":3},2.11,null,"Design, Monitoring, close-out report","Sum"]
[]
[]
[{"$nulls":5},"B","Sub-Total",{"$f":"SUM(H19:H40)","v":0}]
[]
[]
[{"$nulls":5},"SUMMARY"]
[]
[{"$nulls":5},"DESCRIPTION","CODE","AMOUNT"]
[{"$nulls":5},"PRELIMINARIES AND GENERAL","A",{"$f":"H13","v":0}]
[{"$nulls":5},"Piping, connections, valves and supports","B",{"$f":"H42","v":0}]
[]
[{"$nulls":6},"TOTAL",{"$f":"SUM(H48:H50)","v":0}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}