{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Specification"],"read":"whole","date_system":"1900"}

{"sheet":"Specification","index":0,"n_rows":24,"n_cols":4,"rows_kept":24,"merged":[[0,0,0,3]]}
["Building renovations: Hebarium"]
["Service description","UoM","Quantity/size","Cost Vat Exc"]
["Construct drywall partitions to create an office, kitchen space, and passage - As dicussed in the site briefing and refer to the building layout plan"]
["Relocation of an existing aircon and install to another office, 10m length of truncking should be included",null,1]
["Supply and install powder coated security doors/burglar gates similar to Trellis one, covering the entire outside door.","1. 2.1m(h)x1.5m(w(2 doors)                                 2.  2.1 m(h)x 0.8m(w)(1 door)",3]
["Supply and install alluminium full frosted/Sandblasted double glass doors together with a frame and  complete lockset, and ARC logo inserted in the middle","1. 2.1m(h)x1.5m(w)(1 door)                                ",1]
["Supply and install/fit 5ft LED light with double tubes, cabling should be included",null,4]
["Supply and install electric double plugs, cabling should be included",null,2]
["Supply and install electric single light switches, cabling should be included",null,3]
["Supply and install outdoor LED spotlights and,  day and night switches,  cabling should be included","150watts",4]
["Install doors to both the office and kitchen spaces","2.1 m(h)x 0.8m",3]
["Supply and Install kitchen cupboards with highgloss double doors of 70cm(h)x 50cm(w) each inclusive of door handles (with 2 shelves each), double bowl with drainer kitchen inset sink deb 1200 x 500 x 6mm stainless steel, 1.4m kitchen countertop granite, and stainless steel kitchen sinkmixer.",null,1]
["Drainage system ( 25m 110 pvc pipes for drainage including trenching, 90◦ 110 bend x 3, 3m of 50mm pipe, 50mm bend with i'e, gully trap x1, 20m copper pipe 15mm, 15mm polycop pipe 30m, tee compression and 6 x Copper Elbow 90d)"]
[]
[]
[null,null,"Total cost"]
[null,null,"VAT"]
[null,null,"Grand Total "]
[]
["Conditions attached to the project"]
["1. Full payment will be action upon project completion, there will be no partial payment"]
["2. Contractor to clean up all the rubbles from the site"]
["3. Contractor must ensure personell have full PPE regalia relevant to the project, failure to comply with this might result in the termination of the project"]
["4. Contractor to adhere to OHS contract management compliance e.g. Complete contractor SHE file"]