{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["BOQ"],"not_rendered":{"external_links":3,"defined_names":12},"read":"whole","date_system":"1900"}

{"sheet":"BOQ","index":0,"n_rows":611,"n_cols":14,"rows_kept":611,"merged":[[0,1,1,5],[2,1,2,3],[2,5,2,7],[2,8,2,10],[2,11,2,13],[4,1,4,4],[5,1,6,1],[5,2,6,2],[75,2,76,2],[149,6,149,7]]}
[null,"REQUEST FOR A PANEL OF SERVICE PROVIDERS TO SUPPLY, INSTALL, COMMISSION AND REPAIR/MAINTAIN MECHANICAL AND ELECTRICAL COMPONENTS FOR WATER AND WASTEWATER APPLICATIONS FOR UGU DISTRICT MUNICIPALITY FOR A PERIOD OF THIRTY-SIX (36) MONTHS "]
[]
[null,"CONTRACT NO: UGU-07-1687-2024",{"$nulls":3},"YEAR 1",null,null,"YEAR 2",null,null,"YEAR 3"]
[null,"No.","Items","Description of equipment or scope of work","Quantity","Rater (Supply and Deliver)","Rate (Major Overhauling / Maintenance) ","Rate - Installation,  alignment, commissioning and testing  ","Rater (Supply and Deliver)","Rate (Major Overhauling / Maintenance) ","Rate - Installation,  alignment, commissioning and testing  ","Rater (Supply and Deliver)","Rate (Major Overhauling / Maintenance) ","Rate - Installation,  alignment, commissioning and testing  "]
[null,"SECTION 1: PUMPS AND GEARBOXES"]
[null,1.1,"GORMAN-RUPP","PUMPS",1]
[{"$nulls":3},"112B60.B, MODEL NO : 112860-3",1]
[null,1.2,"GORMAN-RUPP","T6A3S.B/FM",1]
[null,1.3,"GORDON RUPP","TYPE : MULTI-V408-0SE.T2A3/B",1]
[null,1.4,"GORMAN RUPP","PRIME CENTRIFUGAL PUMP,MODEL T3A3S/B 835-BFM",1]
[null,1.5,"GORMAN RUPP","SERIF PRIMING CERNTRIFUGAL PUMP,FRAME : T3A3S.8",1]
[null,1.6,"GORMAN RUPP","T6A3-B/FM",1]
[null,1.7,"GORMAN RUPP","SEEPEX GMBH,FRAME : T3A3S/B",1]
[null,1.8,"GORMAN RUPP","MODEL : T8A3-8/FM",1]
[null,1.9,"GORMAN RUPP","S/N 1386597 VS4A60.B",1]
[null,{"v":1.1,"d":"1.10"},"GORMAN RUPP","MODEL : T3A3S-B/FM,S/N : 1123760",1]
[null,1.11,"GORMAN RUPP","T3A3S/B,TYPE : BWP4-41HX,Q 252",1]
[null,1.12,"GORMAN-RUPP","SELF PRIMING CENTRIFUGAL PUMP,MODEL : T4A3S-B/FM",1]
[null,1.13,"GORMAN RUPP","22 KW / 1465 RPM /T3A3S.B\\FM",1]
[null,1.14,"GORMAN RUPP","22 ML/ 2490 RPM / 112D60-B",1]
[null,1.15,"GORMAN-RUPP","22 ML / 1450 RPM / 112D60-B 1",1]
[null,1.16,"GORMAN-RUPP","1347199N / T3A3S-B / 3TD 1",1]
[{"$nulls":3},"                                                     SERVICE KITS"]
[null,1.18,"GORMAN-RUPP","T3",1]
[null,1.19,"GORMAN-RUPP","T4",1]
[null,1.2,"GORMAN-RUPP","T8",1]
[null,1.21,"GORMAN-RUPP","VS4",1]
[null,1.22,"GORMAN-RUPP","VS6",1]
[{"$nulls":3},"                                                    ROTATING ASSEMBLES"]
[null,1.23,"GORMAN-RUPP","T3",1]
[null,1.24,"GORMAN-RUPP","T4",1]
[null,1.25,"GORMAN-RUPP","T8",1]
[null,1.26,"GORMAN-RUPP","VS4",1]
[null,1.27,"GORMAN-RUPP","VS6",1]
[null,1.28,"KSB","4 KW / 1440 RPM / ETA 100-200",1]
[null,1.29,"KSB","4 KW 11440 RPM / WKLN 65-6",1]
[null,1.3,"KSB KSB","100 KW / 525 V / KRTK 250400 4 UNGI„K",1]
[null,1.31,"KSB","/ KWPF 100",1]
[null,1.32,"KSB","S\\N-ZA0100S6/3 / ETA 65-200",1]
[null,1.33,"KSB","WKLn 50\\6 /",1]
[null,1.34,"KSB","ETA 50-125 /",1]
[null,1.35,"KSB","TYPE: MOVITEC V F090/042BID13ES200D5VW",1]
[null,1.36,"KSB","KRTK 200-402 (Margate)",1]
[null,1.37,"KSB","WKLn 40\\3\\",1]
[null,1.38,"KSB","110  / 1480 RPM / RWE-F200-400 ",1]
[null,1.39,"KSB","TYPE : WKLN 40/6",1]
[null,1.4,"KSB","TYPE : BWP44iHX",1]
[null,1.41,"KSB","TYPE KWP-KIOO",1]
[null,1.42,"KSB","TYPE KWPF 100-50,1MPELUAR DIA F/S",1]
[null,1.43,"KSB","TYPE : KWPF 100-250,1MPELLlAR DIA 210",1]
[null,1.44,"KSB","TYPE : KWPF 50 200",1]
[null,1.45,"KSB","88.42 KW / 1485 RPM / ETA 20040",1]
[null,1.46,"KSB","45,27 KW / 1490 RPM / ETA 150400",1]
[null,1.47,"KSB","1,5 KW / 940 RPM / KWP-K",1]
[null,1.48,"KSB","7,5 KW / 715 RPM /KWP-F150-315",1]
[null,1.49,"KSB","2,38 KW / 960 RPM / KWP 100\\250",1]
[null,1.5,"KSB","45 KW / 2950 RPM / 100GDL72-14XIO",1]
[null,1.51,"KSB","TYPE : KWPF 125-500",1]
[null,1.52,"KSB","TYPE : KWP.F150 315",1]
[null,1.53,"KSB","TYPE : KWPFIOO-25C",1]
[null,1.54,"KSB","11 KW / 1164 RPM / KWPF 80-250",1]
[null,1.55,"KSB","110 KW / 1480 RPM / KWPF",1]
[null,1.56,"KSB","630 KW / 1490 RPM / WH 200\\5",1]
[null,1.57,"KSB","ETA 40-250 /  99909938773/100/1",1]
[null,1.58,"KSB","ETA 100-250 /  9970500490/1-010703",1]
[null,1.59,"KSB","ETA 125-200 /  5289",1]
[null,1.6,"KSB","4334 / KWPF",1]
[null,1.61,"KSB","KW / 940 RPM / KWP-K 1",1]
[null,1.62,"KSB","12 ML / 1490 RPM / WLN 200\\5 1",1]
[null,1.63,"GRUNDFOS","TYPE : CRIO»08-A-FJ-A-E-HQQE",1]
[null,1.64,"GRUNDFOS","16SV11F110,CODE : 101511501,PN : 2500KPA,Q = 8-24METERCUBE/H",1]
[null,1.65,"GRUNDFOS","TYPE : CR32-1A-F-A.E-EUBE,MODEL : A9641018-2P3-Oi180002",1]
[null,1.66,"GRUNDFOS","MODEL : A9641018-2P3-01180002,Q = 30METERCUBE/H",1]
[null,1.67,"GRUNDFOS","WKS50-7",1]
[null,1.68,"GRUNDFOS","NT 125/315",1]
[null,1.69,"GRUNDFOS ","16 M/3:CRIS.10.11.O",1]
[null,1.7,null,"MOVITEC,S/N : 9971492954/200/2. REPLACED WITH MOVITEC V15/6",1]
[null,1.71,"GRUNDFOS","10,5 KW / 2900 RPM / CR16-100 A-F-A.AUUE. CR15-10. 11.0KW",1]
[null,1.72,"GRUNDFOS","11 KW / 2924 RPM / CR20-10 A-F-A.E-HOOE",1]
[null,1.73,"GRUNDFOS","75 KW / 1480 RPM / 150GDL 200-20X4",1]
[null,1.74,"GRUNDFOS","30 KW / 2950 RPM / IOOGDL72-14X6",1]
[null,1.75,"GRUNDFOS","15 KW / 2920 RPM / CR15-17-AFAE",1]
[null,1.76,"GRUNDFOS","MODEL : CR-80",1]
[null,1.77,"GROUNDFOS","11 KW/ 1450 RPM / Pilz 100\\2S0",1]
[null,1.78,"SULZER","TYPE BDc-300-400-D2,SERlAL NO : MP29351,RPM : 1480,POWER : 559.3KW",1]
[null,1.79,"SULZER","TYPE : SMH303-800,POWER :14DKW",1]
[null,1.8,"SUZLER","59 ML/ 1490 RPM / SMH 303-800",1]
[null,1.81,"SUZLER","21 ML / BDC-300-400",1]
[null,1.82,"IOWARA",{"v":101511471,"d":"101,511,471"},1]
[null,1.83,"IOWARA","155V08F095",1]
[null,1.84,"ROBORT","KW / 12 A",1]
[null,1.85,"ROBORT","KW / 4.1 A",1]
[null,1.86,"VOGEL","0.25 KW / KV250-25 / 80\\170",1]
[null,1.87,"PRO-PUMPS","MODEL :JS.IOO L",1]
[null,1.88,"MONO (FRANKLIN ELECTRIC)","MODEL : C41M/0004A",1]
[null,1.89,"Hidrostal","1.4KW / 1465rpm: A2QE4",1]
[null,1.9,"Hidrostal","1.8KW: A2QE2",1]
[null,1.91,"Hidrostal","2.6KW: BN3L02",1]
[null,1.92,"Hidrostal","2.8KW: D03U-SHN1+DN003X4",1]
[null,1.93,"Hidrostal","3.6KW: D03U-LHN1+DN003X2",1]
[null,1.94,"Hidrostal","4KW IMMERSIBLE (PENNINGTON 1): C03U-RL+CEYT2",1]
[null,1.95,"Hidrostal","4KW / 1340 RPM: C03U.LH+CNZY2",1]
[null,1.96,"Hidrostal","4.8KW: D03U.MHT1+DN004X2",1]
[null,1.97,"Hidrostal","5.5KW / 1410 RPM: D06U„SLU1+DN007X4",1]
[null,1.98,"Hidrostal","5.5KW: C03U-MHN1+CNYT2",1]
[null,1.99,"Hidrostal","7KW IMMERSIBLE (SEZELA): C03U-HHN3+CEYT2",1]
[null,1.1,"Hidrostal","7KW IMMERSIBLE (MALANGENi)",1]
[null,{"v":1.101,"d":"1.10"},"Hidrostal","7.5KW: D03U„MHN1+DN007X2",1]
[null,1.102,"Hidrostal","11.0KW",1]
[null,1.103,"Hidrostal","11.0KW IMMERSIBLE (BALANCING TANK)",1]
[null,1.104,"Hidrostal","13.SKW: DE4M-LMT3+EN014X2",1]
[null,1.105,"Hidrostal","22.0KW",1]
[null,1.106,"Hidrostal","50 KW",1]
[null,1.107,"Hidrostal","75.0KW IMMERSIBLE H05K-MH3R+HE090X4-GSEK1+NEIB60-10 and base plate",1]
[null,1.108,"Hidrostal","30 KW / 1470 RPM",1]
[null,1.109,"Hidrostal","H05K-S03R - I-IGMIX BEARING FRAME",1]
[null,{"v":1.11,"d":"1.110"},"Hidrostal","IOOKW H08G-MMU3+HN130-4 RIVER EXTRACTION PUMP",1]
[null,1.111,"HANSEN","GEAR-Boxes",1]
[null,1.112,"HANSEN","TYPE : RNB36AN / JB17002002",1]
[null,1.113,"ABS","18,7 KW / 1475 RPM / TYPE:RN36AN",1]
[null,1.114,"ABS","RPM / TYPE:RF40-R70",1]
[null,1.115,"ABS","0.37 KW / RPM /",1]
[null,1.116,"ABS","82,7 RPM / TYPE:RN3 2613 AN /  4018",1]
[null,1.117,"ABS","S/N : 1<141608 3004875479 /  F2M 128B-K4-(180)",1]
[null,1.118,"Flender Himmel","1410 RPM / TYPE FDA41-ZIO-MB4 /",1]
[null,1.119,"Flender Himmel","0,18 KW / 400 V / 1410 RPM",1]
[null,1.12,"Flender Himmel","TYPE : ZF108-K4-180",1]
[null,1.121,"Flender Himmel","TYPE : C514P P63",1]
[null,1.122,"Hansen","45 KW / 1475 RPM / TYPE:RND 36 AN",1]
[null,1.123,"Hansen","TYPE : NDP 903LP/LRGR225",1]
[null,1.124,"Getric Bauer ","TYPE :SK8382/32AFH-900",1]
[null,1.125,"Getric Bauer ","TYPE NDP 903LP\\GR225 / CODE:278 409 184 H0001",1]
[null,1.126,"Getric Bauer ","TYPE : DF61230MIB4 / RATIO-660:1 / 30 KW / ",1]
[null,1.127,"Getric Bauer ","TYPE:FF107LP200 /",1]
[null,1.128,"Getric Bauer ","TYPE : ZF148-K4-200",1]
[null,1.129,"Getric Bauer ","TYPE : FA77 ",1]
[null,{"v":1.13,"d":"1.130"},"Power Drives ","R42 OT71P4 4KW / 52 RPM /",1]
[null,1.131,"Power Drives ","/TYPE : FZM1688-K4-225",1]
[null,1.132,"Power Drives ","/ OIL:16L /",1]
[null,1.133,"Power Drives ","TYPE : RNC36 AN / ",1]
[null,1.134,"Power Drives ","TYPE : K88-K4-80 / ",1]
[null,1.135,"BMG","TYPE : JFN4B / ",1]
[null,1.136,"BMG","4CKW / FRAME:DG225MD /",1]
[null,1.137,"BMG","TYPE: D88-238-LA715A / 0,25 KW",1]
[null,1.139,"SIEMENS","11 KW / 1460 RPM",1]
[{"$nulls":3},"SECTION 2: VALVES"]
[null,2.1,"BUTTERFLY VALVES 250mm","GEARBOX RATIO 50:1",1]
[null,{"v":2.2,"d":"2.200"},"BUTTERFLY VALVES 300mm","GEARBOX RATIO 50:1",1]
[null,2.3,"BUTTERFLY VALVES 350mm","GEARBOX RATIO 50:1",1]
[null,2.4,"O-TEC","TYPE: FDA888-238-LA7184 / OIL: 6,8L / 1400 RPM 'RATIO: 27,13 {'OIL: 17,4L",1]
[null,2.5,"GORMAN RUPP","1Inch AIR RELEASE VALVE",1]
[null,2.6,"FLENDER HIMMEL RSA","/ TYPE: ZF1218K4{160) / RATIO: 27,13 / OIL: 22L",1]
[null,2.7,"RENOLD RENOLD","SIZE: GM4T / OUTPUT: 726 KW / 700 RPM",1]
[null,2.8,"RENOLD","SIZE: 40 / RATIO: 30:1 / SIZE: 40 / RATIO: 30:1 /",1]
[null,2.9,"ROBUSCH","TYPE: RVT60 / S\\N-E4119",1]
[null,2.1,"O-TEC","TYPE:ZF108-K4-132 / RATIO: 14,63 / OIL: 13,8L",1]
[null,{"v":2.11,"d":"2.1"},"O-TEC","TYPE: FZM148B-K2-180 / S\\N-JHK10093002150194 / RATIO:",1]
[null,{"v":2.12,"d":"2.1"},"VOSA","CRA/ PN4 / GHDC ",1]
[null,{"v":2.13,"d":"2.1"},"VOSA","DN400 SCPN",1]
[null,2.14,"VOSA","VIV272 664 22705",1]
[null,2.15,"VOSA","DN200",1]
[null,2.16,"VOSA","CF EUR016 LIC PAM",1]
[null,2.17,"VOSA","DN250 / PN16",1]
[null,2.18,"VOSA","DN 250 / PN 16/ 664",1]
[null,2.19,"VOSA","DN 100 / PN 16/ GGG",1]
[null,{"v":2.2,"d":"2.20"},"VOSA","DN150/ PN16 /GGG",1]
[null,2.21,"VOSA","DN 250 / PN 16/",1]
[null,2.22,"VOSA","AH5 / RIGHT/6135 /DN 250",1]
[null,2.23,"VOSA","AH51551",1]
[null,2.24,"VOSA","CF664",1]
[null,2.25,"VOSA","CF 21 10043 T7",1]
[null,2.26,"VOSA","CF 100 B162",1]
[null,2.27,"VOSA","CF 21 IOOB4W7",1]
[null,2.28,"VOSA","CF 2L 100 A4V7",1]
[null,2.29,"VOSA","CF 21 100 5)'",1]
[null,{"v":2.3,"d":"2.30"},"VOSA","DN 100 /PN 16/ SG",1]
[null,2.31,"VOSA","DN 100 /PNIO DIOO",1]
[null,2.32,"VOSA","DNIOO/ PN16/TYPE:55 130 705",1]
[null,2.33,"VOSA","DNIOO/ ?N18",1]
[null,2.34,"VOSA","TYPE : 6WW -125",1]
[null,2.35,"VOSA","CF 1080 BiD8",1]
[null,2.36,"VOSA","CF 1080 B2U8",1]
[null,2.37,"VOSA","CF 1080 IB4K7",1]
[null,2.38,"VOSA","CF 1080 16B4K7",1]
[null,2.39,"VOSA","CFDL 100 PN16",1]
[null,{"v":2.4,"d":"2.40"},"VOSA","DN 80 / PN16 SG",1]
[null,2.40999999999999,"VOSA","DN 50 /PN 16/ SG",1]
[null,{"v":2.41999999999999,"d":"2.42"},"VOSA","B53464",1]
[null,2.42999999999999,"VOSA","664 PN16",1]
[null,{"v":2.43999999999999,"d":"2.44"},"VOSA","MODEL:3840VF /",1]
[null,2.44999999999999,"VOSA","PN40 / C\\80",1]
[null,{"v":2.45999999999999,"d":"2.46"},"VOSA","DNIOO PN16/ WA12 664",1]
[null,2.46999999999999,"VOSA","CF 2L 100 IOX5",1]
[null,{"v":2.47999999999999,"d":"2.48"},"VOSA","38344-004D",1]
[null,2.48999999999999,"VOSA","AVK / DNIOO /PN16",1]
[null,{"v":2.49999999999999,"d":"2.50"},"VOSA","SABS664 PN16/ Dl",1]
[null,2.50999999999999,"VOSA","D62-75 DN DN2 EPDM",1]
[null,{"v":2.51999999999999,"d":"2.52"},"VOSA","LRC 555-RES-SG",1]
[null,2.52999999999999,"VOSA","/ DISC:SG62 / BODY:5642",1]
[null,{"v":2.53999999999999,"d":"2.54"},"VOSA","DNIOO /  3PLO\\4489 / MODEL .• 4770v",1]
[null,2.54999999999999,"VOSA","PN400",1]
[null,{"v":2.55999999999999,"d":"2.56"},"VOSA","PN16 / DN8C",1]
[null,2.56999999999999,"VOSA","DN150 /PN16/C1/ REFLELUX/VB104",1]
[null,{"v":2.57999999999999,"d":"2.58"},"VOSA","PN16 / DN80",1]
[null,2.58999999999999,"VOSA","DNIOO / PN25",1]
[null,{"v":2.59999999999999,"d":"2.60"},"VOSA","DN150 / PN25",1]
[null,2.60999999999999,"VOSA ","3Inch PN16 NRV COUNTER WEIGHT T/D",1]
[null,{"v":2.61999999999999,"d":"2.62"},"VOSA ","4Inch PN16 NRV COUNTER WEIGHT T/D",1]
[null,2.62999999999999,"VOSA ","6Inch PN16 NRV COUNTER WEIGHT T/D",1]
[null,{"v":2.63999999999999,"d":"2.64"},"VOSA","DN 150 / \"NIS",1]
[null,2.64999999999999,"ROCKWEN","IES 1585 SG",1]
[null,{"v":2.65999999999999,"d":"2.66"},"ROCKWEN","DN 150",1]
[null,2.66999999999999,"ROCKWEN","KW PN16 DN150",1]
[null,{"v":2.67999999999999,"d":"2.68"},"ROCKWEN","OY1207 / SABS664 PN16\\SG",1]
[null,2.68999999999999,"ROCKWEN","PN 25W 664 VAG",1]
[null,{"v":2.69999999999999,"d":"2.70"},"ROCKWEN","DN80 / PN16/ LIC PAM",1]
[null,2.70999999999999,"ROCKWEN","DN200 PNZ46",1]
[null,{"v":2.71999999999999,"d":"2.72"},"ROCKWEN","DN150/ PN16 /SG 121223-1",1]
[null,2.72999999999999,"ROCKWEN","CFIOO BIL2 KRO",1]
[null,{"v":2.73999999999999,"d":"2.74"},"ROCKWEN","CFIOO 8164 NO",1]
[null,2.74999999999999,"ROCKWEN","CFIOO B164 ZO",1]
[null,{"v":2.75999999999999,"d":"2.76"},"ROCKWEN","CFIOO 8164 YO",1]
[null,2.76999999999999,"BERMAD","24 V DC / W / 170mA /",1]
[null,{"v":2.77999999999999,"d":"2.78"},"NEWAY","3 /300 / WCB /P247K",1]
[null,2.78999999999998,"NEWAY","DN80/ PN25/ JS030",1]
[null,{"v":2.79999999999999,"d":"2.80"},"NEWAY","DN250 / PN16 /UNI-FIO",1]
[null,2.80999999999998,"NEWAY","DN2SO / ELVP 50",1]
[null,{"v":2.81999999999999,"d":"2.82"},"NEWAY","DN150 PATT 55/2",1]
[null,2.82999999999998,"NEWAY","DN130 / PN16",1]
[null,{"v":2.83999999999998,"d":"2.84"},"NEWAY","VIV 414 / DN150 / SG42",1]
[null,2.84999999999998,"NEWAY","DN 150 /VIV 398 / SC42",1]
[null,{"v":2.85999999999998,"d":"2.86"},"NEWAY","DN150 / FL PNIO-16\\EP-EP",1]
[null,2.86999999999998,"NEWAY","DN250 / PN16 /SG\\091010",1]
[null,{"v":2.87999999999998,"d":"2.88"},"NATCO","PATTI-2",1]
[null,2.88999999999998,"NATCO","201 / MODEL:SFV-W",1]
[null,{"v":2.89999999999998,"d":"2.90"},"EAST-RAND BERMAD","DN400 / PN25 /",1]
[null,2.90999999999998,"UVONGO P/S 2","DN200 / CLASS 16",1]
[null,{"v":2.91999999999998,"d":"2.92"},"VOSA","PN16 / DNIOO",1]
[null,2.92999999999998,"KAIZERS P/S","/ DN150",1]
[null,{"v":2.93999999999998,"d":"2.94"},"KAIZERS P/S","PN15 / ONIOO",1]
[null,2.94999999999998,"KAIZERS P/S","FL.PNIO.16\\EP-EP / DN150",1]
[null,{"v":2.95999999999998,"d":"2.96"},"BERMAD","16,7 W / 220 V / S\\N: 1370120004",1]
[null,2.96999999999998,"UNI-FLO","PN16 / DN50",1]
[null,{"v":2.97999999999998,"d":"2.98"},"NS","DN 80/PN16 SABS 664 RSV C/W HANDWHEEL CLOCKWISE CLOSING.NRS",1]
[null,2.98999999999998,"NS","DNIOO/PN16 SABS 664 RSV C/W HANDWHEEL CLOCKWISE CLOSING.NRS",1]
[null,2.1,"NS","DN150/PN16 SAes 664 RSV C/W HANDWHEEL CLOCKWISE CLOSWG.NRS",1]
[null,2.101,"NS","DN200/PN16 SABS 664 RSV C/W HANDWHEEL CLOCKWISE CLOSING.NRS",1]
[null,2.102,"NS","DN250/PN16 SABS 664 RSV C/W HANDWHEEL CLOCKWISE CLOSING.NRS",1]
[null,2.103,"NS","DN300/PN16 SABS 664 RSV C/W HANDWHEEL CLOCKWISE CLOSING.NRS",1]
[null,2.104,"NS","DN350/PN16 SABS 664 RSV C/W HANDWHEEL CLOCI<WISE CLOSING.NRS",1]
[null,2.105,"NS","DN400/PN16 SABS 664 RSV C/W HANDWHEEL CLOCKWISE CLOSING.NRS",1]
[null,2.106,"VOSA","DN80/PN16 SABS 616154 C/' GUNMETAL TRIM INC LEVER & WEIGHT",1]
[null,2.107,"VOSA","DNIOO/PN16 SABS 616154 C/l GUNMETAL TRIM INC LEVER & WEIGHT",1]
[null,2.108,"VOSA","DN150/PN16 SABS 616154 C/' GUNMETAL TRIM INC LEVER & WEIGHT",1]
[null,2.109,"VOSA","DN200/PN16 SABS 616154 C/l GUNMETAL TRIM  LEVER & WEIGHT",1]
[null,2.11,"VOSA","DN250/PN16 SABS 616154 C/l GUNMETAL TRIM INC LEVER & WEIGHT",1]
[null,2.111,"VOSA","DN300/PN16 SABS 616154 C/l GUNMETAL TRIM INC LEVER & WEIGHT",1]
[null,2.112,"VOSA","DN350/PN16 SABS 616154 C/' GUNMETAL TRIM  LEVER & WEIGHT",1]
[null,2.113,"VOSA","DN400/PN16 SABS 616154 C/' GUNMETAL TRIM INC LEVER & WEIGHT",1]
[{"$nulls":3},"Section 3: Motors Electrical "]
[null,3.1,"WEG","75KW / 140 A/ 1475 rpm /380V / DG250M",1]
[null,3.2,"WEG","110 KW / 2970 RPM / 196\\113 A/ 380 V",1]
[null,3.3,"WEG","30 KW /2940 RPM / 56 A / 2001",1]
[null,3.4,"WEG","22 KW /2940 RPM / 39 A / 400V",1]
[null,3.5,"WEG","55 KW / 11 A/ 2960 RPM / FRAME:112/  SON 4431",1]
[null,3.6,"WEG","37 KW/ 1470 RPM / 70 2 A/ 380 V",1]
[null,3.7,"WEG","0,37 KW / 890 RPM / 380V / 1,08 A",1]
[null,3.8,"WEG","22 KW / 1455 RPM / DX180LD",1]
[null,3.9,"WEG","7,5 KW / 1435 RPM / 6,6 A/ DX32M",1]
[null,{"v":3.1,"d":"3.10"},"WEG","15 KW / 1460 RPM / 28 7 A / 4COV / Y3-160L„4B3PTC",1]
[null,3.11,"WEG","0,55 KW / 1105 RPM / 2,67 A/ 80'.",1]
[null,3.12,"WEG","4 KW/ 1430 RPM / A/ 112M",1]
[null,3.13,"WEG","90 KW / 1480 RPM / 158 A/ 400 V /FRAME : IL 2805/M1/4 B2",1]
[null,3.14,"WEG","132 KW / 244 A / 380 V / D31S /  : GRB1738/2",1]
[null,3.15,"WEG","2,2 KW / 2850 RPM / FRAME:DA90LZ-H",1]
[null,3.16,"WEG","5,5 KW / 2910 RPM / 10,8 A/  / FRAME:1325",1]
[null,3.17,"WEG","3 KW / 2900 RPM / 6 35 A/ 380 V /MG 100 tA2-28FT130-D2",1]
[null,3.18,"WEG","11 KW / 2880 RPM / 21,5 A/ 380 V/",1]
[null,3.19,"WEG","110 KW / 1480 RPM / 217 A/ 380 V / D280M / S\\N-GRB198812",1]
[null,{"v":3.2,"d":"3.20"},"WEG","22 KW / 2910 RPM / 42 A/ 380 V",1]
[null,3.21,"WEG","11 KW / 1164 RPM / 400 V / 13-160L683PTO",1]
[null,3.22,"WEG","22 KW / 1465 RPM/ i00M / 380 V",1]
[null,3.23,"WEG","30 KW / 1470 RPM / 58,5 A/ 380 V / 200A",1]
[null,3.24,"WEG","5,5 KW / 1460 RPM / 6,56 A/ 132S",1]
[null,3.25,"WEG","45 KW / 2965 RPM / 82 A / 2255\\M",1]
[null,3.26,"WEG","3 KW / 1410 RPM / 14001 2-4",1]
[null,3.27,"WEG","3 KW / 1470 RPM / 43,6 A/ 1801",1]
[null,3.28,"WEG","0,55 KW / 1390 RPM / A / 400 V / CAD 68/M71MB4",1]
[null,3.29,"WEG","1,5 kw / 1400 RPM / FDAF108D-M90L4",1]
[null,{"v":3.3,"d":"3.30"},"WEG","15 KW / 2935 RPM / 380 V",1]
[null,3.31,"WEG","11 KW / 1465 RPM /  20038EAJ",1]
[null,{"v":3.31999999999999,"d":"3.32"},"WEG","1,5 KW / 940 RPM / 3,8 A/ 400 V",1]
[null,3.33,"WEG","18,5 KW / 1465 RPM / 39,6 A/ 400 V / 180M",1]
[null,{"v":3.33999999999999,"d":"3.34"},"WEG","5,5 KW / 960 RPM / 400\\690V / 132M",1]
[null,3.35,"WEG","75 KW / 2960 RPM / 76,6 A / 380 V",1]
[null,{"v":3.35999999999999,"d":"3.36"},"WEG","0,75 KW / 1440 RPM / 801",1]
[null,{"v":3.36999999999999,"d":"3.37"},"WEG","3 KW / 1410 RPM / 14001 2-4",1]
[null,{"v":3.37999999999999,"d":"3.38"},"WEG","22 KW / 1460 RPM / 42,9 A/ 180L",1]
[null,{"v":3.38999999999999,"d":"3.39"},"WEG","7,5 KW / 725 RPM / 18 A/ DZ1601",1]
[null,{"v":3.39999999999999,"d":"3.40"},"WEG","3 KW / 1470 RPM / 43,6 A/ 1801",1]
[null,{"v":3.40999999999999,"d":"3.41"},"WEG","0,55 KW / 1390 RPM / A / 400 V / CAD 68/M71MB4",1]
[null,{"v":3.41999999999999,"d":"3.42"},"WEG","1,5 kw / 1400 RPM / FDAF108D-M90L4",1]
[null,{"v":3.42999999999999,"d":"3.43"},"WEG","15 KW / 2935 RPM / 380 V",1]
[null,{"v":3.43999999999999,"d":"3.44"},"WEG","11 KW / 1465 RPM /  20038EAJ",1]
[null,{"v":3.44999999999999,"d":"3.45"},"WEG","75 KW / 1470 RPM /  A/ 250S\\M",1]
[null,{"v":3.45999999999999,"d":"3.46"},"WEG","0,75 KW / 1380 RPM / 2,05 A/ IP55",1]
[null,{"v":3.46999999999999,"d":"3.47"},"WEG","1,5 KW / 940 RPM / 3,8 A/ 400 V",1]
[null,{"v":3.47999999999999,"d":"3.48"},"WEG","7,5 KW / 1450 RPM / 15,1 A / 380 V",1]
[null,{"v":3.48999999999999,"d":"3.49"},"WEG","18,5 KW / 1465 RPM / 39,6 A/ 400 V / 180M",1]
[null,{"v":3.49999999999999,"d":"3.50"},"WEG","5,5 KW / 960 RPM / 400\\690V / 132M",1]
[null,{"v":3.50999999999999,"d":"3.51"},"W EG","2,2 KW / 2855 RPM / A /200-240 V",1]
[null,{"v":3.51999999999999,"d":"3.52"},"WEG","18,5 KW / 2940 RPM / 34,5 A / 380 V",1]
[null,{"v":3.52999999999999,"d":"3.53"},"WEG","5,5 KW / 12 A /525 V / S\\N-HKD122",1]
[null,{"v":3.53999999999999,"d":"3.54"},"WEG","15 KW / 1460 RPM / 30 A / MLSA160-4",1]
[null,{"v":3.54999999999999,"d":"3.55"},"WEG","18,5 KW / 1465 RPM / 36,4 A /180M",1]
[null,{"v":3.55999999999999,"d":"3.56"},"WEG","22 KW / 1465 RPM / 42,5 A / TH.Cl.155(F)",1]
[null,{"v":3.56999999999999,"d":"3.57"},"WEG","4 KW / 2880 RPM / 7/3 A ",1]
[null,{"v":3.57999999999999,"d":"3.58"},"WEG","11 KW / 2945 RPM / 20 A/ 380-400 V ",1]
[null,{"v":3.58999999999999,"d":"3.59"},"WE-G","7,5 KW / 2910 RPM / 14,3 A/ 132S ",1]
[{"$nulls":3},"Section 4: Electrical small component"]
[null,4.1,"ABB","A95-30",1]
[null,4.2,"ABB","A75-30",1]
[null,4.3,"ABB","A50-30",1]
[null,4.4,"ABB","AF09-30-10-13",1]
[null,4.5,"ABB","100-250 V „'AF140-30 / S\\N-1516011211132S1399",1]
[null,4.6,"ABB","230-240 V / E8B24-40",1]
[null,4.7,"ABB","110 V / A145-30",1]
[null,4.8,"ABB","CA5-22E",1]
[null,4.9,"SCHNEIDER ELECTRIC","LCID09/220V coll",1]
[null,{"v":4.1,"d":"4.10"},"SCHNEIDER ELECTRIC","LCID12/220V coil",1]
[null,4.11,"SCHNEIDER ELECTRIC","LCID18/220V",1]
[null,4.12,"SCHNEIDER ELECTRIC","LCID25/220V coil",1]
[null,4.13,"SCHNEIDER ELECTRIC","LCID32/220V coil",1]
[null,4.14,"SCHNEIDER ELECTRIC","LCID40/220V",1]
[null,4.15,"SCHNEIDER ELECTRIC","LCID50/220V coil",1]
[null,4.16,"SCHNEIDER ELECTRIC","LCID65/22CV coll",1]
[null,4.17,"SCHNEIDER ELECTRIC","LCID80/220V",1]
[null,{"v":4.18000000000001,"d":"4.18"},"SCHNEIDER ELECTRIC","LCID95/220V",1]
[null,{"v":4.19000000000001,"d":"4.19"},"SCHNEIDER ELECTRIC","LC1G115KUEN",1]
[null,{"v":4.2,"d":"4.20"},"SCHNEIDER ELECTRIC","LC1G150KUEN",1]
[null,4.21,"SCHNEIDER ELECTRIC","LC1G185KUEN",1]
[null,{"v":4.21999999999998,"d":"4.22"},"SCHNEIDER ELECTR'C","LC1G22KUEN",1]
[null,{"v":4.22999999999997,"d":"4.23"},"LOVATO","230 V / BF5000X4",1]
[null,{"v":4.23999999999996,"d":"4.24"},"LOVATO","230 V / BFK2600A",1]
[null,{"v":4.24999999999995,"d":"4.25"},"LOVATO","10 A/ BFK3800A",1]
[null,{"v":4.25999999999994,"d":"4.26"},"LOVATO","380 V / 10 A/ BFI<12",1]
[null,{"v":4.26999999999993,"d":"4.27"},"ALLEN BRADLEY","230 V/32A",1]
[null,{"v":4.27999999999992,"d":"4.28"},"HASCONGH","24 V / CJX2099",1]
[null,{"v":4.28999999999991,"d":"4.29"},"Schneider Electric","ADD-ON BLOCKS LADN11",1]
[null,{"v":4.2999999999999,"d":"4.30"},"Schneider Electric","LADN13",1]
[null,{"v":4.30999999999989,"d":"4.31"},"Schneider Electric","LADN22",1]
[null,{"v":4.31999999999988,"d":"4.32"},"Schneider Electric","LADN31",1]
[null,{"v":4.32999999999987,"d":"4.33"},"Schneider Electric","LRD01",1]
[null,{"v":4.33999999999986,"d":"4.34"},"Schneider Electric","LRD14",1]
[null,{"v":4.34999999999985,"d":"4.35"},"Schneider Electric","LRD16",1]
[null,{"v":4.35999999999984,"d":"4.36"},"Schneider Electric","LRD21",1]
[null,{"v":4.36999999999983,"d":"4.37"},"Schneider Electric","LRD22",1]
[null,{"v":4.37999999999982,"d":"4.38"},"Schneider Electric","LRD32",1]
[null,{"v":4.38999999999981,"d":"4.39"},"Schneider Electric","LRD365",1]
[null,{"v":4.3999999999998,"d":"4.40"},"Schneider Electric","LRD3363",1]
[null,{"v":4.40999999999979,"d":"4.41"},"Schneider Electric","LRD3355",1]
[null,{"v":4.41999999999978,"d":"4.42"},"Schneider Electric","LRD3357",1]
[null,{"v":4.42999999999977,"d":"4.43"},"Schneider Electric","LRD3363",1]
[null,{"v":4.43999999999976,"d":"4.44"},"Schneider Electric","IRD3365",1]
[null,{"v":4.44999999999975,"d":"4.45"},"Schneider Electric","LRD01",1]
[null,{"v":4.45999999999974,"d":"4.46"},"Schneider Electric","LRD02",1]
[null,{"v":4.46999999999973,"d":"4.47"},"Schneider Electric","LRD03",1]
[null,{"v":4.47999999999972,"d":"4.48"},"Schneider Electric","LRD04",1]
[null,{"v":4.48999999999971,"d":"4.49"},"Schneider Electric","LRD05",1]
[null,{"v":4.4999999999997,"d":"4.50"},"Schneider Electric","LRD06",1]
[null,{"v":4.50999999999969,"d":"4.51"},"Schneider Electric","LRD07",1]
[null,{"v":4.51999999999968,"d":"4.52"},"Schneider Electric","LRD08",1]
[null,{"v":4.52999999999967,"d":"4.53"},"Schneider Electric","LRD12",1]
[null,{"v":4.53999999999966,"d":"4.54"},"Schneider Electric","LRD35",1]
[null,{"v":4.54999999999965,"d":"4.55"},"Schneider Electric","LRD3322",1]
[null,{"v":4.55999999999964,"d":"4.56"},"Schneider Electric","LRD3353",1]
[null,{"v":4.56999999999963,"d":"4.57"},"Schneider Electric","LRD3359",1]
[null,{"v":4.57999999999962,"d":"4.58"},"Schneider Electric","LRD3361",1]
[null,{"v":4.58999999999961,"d":"4.59"},"Schneider Electric","LRD4365",1]
[null,{"v":4.5999999999996,"d":"4.60"},"Schneider Electric","LRD4367",1]
[null,{"v":4.60999999999959,"d":"4.61"},"Schneider Electric","LRD4369",1]
[null,{"v":4.61999999999958,"d":"4.62"},"Schneider Electric","LRD 33696",1]
[null,{"v":4.62999999999957,"d":"4.63"},"Schneider Electric","LRD1508",1]
[null,{"v":4.63999999999956,"d":"4.64"},"Schneider Electric","LRD1510",1]
[null,{"v":4.64999999999955,"d":"4.65"},"Schneider Electric","LRD1512",1]
[null,{"v":4.65999999999954,"d":"4.66"},"Schneider Electric","LRD1514",1]
[null,{"v":4.66999999999953,"d":"4.67"},"Schneider Electric","LRD1516",1]
[null,{"v":4.67999999999952,"d":"4.68"},"Schneider Electric","LRD1521",1]
[null,{"v":4.68999999999951,"d":"4.69"},"Schneider Electric","LRD1522",1]
[null,{"v":4.6999999999995,"d":"4.70"},"Schneider Electric","LRD1530",1]
[null,{"v":4.70999999999949,"d":"4.71"},"Schneider Electric","LRD1532",1]
[null,{"v":4.71999999999948,"d":"4.72"},"Schneider Electric","GV2ME03",1]
[null,{"v":4.72999999999947,"d":"4.73"},"Schneider Electric","GV2ME04",1]
[null,{"v":4.73999999999946,"d":"4.74"},"Schneider Electric","GV2ME-21",1]
[null,{"v":4.74999999999945,"d":"4.75"},"Schneider Electric","GV2ME05",1]
[null,{"v":4.75999999999944,"d":"4.76"},"Schneider Electric","GV2ME02",1]
[null,{"v":4.76999999999943,"d":"4.77"},"Schneider Electric","GV2ME10 / 400/415V / RANGE .• 4-6,3A",1]
[null,{"v":4.77999999999942,"d":"4.78"},"Schneider Electric","GV2ME06",1]
[null,{"v":4.78999999999941,"d":"4.79"},"Schneider Electric","GV2ME 08 / RANGE : 2,5-4A",1]
[null,{"v":4.7999999999994,"d":"4.80"},"Schneider Electric","GV3P65",1]
[null,{"v":4.80999999999939,"d":"4.81"},"Schneider Electric","GV2ME16 / 9-14A /380V",1]
[null,{"v":4.81999999999938,"d":"4.82"},"Schneider Electric","GV3P5O",1]
[null,{"v":4.82999999999937,"d":"4.83"},"Schneider Electric","GV2ME32",1]
[null,{"v":4.83999999999936,"d":"4.84"},"Schneider Electric","690 V / GV2ME16",1]
[null,{"v":4.84999999999935,"d":"4.85"},"Schneider Electric","GV2ME14",1]
[null,{"v":4.85999999999934,"d":"4.86"},"Schneider Electric","GV3P40",1]
[null,{"v":4.86999999999933,"d":"4.87"},"Schneider Electric","GV2ME07",1]
[null,{"v":4.87999999999932,"d":"4.88"},"Schneider Electric","GV2ME20",1]
[null,{"v":4.88999999999931,"d":"4.89"},"CBI","10 amp single pole circuit breaker",1]
[null,{"v":4.8999999999993,"d":"4.90"},"CBI","15 amp single pole circuit breaker",1]
[null,{"v":4.90999999999929,"d":"4.91"},"CBI","20 amp single pole circuit breaker",1]
[null,{"v":4.91999999999928,"d":"4.92"},"CBI","25 amp single pole circuit breaker",1]
[null,{"v":4.92999999999927,"d":"4.93"},"CBI","5 amp single pole circuit breaker",1]
[null,{"v":4.93999999999926,"d":"4.94"},"Schneider Electric","MAGNETIC CIRCUIT BRÉAKERS"]
[null,{"v":4.94999999999925,"d":"4.95"},"Schneider Electric","GV-L03",1]
[null,{"v":4.95999999999924,"d":"4.96"},"Schneider Electric","GV2-LE04",1]
[null,{"v":4.96999999999923,"d":"4.97"},"Schneider Electric","GV2L04",1]
[null,{"v":4.97999999999922,"d":"4.98"},"Schneider Electric","GV2-LE05",1]
[null,{"v":4.98999999999921,"d":"4.99"},"Schneider Electric","GV2-L05",1]
[null,{"v":4.1,"d":"4.100"},"Schneider Electric","GV2-LE06",1]
[null,4.101,"Schneider Electric","GV2-L06",1]
[null,4.102,"Schneider Electric","GV2-LE07",1]
[null,4.103,"Schneider Electric","GV2-L07",1]
[null,4.104,"Schneider Electric","GV2-LE08",1]
[null,4.105,"Schneider Electric","GV2-L08",1]
[null,4.106,"Schneider Electric","GV3-L50",1]
[null,4.107,"Schneider Electric","GV3-L80",1]
[null,4.109,"Schneider Electric","GV2-LE14",1]
[null,{"v":4.11,"d":"4.110"},"Schneider Electric","GV3-L65",1]
[null,4.111,"Schneider Electric","GV2-LE16",1]
[null,4.112,"Schneider Electric","GV2-L16",1]
[null,4.113,"Schneider Electric","GV2-LE20",1]
[null,4.114,"Schneider Electric","GV2L20",1]
[null,4.115,"Schneider Electric","GV2-LE22",1]
[null,4.116,"Schneider Electric","GV3-L40",1]
[null,{"v":4.11700000000001,"d":"4.117"},"Schneider Electric","GV2-L32",1]
[null,{"v":4.11800000000001,"d":"4.118"},"Schneider Electric","GV2-LE32",1]
[{"$nulls":3},"Section 5: Motor control panels"]
[null,5.1,"Schneider ","2. 6 kw motor control panel as per Ugu spec",1]
[null,5.2,"Schneider ","7.5 kw motor control panel as per Ugu spec",1]
[null,5.3,"Schneider ","11 kw motor control panel as per Ugu spec",1]
[null,5.4,"Schneider ","22 kw motor control panel as per Ugu spec",1]
[null,5.5,"Schneider ","30 kw motor control panel as per Ugu spec",1]
[null,5.6,"Schneider ","45 kw motor control panel as per Ugu spec",1]
[null,5.7,"Schneider ","75 kw motor control panel as per Ugu spec",1]
[null,5.8,"Schneider ","110 kw motor control panel as per Ugu spec",1]
[{"$nulls":3},"Section 6: Push buttons"]
[null,6.1,"Scheneider  Electric "," XB7NA21",1]
[null,6.2,"Scheneider  Electric ","XB7NA25",1]
[null,6.3,"Scheneider  Electric ","XB7NA31",1]
[null,6.4,"Scheneider  Electric ","XB7NA42",1]
[null,6.5,"Scheneider  Electric ","XB7NA35",1]
[null,6.6,"Scheneider  Electric ","XB7NA81",1]
[{"$nulls":3},"Section 7: Transformers "]
[null,7.1,"Alsthom or similar","11kv /3,3 kv 1600kva open bushing ",1]
[null,7.2,"Alsthom or similar","22kv / 3.3kv 1600 kva open bushing ",1]
[null,7.3,"Alsthom or similar","11kv /400 volt 100kva minisub type enclosed",1]
[null,7.4,"Alsthom or similar","11kv /400 volt 200kva minisub type enclosed",1]
[null,7.5,"Alsthom or similar","11kv /400 volt 350kva minisub type enclosed",1]
[null,7.6,"Alsthom or similar","11kv /400 volt 500kva minisub type enclosed",1]
[null,7.7,"Alsthom or similar","11kv /400 volt 650kva minisub type enclosed",1]
[{"$nulls":3},"                                                                     Section 8: Conduit"]
[null,8.1,"ACDC ","20 MM",1]
[null,8.2,"ACDC ","25MM",1]
[null,8.3,"ACDC ","32MM",1]
[{"$nulls":3},"                                                                       Section 9: Trunking"]
[null,9.1,"ACDC ","16x16MM",1]
[null,9.2,"ACDC ","25X25MM",1]
[null,9.3,"ACDC ","40X40MM",1]
[null,9.4,"ACDC ","100X100MM",1]
[{"$nulls":3},"Section 10 : PVC Round boxes"]
[null,10.1,"ACDC ","one way 20MM",1]
[null,10.2,"ACDC ","Two way 20MM",1]
[null,10.3,"ACDC ","Three way 20MM",1]
[null,10.4,"ACDC ","Four way 20MM",1]
[null,10.5,"ACDC ","U box 20MM",1]
[null,10.6,"ACDC ","Y box 20MM",1]
[null,10.7,"ACDC ","Adapter male 20MM",1]
[null,10.8,"ACDC ","Female adapter 20MM",1]
[{"$nulls":3},"Section 11: HILTY'S"]
[null,11.1,"Fischer","6x35MM",1]
[null,11.2,"Fischer","6X50MM",1]
[{"$nulls":3},"Section 12:  Socket Outlets "]
[null,12.1,"Crabtree","4 x 2 switched socket outlet",1]
[null,12.2,"Crabtree","4 x 4 x 2 switched socket outlet",1]
[null,12.3,"Crabtree"," (DEDICATED PLUG) BLUE",1]
[null,12.4,"Crabtree","4x4x2 (DEDICATED socket) blue",1]
[null,12.5,"Crabtree","4x4x2(DEDICATED socket) RED",1]
[{"$nulls":3},"Section 13: Cables Single Phase "]
[null,13.1,"Aberdare or similar","1.5 mm x 2 core +earth round surfix/100m",1]
[null,13.2,"Aberdare or similar","2.5 mm x 2 core +earth round surfix/100m",1]
[null,13.3,"Aberdare or similar","4 mm x 4 core +earth round surfix/100m",1]
[null,13.4,"Aberdare or similar","1.5 mm x 4 core +earth round surfix/100m",1]
[null,13.5,"Aberdare or similar","2.5 mm x 4 core +earth round surfix/100m",1]
[null,13.6,"Aberdare or similar","70MM FLEX WIRE/M",1]
[null,13.7,"Aberdare or similar","95MM FLEX WIRE/M",1]
[{"$nulls":3},"Section 14: Amoured Cables "]
[null,14.1,"Aberdare or similar"," 1,5MM * 4 CORE ECC /METER",1]
[null,14.2,"Aberdare or similar","2,5MM * 4 CORE ECC [METER",1]
[null,14.3,"Aberdare or similar","4MM 4 CORE ECC /METER",1]
[null,14.4,"Aberdare or similar","6MM * 4 CORE ECC/METER",1]
[null,14.5,"Aberdare or similar","IOMM * 4 CORE ECC/METER",1]
[null,14.6,"Aberdare or similar","16MM * 4 CORE ECC/METER",1]
[null,14.7,"Aberdare or similar","25MM * 4 CORE ECC/METER",1]
[null,14.8,"Aberdare or similar","35MM * 4 CORE ECC/METER",1]
[null,14.9,"Aberdare or similar","50MM * 4 CORE ECC/METER",1]
[null,{"v":14.1,"d":"14.10"},"Aberdare or similar","70MM * 4 CORE ECC/METER",1]
[null,14.11,"Aberdare or similar","95MM * 4 CORE ECC/METER",1]
[{"$nulls":3},"Section 15: Glands "]
[null,15.1,"CCG","NUMBER ZERO",1]
[null,15.2,"CCG","NUMBER ONE",1]
[null,15.3,"CCG","NUMBER TWO",1]
[null,15.4,"CCG","NUMBER THREE",1]
[null,15.5,"CCG","NUMBER FOUR",1]
[null,15.6,"CCG","NUMBER FIVE",1]
[{"$nulls":3},"Section 16: Joint  kits"]
[null,16.1,"3M scotchgaurd","NUMBER ZERO",1]
[null,16.2,"3M scotchgaurd","NUMBER ONE",1]
[null,16.3,"3M scotchgaurd","NUMBER TWO",1]
[null,16.4,"3M scotchgaurd","NUMBER THREE",1]
[null,16.5,"3M scotchgaurd","NUMBER FOUR",1]
[null,16.6,"3M scotchgaurd","PVC GLUE",1]
[null,16.7,"3M scotchgaurd","SILICON WHITE",1]
[null,16.8,"3M scotchgaurd","SILICON GUN",1]
[null,16.9,"3M scotchgaurd","RUBBER TAPE",1]
[null,16.1,"3M scotchgaurd","6mm raw' bolt",1]
[null,16.11,"3M scotchgaurd","8mm rawl bolt",1]
[null,16.12,"3M scotchgaurd","10 mm rawl bolt",1]
[{"$nulls":3},"Section 17:  Light fittings"]
[null,17.1,"3M scotchgaurd"," 200 w LED FLOOD LIGHT",1]
[null,17.2,"Nordeland"," 4 foot led FITTING WEATHER PROOF",1]
[null,17.3,"Osram","pin type led 220 volt bulb",1]
[null,17.4,"Osram","screw type led 220 volt bulb",1]
[null,17.5,"Osram","2FOOT led 220 volt florescent tube",1]
[null,17.6,"Osram","4FOOT led 220 volt (florescent tube)",1]
[null,17.7,"Osram","5FOOT led 220 volt ( florescent tube)",1]
[null,17.8,"NOrdeland","5 foot double weatherproof Nordeland LED",1]
[{"$nulls":3},"Section 18: Cable Ties"]
[null,18.1,"ACDC"," T20R",1]
[null,18.2,"ACDC","T5OR",1]
[null,18.3,"ACDC","T80R",1]
[null,18.4,"ACDC","TIOOR",1]
[null,18.5,"ACDC","T120R",1]
[null,18.6,"ACDC","T150R",1]
[null,18.7,"ACDC","INSULATION  RED",1]
[null,18.8,"Nitto","WHITE",1]
[null,18.9,"Nitto","BLUE",1]
[null,18.1,"Nitto","GREEN",1]
[null,18.11,"Nitto","BLACK",1]
[null,18.12,"Nitto","YELLOW",1]
[{"$nulls":3},"Section 19: Testing Equipment"]
[null,19.1,"Hellermanntyton","Ironmeter -Trms AC/DC",1]
[null,19.2,"TBM","600A AC Clampmeter",1]
[null,19.3,"CC500 ","CC 500 Cable Cutter",1]
[null,19.4,"HD ","HD 06120 AV HEX Crimper",1]
[null,19.5,"TCT","TCT8KT TUNGSTEN Holbsaw kit",1]
[null,19.6,"TP "," 200KT Soldering Iron Kit",1]
[null,19.7,"VB","Vibration Monitoring Machinery",1]
[null,19.8,"LA ","Lase alignment Machinery",1]
[null,19.9,"BE","Bearing check machinery",1]
[{"$nulls":3},"Section 20: Wastewater pump station sump maintenaince"]
[null,20.1,"Sump Cleaning volume ","100-130 meter cube ",1]
[null,20.2,"Sump Cleaning volume ","140-160 meter cube ",1]
[null,20.3,"Sump Cleaning volume ","170-190 meter cube ",1]
[null,20.4,"Sump Cleaning volume ","200-240 meter cube ",1]
[null,20.5,"Sump Cleaning volume ","250-290 meter cube ",1]
[null,20.6,"Sump Cleaning volume ","300-340 meter cube ",1]
[null,20.7,"Sump Cleaning volume ","350-400 meter cube ",1]
[{"$nulls":3},"Section 21: Boreholes with Controls "]
[null,21.1,"Boreholes equipment with solar panels and battery pack. ","0.55 kW ",1]
[null,21.2,"Boreholes equipment with solar panels and battery pack. ","0.75 kW",1]
[null,21.3,"Boreholes equipment with solar panels and battery pack. ","1.2 kW",1]
[null,21.4,"Boreholes equipment with solar panels and battery pack. ","2.2 kW ",1]
[null,21.5,"Boreholes equipment with solar panels and battery pack. ","3 kW ",1]
[null,21.6,"Boreholes equipment with solar panels and battery pack. ","4 kW ",1]
[null,21.7,"Boreholes equipment with solar panels and battery pack. ","5 kW ",1]
[null,21.8,"Boreholes equipment with solar panels and battery pack. ","7.5 kW ",1]
[null,21.9,"Boreholes equipment with solar panels and battery pack. ","18 kW",1]
[{"$nulls":3},"SECTION 22: CLARIFIER WHEEL REBONDING"]
[null,22.1,"GOOSE NECK 4Inch",null,1]
[null,22.2,"GOOSE NECK 3Inch"]
[null,22.3,"VS4 GORMAN RUPP PRIMING FLAP",null,1]
[null,22.4,"VS6 GORMAN RUPP PRIMING FLAP",null,1]
[{"$nulls":4},1]
[null,22.5,"V BELTS SPB 2020",null,1]
[null,22.6,"V BELTS SPB 2500",null,1]
[{"$nulls":4},1]
[null,22.7,"TAPER LOCK BUSHES ","50mm",1]
[null,22.8,"TAPER LOCK BUSHES ","60mm",1]
[null,22.9,"TAPER LOCK BUSHES ","80mm",1]
[{"$nulls":4},1]
[null,22.1,"Tyre flange coupling  ","Complete set   - F120",1]
[null,22.11,null,"Complete set   - F100",1]
[null,22.12,null,"Complete  set   - F90"]
[null,22.13,null,"Complete set  -  F80",1]
[null,22.14,null,"Complete set   -F 60",1]
[{"$nulls":4},1]
[null,22.15,"Coupling Tyres  ","F120",1]
[null,22.15,null,"F100",1]
[null,22.16,null,"F90",1]
[null,22.17,null,"F80",1]
[null,22.18,null,"F60"]
[{"$nulls":3},"Section 23 Solar Highmasts lighting "]
[null,23.1,"Solar ","Intergate solar streetyard ",1]
[null,23.2,"Solar ","Design supply and deliver solar highmast light ",1]
[null,23.3,"Solar ","Installation and energizing of a complete solar yard light rate include plant hire all material items ",1]
[null,23.4,"Solar ","Erect complete solar highmast light -rate inclusive of crane hire , all material items ",1]
[null,23.5,"Solar ","Solar led ( Street yards) luminaire -complete including pole , bracket and all accessories ",1]
[null,23.6,"Solar ","Soil Testing ",1]
[null,23.7,"Solar ","Foundation , Excavations , operation , backfilling ,compaction and testing ",1]
[null,23.8,"Solar ","Training on installations , operations and maintenance of solar products ( as when as required )",1]