{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"merged":[[1,1,1,7],[3,1,3,7],[4,1,4,7],[7,1,7,7]]}
[]
[null,"PRICING SCHEDULE "]
[]
[null,"TRAFFIC SIGNAL EQUIPMENT"]
[]
[null,"ITEM","DESCRIPTION","EACH","PRICE PER UNIT","15%","BID PRICE","DELIVER IN RUSTENBURG"]
[{"$nulls":4},"FOR RUSTENBURG ","VAT","(VAT INCLUDED","(PERIOD IN  WEEKS)"]
[]
[null,"A","CONTROLLERS"]
[]
[null,1,"4(FOUR) PHASE  MICRO PROCESSOR BASED CONTROLLERS"]
[]
[null,2,"8(EIGHT) PHASE MICRO PROCESSOR BASED CONTROLLER"]
[]
[null,3,"12(TWELVE) PHASE MICRO PROCESSOR BASED CONTROLLERS"]
[]
[null,4,"16(SIXTEEN) PHASE MICRO PROCESSOR BASED CONTROLLERS"]
[]
[null,5,"PEDESTRIAN PUSHBUTTON STATIONS C/W POLE STRAPS"]
[]
[null,6,"FOUR CHANNEL LOOP DETECTORS"]
[]
[null,null,"TOTAL FOR THE BATCH"]
[]
[]
[null,"B  ","COMPLETE TRAFFIC SIGNAL HEADS (220V)"]
[]
[null,7,"SARTSM SB TO S9 - 5 ASPECT CONFIGURATION (220 V) - COMPLETE"]
[]
[null,8,"SARTSM TO S7 - 4 ASPECT CONFIGURATION (220 V) - COMPLETE"]
[]
[null,9,"SARTSM S1 - 3 ASPECT CONFIGURATION (220 V) - COMPLETE"]
[]
[]
[null,10,"SARTSM S10 L/R - 2 ASPECT CONFIGURATION ( 220 V) ARROWS - COMPLETE"]
[]
[null,null,"TOTAL FOR THE BATCH"]
[]
[]
[null,"C","REPLACEMENT BACKBOARD FOR NON ALUMINIUM SIGNAL HEADS"]
[]
[null,11,"SARTSM S8 TO S9 - 5 ASPECT CONFIGURATION C/W DIDE MOUNTING BRACKETS"]
[]
[null,12,"SARTSM S5 TO S7 - 4 ASPECT CONFIGURATIION"]
[]
[null,13,"SARTSM S10 L/R - 3 ASPECT CONFIGURATION ARROWS"]
[]
[null,14,"SARTSM S10 L/R - 2 ASPECT CONFIGURATION ARROWS"]
[]
[null,15,"SARTSM S11 - 2 ASPECT CONFIGURATION  PEDESTRIAN "]
[]
[null,null,"TOTAL FOR THE BATCH"]
[]
[]
[null,"D","TRAFFIC SIGNAL POLES WITH RUST RESISTANT UNDERCOAT (RED OXIDE) PAINTED YELLOW"]
[]
[null,16,"3.3 METER C/W FOUNDATION FRAMES, CABLE DUCTES AND BOLTS"]
[]
[]
[null,17,"6.2 METER C/W FOUNDATION FRAMES, CABLE DUCTES AND BOLTS"]
[]
[null,18,"5 METER C/W FIXED (CANTILEVER) OVERHEAD SUSPENSION, FOUNDATION FRAMES, CABLE DUCTS AND BOLTS"]
[]
[null,null,"TOTAL FOR THE BATCH"]