Specifications for tractor services required in Marobala Village, Capricon District, Limpopo
The following specification is for planting an experimental trial for scientific purposes.
1. Ploughing or ripping 1ha of land.
2. Discing 1ha of ploughed/ ripped land.
3. Planting two cultivars of sorghum on the 1ha. 
4. Service provider must bring own tractor & implements, driver for the tractor and the appropriate sorghum seed plates for the planter.
Operations are to be carried out as follows:
Location: Marobala Village, Capricon District, Limpopo. 
Date: 4 – 6 December 2024 and 20 – 21 January 2025
1. Service provider must select the appropriate tractor depending on the size of the implements (plough, ripper, disc or planter) they will use. Here are some details for the planter:
1. Planting is to be done on an experimental trial that has 72 plots which fit in 1 hector. Each plot is +/- 54 m² (12 x 4.5 m) and has 7 rows (the length and width of the plots can be adjusted according to the size of the planter and tractor used) 
1. A 6-row or 4-row sorghum/maize planter is preferred to minimize the number of tractor rotations in the field. However, small planters are not discouraged.
1. The interrow spacing is 75 / 76 cm and intra-row spacing is 30 cm.
1. The design of the experimental trail can be supplied upon request to the service provider if further clarification is required.
1. Two cultivars of sorghum will be planted on designated plots. 36 plots for each cultivar
1. The plots are at located at random.
1. There will be two planting dates, half of the trial (36 plots) will be planted in December 2024 and the remaining 36 plots will be planted in January 2025
N.B: Service provider must bring sorghum/maize planter with appropriate plates for sorghum (sorghum planting plates or similar).
Explanations:
1. The experimental trial is the sum total of the 72 plots that are within the 1 ha of land.
2. The plots are the 72 planting bays /areas on which the two cultivars of sorghum will be planted.
