Specifications for repairs to Biosystematics fire system

Location: Biosystematics Building 
Site inspection is required 

Part 1 
· Major service to all the sprinkler systems, electrical fire system and jockey pumps
· All values need to be checked and replaced if needed
· Services of alarm valves
· Traveling costs must be included and indicated in quotation

Part 2 
· The sprinkler system needs to be pressurized in the main trunk to ensure that there is no leaking
· The first wing of the Biosystematics building will be pressurized, monitored and repairs done to any leaks
· The second wing of the Biosystematics building will be pressurized, monitored and repairs done to any leaks
· The third wing of the Biosystematics building will be pressurized, monitored and repairs done to any leaks
· Consumables to be included is included, and not limited to, bucket and drop sheets
· Traveling costs must be included and indicated in quotation


