{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Preliminaries","Bills Of Quantities","Final Summary"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Preliminaries","index":0,"n_rows":631,"n_cols":5,"rows_kept":631,"merged":[[7,0,7,2],[10,0,10,2],[12,0,12,2],[14,0,14,2],[17,0,17,2],[20,0,20,2],[23,0,23,2],[26,0,26,2],[28,0,28,2],[31,0,31,2],[34,0,34,2],[37,0,37,2],[39,0,39,2],[46,0,46,2],[49,0,49,2],[52,0,52,2],[55,0,55,2],[58,0,58,2],[61,0,61,2],[64,0,64,2],[67,0,67,2],[70,0,70,2],[73,0,73,2],[76,0,76,2],[79,0,79,2],[84,0,84,2],[87,0,87,2],[90,0,90,2],[93,0,93,2],[96,0,96,2],[99,0,99,2],[102,0,102,2],[105,0,105,2],[108,0,108,2],[111,0,111,2],[113,0,113,2],[116,0,116,2],[119,0,119,2],[122,0,122,2],[125,0,125,2],[128,0,128,2],[131,0,131,2],[134,0,134,2],[137,0,137,2],[140,0,140,2],[143,0,143,2],[146,0,146,2],[149,0,149,2],[152,0,152,2],[155,0,155,2],[158,0,158,2],[161,0,161,2],[164,0,164,2],[167,0,167,2],[170,0,170,2],[173,0,173,2],[176,0,176,2],[179,0,179,2],[182,0,182,2],[185,0,185,2],[188,0,188,2],[191,0,191,2],[195,0,195,2],[198,0,198,2],[201,0,201,2],[204,0,204,2],[206,0,206,2],[210,0,210,2],[213,0,213,2],[216,0,216,2],[219,0,219,1],[222,0,222,2],[225,0,225,2],[228,0,228,2],[231,0,231,2],[234,0,234,2],[237,0,237,2],[238,0,238,2],[241,0,241,2],[244,0,244,2],[247,0,247,2],[250,0,250,2],[253,0,253,2],[256,0,256,2],[260,0,260,2],[261,0,261,2],[263,0,263,2],[266,0,266,2],[269,0,269,2],[272,0,272,2],[275,0,275,2],[281,0,281,2],[283,0,283,2],[286,0,286,2],[288,0,288,2],[291,0,291,2],[294,0,294,2],[296,0,296,2],[299,0,299,2],[301,0,301,2],[305,0,305,2],[308,0,308,2],[311,0,311,2],[314,0,314,2],[317,0,317,2],[320,0,320,2],[323,0,323,2],[326,0,326,2],[329,0,329,2],[332,0,332,2],[335,0,335,2],[338,0,338,2],[341,0,341,2],[344,0,344,2],[347,0,347,2],[350,0,350,2],[353,0,353,2],[356,0,356,2],[406,0,406,2],[408,0,408,2],[411,0,411,2],[414,0,414,2],[417,0,417,2],[420,0,420,2],[423,0,423,2],[426,0,426,2],[429,0,429,2],[431,0,431,2],[434,0,434,2],[437,0,437,2],[440,0,440,2],[443,0,443,2],[446,0,446,2],[452,0,452,2],[454,0,454,2],[457,0,457,2],[459,0,459,2],[462,0,462,2],[465,0,465,2],[468,0,468,2],[471,0,471,2],[474,0,474,2],[477,0,477,2],[480,0,480,2],[483,0,483,2],[486,0,486,2],[489,0,489,2],[492,0,492,2],[495,0,495,2],[498,0,498,2],[501,0,501,2],[504,0,504,2],[506,0,506,2],[509,0,509,2],[511,0,511,2],[514,0,514,2],[516,0,516,2],[519,0,519,2],[522,0,522,2],[525,0,525,2],[527,0,527,2],[530,0,530,2],[532,0,532,2],[535,0,535,2],[538,0,538,2],[541,0,541,2],[543,0,543,2],[546,0,546,2],[549,0,549,2],[551,0,551,2],[556,0,556,2],[559,0,559,2],[562,0,562,2],[565,0,565,2],[568,0,568,2],[571,0,571,2],[574,0,574,2],[577,0,577,2],[579,0,579,2],[581,0,581,2],[584,0,584,2],[587,0,587,2],[590,0,590,2],[593,0,593,2],[596,0,596,2],[599,0,599,2],[602,0,602,2],[605,0,605,2],[608,0,608,2],[611,0,611,2],[614,0,614,2],[617,0,617,2],[620,0,620,2],[630,0,630,2]],"flags":["formulas_cached_only"]}
["SECTION NO. 1"]
["PRELIMINARIES"]
[{"$nulls":4},"Amount"]
["SECTION NO. 1 PRELIMINARIES"]
[]
[]
[]
["BUILDING AGREEMENT AND PRELIMINARIES\nThe JBCC Preliminaries Code 2103, May 2005 edition for use with the JBCC Principal Building Agreement Edition 4.1 Code 2101, March 2005 as prepared by the Joint Building Contract Committee shall be the applicable building agreement, amended as hereinafter described\nThe ASAQS Preliminaries published by the Association of South African Quantity Surveyors for use with the said JBCC Principal Building Agreement shall be deemed to be incorporated in these bills of quantities\nContractors are referred to the above mentioned documents for the full intent and meaning of each clause thereof\nThese clauses are hereinafter referred to by clause number and heading  only. Where standard clauses or alternatives are not entirely applicable to this contract such modifications, corrections or supplements as will apply are given under each relevant clause heading and such modifications,  corrections or supplements shall take precedence notwithstanding anything contrary contained in the above mentioned documents\nWhere any item is not relevant to this specific contract such item is marked N/A, signifying \"not applicable\"\nPREAMBLES FOR TRADES\nThe Model Preambles for Trades (1999 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claim arising from brevity of description of items fully described in the said Model Preambles will be entertained\nSupplementary preambles are incorporated in these bills of quantities to satisfy the requirements of this project.  Such supplementary preambles shall take precedence over the provisions of the said Model Preambles\nThe contractor's prices for all items throughout these bills of quantities must take account of and include for all of the obligations, requirements and specifications given in the said Model Preambles and in any supplementary preambles\nPRICING OF PRELIMINARIES\nPricing of Prelims\n1   Should the contractor select Option A in terms of clause 10.3 for the purpose of adjustment of these preliminaries, the amount entered in the amount column in these preliminaries is to be divided into one or more of the three categories provided namely Fixed (F), Value Related (V) and Time Related (T)"]
["F:  .......................","V:  .......................","T:  ......................."]
[]
["SECTION A - PRINCIPAL BUILDING AGREEMENT\nDefinitions\n2   Clause 1.0 - Definitions and interpretation\n1.1 Definition of \"Commencement Date\" is added:\n\"COMMENCEMENT DATE\" means the date that the agreement, made in terms of the Form of Offer and Acceptance, comes into effect  Clause 1.1 Definition of \"Construction Period\" is amended by replacing it with the following:\n\"CONSTRUCTION PERIOD\" means the period commencing on the date that possession of the site is given to the contractor and ending on the date of practical completion\nClause 1.1 Definition of \"Interest\" is amended by replacing it with the following:\nINTEREST means the interest rates applicable on this contract, whether specifically indicated in the relevant clauses or not, will be the rate as determined by the Minister of Finance, from time to time, in terms of section 80(1 )(b) of the Public Finance Management Act, 1999 (Act No.1 of 1999)\n(a) In respect of interest owed by the employer, the interest rate as determined by the Minister of Justice and Constitutional Development, from time to time, in terms of section 1 (2) of the Prescribed Rate of Interest Act, 1975 (Act No. 55 of 1975), will apply; and\n(b) in respect of interest owed to the employer, the interest rate as determined by the Minister of Finance, from time to time, in terms of section 80(1 )(b) of the Public Finance Management Act, 1999 (Act No. 1 of 1999), will apply."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
["Objective and preparation\n3   Clause 2.0 - Offer, acceptance and performance"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
["4   Clause 3.0 - Documents\nClause 3.7 is amended by the addition of the following:\nThe contractor shall supply and keep a copy of the JBCC Series 2000 Principal Building Agreement and Preliminaries applicable to this contract on the site, to which the employer, principal agent and agents shall have access at all times"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["5   Clause 4.0 - Design responsibility                                                                                "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["6   Clause 5.0 - Employer's agents                                                                                    "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["7   Clause 6.0 - Site representative                                                                             "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["8   Clause 7.0 - Compliance with regulations                                      "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
["9   The provisions herein include inter alia, compliance with all the requirements, without limiting the generality of the provisions of Clause 7.0, the contractor's attention is drawn to the provisions of the Construction Regulations, 2014 issued in terms of the Occupational Health and Safety Act, 1993 (Act No 85 of 1993) and in particular with Regulation 7(1 )(a) requiring the compilation of a health and safety plan, as well as Regulation 8(5) requiring the appointment of a Construction Health and Safety Officer, the necessary documented health and safety specifications for the works and that the employer shall ensure that the contractor has made provision for the cost of health and safety measures during the execution of the works. The contractor shall price opposite this item for compliance with the act and the regulations and the reasonable provisions of the aforementioned health and safety specifications"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["10   Clause 8.0 - Works risk                                                                                  "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["11   Clause 9.0 - Indemnities                                                                                        "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12   Clause 10.0 - Works insurances                                                                         "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
["Clause 10.0 is amended by the addition of the following clauses:\n10.5 Damage to the Works\n( a ) Without in any way limiting the contractors obligations in terms of the contract, the contractor shall bear the full risk of damage to and/or destruction of the works by whatever cause during construction of the works and hereby indemnifies and holds harmless the employer against any such damage. The contractor shall take such precautions and security measures and other steps for the protection and security of the works as the contractor may deem necessary\n(b) The contractor shall at all times proceed immediately to remove or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works\n(c) The employer shall carry the risk of damage to or destruction of the works and material paid for by the employer that is the result of the excepted risks as set out in\n10.6\n(d) Where the employer bears the risk in terms of this contract, the contractor shall, if requested to do so, reinstate any damage or destroyed portions of the works and the costs of such reinstatement shall be measured and valued in terms of 32.0 hereof\n10.6 Injury to Persons or loss of or damage to Properties"]
[]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["14   Clause 11.0 - Liability insurances                                                     "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["15   Clause 12.0 - Effecting insurances                                        "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["16   Clause 13.0 - No clause                                                                                                 N/A"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["17   Clause 14.0 - Security                                                                                "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["18   Clauses 14.1 - 14.8 are amended by replacing them with the following:"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["19   Clause 15.0 - Preparation for and execution of the works                                      "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 15.1.1 is amended by replacing it with:\nNo Clause\nClause 15.1 is amended by the addition of the following clause:\n15.1.4 An acceptable health and safety plan, required in terms of the Occupational Health and Safety Act, 1993 (Act 85 of 1993), Construction Regulations 2014 as per Government notice within twenty-one (21) calendar days of commencement date\nClause 15.2.1 is amended by replacing it with the following clause:\nGive the contractor possession of the site within ten (10) working days of the contractor complying with the terms of 15.1.2 and 15.1.4"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["21   Clause 16.0 - Access to the works                                                                        "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["22   Clause 17.0 - Contract instructions                                                           "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["23   Clause 18.0 - Setting out of the works                                         "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["24   The contractor shall notify the principal agent if any encroachments of adjoining foundations, buildings, structures, pavements, boundaries, etc exist in order that the necessary arrangements may be made for the rectification of any such encroachments"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["25   Clause 19.0  - Assignment                                                          "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["26   Clause 20.0 - Nominated subcontractors                                                    "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
["Note: See item B9.1 hereinafter for adjustment of attendance on nominated subcontractors executing work allowed for under provisional sums"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["27   Clause 20.1.3 is amended by replacing it with the following: No Clause\n28   Clause 21.0 - Selected subcontractors"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["29   Clause 21 is amended by replacing it with:\nNo Clause"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["30   Clause 22.0 - Employer's direct contractors                                   "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["31   Clause 23.0 - Contractor's domestic subcontractors                                "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["32   Clause 24.0 - Practical completion                                                                 "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["33   Clause 25.0 - Works completion                                                                                   "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["34   Clause 26.0 - Final completion                                                                                      "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["35   Clause 27.0 - Latent defects liability period                                                                   "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["36   Clause 28.0 - Sectional completion                                                                               "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["37   Clause 29.0 - Revision of the date for practical completion                                           "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
["38   The removal and replacement of materials and/or workmanship which do not conform to specification or drawings shall not constitute grounds for an extension of the construction period nor for an adjustment to the contract value (clause 29.3)"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["39   Clause 30.0 - Penalty for noncompletion                                                                       "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["40   Clause 31.0 - Interim payment to the contractor                                                      "]
["F:  .......................","V:  .......................","T:  ......................."]
[]
["41   The inclusion of materials and goods stored off site in the amount authorised for payment in terms of clause 31.4 shall be at the sole discretion of the principal agent and such inclusion shall only be considered upon the provision, by the contractor, of an approved guarantee issued by a registered commercial bank.  Clause 31.6.5 is therefore not applicable"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["42   Clause 31.8 is amended by replacing it with the following two alternative clauses:\nAlternative A\n31.8(A) Where a security is selected in terms of 14.1; 14.5 or 14.6, the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:\n31.8(A).1 Ninety-five per cent (95%) of such value in interim payment certificates issued up to the date of practical completion\n31.8(A).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of practical completion and up to but excluding the date of final completion\n31.8(A).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of final completion and up to but excluding the final payment certificate in terms of 34.6\n31.8(A).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate\nAlternative B\n31.8(8) Where security is a payment reduction in terms of 14.7 the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:\n31.8(8).1 Ninety per cent (90%) of such value in interim payment certificates issued up to the date of practical completion\n31.8(8).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of practical completion and up to but excluding the date of final completion\n31.8(8).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of final completion and up to but excluding the final payment certificate in terms of 34.6"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["43   Clause 32.0 - Adjustment to the contract value                                                "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["44   Clauses 32. 5. 1, 32. 5.4 and 32. 5. 7 are amended by the addition of the following at the end of the sentence:\n\"due to no fault of the contractor\""]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["45   Clause 33.0 - Recovery of expense and loss                                                       "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["46   Clause 33.2 is amended by adding the following clauses:\n33.2.9 the contractors failure or neglect to commence with the works on the dates prescribed in the contract\n33.2.10 the contractors failure or neglect to proceed with the works in terms of the contract\n33.2.11 the contractors failure or neglect for any reason to complete the works in accordance with the contract\n33.2.12 the contractors refusal or neglect to comply strictly with any of the conditions of contract or any contract instructions and/or orders in writing given in terms of the contract\n33.2.13 the contractors estate being sequestrated, liquidated or surrendered in terms of the insolvency laws in force within the Republic of South Africa"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["47   Clause 34.0 - Final account and final payment                                                              "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["48   Clause 34.13 is amended by replacing seven (7) calendar days with twenty- one (21) calendar days and deleting the words subject to the employer giving the contractor a tax invoice for the amount due"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["49   Clause 35.0 - Payment to other parties                                                                         "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["50   Clause 36.0 - Cancellation by employer - contractor's default                                       "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["52   Clause 37.0 - Cancellation by employer - loss and damage                                          "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["53   Clause 37.0 is amended by the addition of the following clause:\n37.5 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["54   Clause 38.0 - Cancellation by contractor - employer's default                                       "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["55   Clause 38.0 is amended by the addition of the following clause:\n38.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["56   Clause 39.0 - Cancellation - cessation of the works                                                      "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["57   Clause 40.0 - Dispute settlement                                                                                   "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["58   Clause 40.2.2 is amended by replacing one (1) year with three (3) years Clause 40.6 is amended by removing the reference to:\nNo clause\nClause 40. 7.1 is amended by replacing (10) with (15) and by the addition of the following:"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Substitute provisions\n59   Clause 41.0 - State clauses"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Contract variables\n60   Clause 42.0 - Pre-tender information"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["61   User Note -All information for this section requires consultation with the contractor.  The principal agent should not pre-select any of the alternatives available to the contractor"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["62   Information necessary for the completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["63   Clause 42.0 -  Post-tender information                                                                 "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["64   The required post-tender information shall be inserted in the agreement after consultation with the contractor"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["42.1 CONTRACTING AND OTHER PARTIES\n42.1.1 Employer: ........................................................\nPostal\naddress: ................................................ ..............................................Code: ...\n.............\nTel: ............................Fax: ..............................\nE-mail                                                                       Tax/VAT registration\nNo: ..................................\nPhysical\naddress: ............................................. ..............................................................\n..........\n........................................................................\n42.1.2 Principal agent: .................................................."]
[]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["66   42.2.3 Work or installations by direct contractors .............\n...........................................................................\n...........................................................................\n...........................................................................\n...........................................................................\n...........................................................................\n...........................................................................\n..........................................................................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["67   42.2.2 Site description: ..................................................\n..........................................................................\n..........................................................................\n.........................................................................."]
["F:  .......................","V:  .......................","T:  ......................."]
[{"$nulls":3},"Item"]
["68   42.2.4 Specific options that are applicable to a state  organ only Where so:\n(1) Interest rate legislation: ...............................\n(2) Lateral support insurance to be effected by the  contractor    - Yes\n(3) Payment will be made for materials and goods                           - Yes"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["(4) Dispute resolution by litigation - No\n(5) Extended defects liability period applicable"]
[]
[]
[{"$nulls":3},"Item"]
["F:  .......................","V:  .......................","T:  ......................."]
[]
["69   42.2.5 Possession of the site is intended to be given on (date)...(once adjudication is completed, NoC is approved and contract is signed)…."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["70   42.2.6 Period for the commencement of the works after\nthe contractor takes possession of the site  (No of working days) ........To be confirmed upon contract award..............................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["71   42.2.7 For the works as a whole: The date for practical  completion and the penalty per calendar day\nDate ............................. Penalty R......................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["72   42.2.8 For the works in sections:  The date for practical  completion and the penalty per calendar day  - N/A\nSection 1 Date .................... Penalty R..................\nSection 2 Date .................... Penalty R..................\nSection 3 Date .................... Penalty R..................\nSection 4 Date .................... Penalty R..................\nSection 5 Date .................... Penalty R .................\nSection 6 Date .................... Penalty R ................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["73   42.2.9 The law applicable to this agreement shall be that of (country) ................South Africa........................................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["42.3 INSURANCES\n74   42.3.1 Contract works insurance to be effected by contractor\nFor the sum of:          R ...................................\nWith a deductible of:  R ................................…."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["75   42.3.2 Supplementary insurance is required - No                                                       "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["76   42.3.3 Public liability insurance to be effected by contractor\nFor the sum of:     R.....................................\nWith a deductible of:  R..................................…"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["77   42.3.4 Support insurance to be effected by employer For the sum of:  R.....................................\nWith a deductible of: R....................................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["42.4 DOCUMENTS\n"]
["78   42.4.1 Waiver of the contractor's lien or right of continuing  posession is required - Yes"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["79   42.4.2 Construction document copies to be supplied to the  contractor free of charge  (No of 3) - Yes"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["80   42.4.3 State measuring system used for drawing up bills\nof quantities - Lump sum document..................... .........................................................................."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["81   42.4.4 Number of working days for submission of priced\ndocuments     (No of working days from advert to closing date of tender  )"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["82   42.4.5 JBCC Engineering General Conditions are to be included in the contract documents - No"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["83   42.4.6 The contract value is to be adjusted using CPAP  indices - Yes \nWhere CPAP is to be used (base month) ............\nAlternative indices (if applicable) ......................…"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["84   42.4.7 Details of changes made to the provisions of JBCC standard documentation - .................\n...refer to contract data JBCC amendments...................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................\n......................................................................"]
[]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["SECTION B - PRELIMINARIES\nDefinitions and interpretation\n85   Clause 1.0 - Definitions and interpretation"]
["F:  .......................\nDocuments"]
[]
["86   Clause 2.1 - Checking of documents                                                                            "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["87   Clause 2.2 - Provisional bills of quantities                                                                     "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["88   Clause 2.3 - Availability of construction documentation                                                 "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["89   Clause 2.4 - Interests of agents                                                                                     "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["90   Clause 2.5 - Priced documents                                                                                     "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["91   Clause 2.6 - Tender submission                                                                                    Item"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["92   Tenders shall be valid for a period of ? days from the closing date of tenders             "]
[]
["93    Clause 2.6 is amended by replacing JBCC Form of Tender with \"Form of Offer/Tender\" included in the returnable schedules"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["94   Clause 3.1 - Defined works area                                                                                   "]
[]
["95   The area of the works to be occupied by the contractor is indicated on architect's drawing"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["96   Clause 3.2 - Geotechnical investigation                                                                         "]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["97   Clause 3.3 -  Inspection of the site                                                                               "]
[]
["98   Tenderers shall complete the Site INspection Certificate included in the tender documents and return the same with the tender submission"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["99   Clause 3.4 - Existing premises occupied                                                                      "]
[]
["100 Clause 3.5 - Previous work - dimensional accuracy"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
[]
["101 Clause 3.6 - Previous work - defects"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["102 Clause 3.7 - Services - known"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["103 Clause 3.8 - Services - unknown"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["104 Clause 3.9 - Protection of trees"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["105 Clause 3.10 - Articles of value"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["106 Clause 3.11 - Inspection of adjoining properties"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["107 Management of contract\nClause 4.1 - Management of the works"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["108 Clause 4.2 - Programme for the works"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["109 Clause 4.3 - Progress meetings"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["110 Clause 4.4 - Technical meetings"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["111 Clause 4.5 - Labour and plant records"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["112 Samples, shop drawings and manufacturer's instructions\nClause 5.1 - Samples of materials"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 5.2 - Workmanship samples"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 5.3 - Shop drawings"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 5.4 - Compliance with manufacturers' instructions"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Temporary works and plant\nClause 6.1 - Deposits and fees"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 6.2 - Enclosure of the works"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 6.3 - Advertising"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 6.4 - Plant, equipment, sheds and offices"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 6.5 - Main noticeboard"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 6.6 - Subcontractors' noticeboard"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Temporary services\nClause 7.1 - Location"]
[]
["Clause 7.2 - Water"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 7.3 - Electricity"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 7.4 - Telecommunication facilities"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 7.5 - Ablution facilities"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Prime cost amounts\nClause 8.1 - Responsibility for prime cost amounts"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Attendance on nominated/selected subcontractors\nClause 9.1 - General attendance"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 9.2 - Special attendance"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 9.3 - Commissioning - fuel, water and electricity"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Financial aspects\nClause 10.1 - Statutory taxes, duties and levies"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision is made in the summary of these bills of quantities for the inclusion of Value Added Tax (VAT)"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 10.2 - Payment of preliminaries"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 10.3 - Adjustment of preliminaries"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Should the contractor select Option B but fail to provide the information required prior to the signing of the contract, the principal agent shall have the right to select either Option A or B for the adjustment of preliminaries.  If the principal agent selects Option B he shall be entitled to make assumptions at his discretion regarding the information which the contractor would normally have provided prior to the signing of the contract"]
[]
["Clause 10.4 - Payment certificate cash flow"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.1 - Protection of the works"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.2 - Protection/isolation of existing/sectionally occupied works"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.3 - Security of the works"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.4 - Notice before covering work"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.5 - Disturbance"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.6 - Environmental disturbance"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["?A copy of the environmental management plan is annexed to these bills of quantities.  The contractor shall comply with all the requirements of such environmental management plan?"]
[]
["Clause 11.7 - Works cleaning and clearing"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.8 - Vermin"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.9 - Overhand work"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.10 - Instruction manuals and guarantees"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.11 - As built information"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Clause 11.12 - Tenant installations"]
[]
[]
["Schedule of variables\n12.1 - Pre-tender information"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Information necessary for elections and completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder.  Where no information is given it shall mean that either specific requirements are not required or that the clause is not relevant to this specific contract"]
[]
["12.1.1 - Provisional bills of quantities [clause 2.2]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["The quantities are provisional - yes"]
[]
["12.1.2 - Availability of construction documentation [clause 2.3]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Construction documentation is complete - yes"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.3 - Interests of agents [clause 2.4] - None"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.4 - Defined works area [clause 3.1]\nRestrictions will be pointed out at the site inspection"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.5 - Geotechnical investigation [clause 3.2]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.6 - Existing premises occupied [clause 3.4] - Yes, operational school"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.7 - Previous work - dimensional accuracy [clause 3.5]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.8 - Previous work - defects [clause 3.6]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.9 - Services - known [clause 3.7]\nExisting services and points of connection will be pointed out on site by the principal agent"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.10 - Protection of trees [clause 3.9]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.11 - Inspection of adjoining properties [clause 3.11]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.12 - Enclosure of the works [clause 6.2]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.13 - Offices [clause 6.4.3] Specific requirements:\n"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.14 - Main noticeboard [clause 6.5] Specific requirements:\nThe contractor shall provide, erect where directed, maintain and remove on\ncompletion of the works a notice board size 3 x 3m, constructed of suitable boarding with flat smooth surface and with edging bead 19mm thick round outer edges and projecting 12mm from face of boarding and rounded on front edge. The board shall be securely fixed to hoarding, where hoarding is provided, or fixed to and including a suitable supporting structure of timber or tubular posts and braces. The board is to be painted ivory white and the bead and 12mm wide dividing lines dark green. All wording shall be inscribed in dark green as per the coat of arms for SA. All wording shall be inscribed in dark green painted sans serif lettering."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.15 - Subcontractors' noticeboard [clause 6.6]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["A noticeboard is required - yes"]
[]
["12.1.16 - Water [clause 7.2]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Option A (by contractor)    yes\nOption B (by employer - free of charge)   no Option C (by employer - metered)   no"]
[]
["12.1.17 - Electricity [clause 7.3]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Option A (by contractor)     yes\nOption B (by employer - free of charge)   no Option C (by employer - metered)   no"]
[]
["12.1.18 - Telecommunications [clause 7.4]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Telephone    yes\nFacsimile     yes E-mail   yes"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.19 - Ablution facilities [clause 7.5]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Option A (by contractor)   yes\nOption B (by employer)    no"]
[]
["12.1.20 - Protection/isolation of existing/sectionally occupied works [clause 11.2]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Protection/isolation is required -  yes"]
[]
["12.1.21 - Special attendance [clause 9.2]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.22 - Protection of the works [clause 11.1]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.1.23 - Disturbance [clause 11.5]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["[11.5] Specific requirements:\nThe contractor shall keep the site, structures, etc well watered during operations to prevent dust and shall provide and erect and remove on completion of the works all necessary temporary dust screens all to the satisfaction of the principal agent"]
[]
["12.1.24 - Environmental disturbance [clause 11.6]"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["12.2 - Post-tender information"]
[]
[]
["The required post-tender information shall be inserted in the preliminaries after consultation with the contractor"]
[]
["SECTION C - SPECIFIC PRELIMINARIES\nUser Notes-\nUser Note - All information for this section requires consultation with the contractor.  The principal agent should not pre-select any of the alternatives available to the contractor\nUser Note - Selected examples of typical clauses are provided to show possible ways of describing such clauses.  Users must delete, adapt or add to these examples to suit their particular circumstances"]
[]
["Site instructions\nSite instructions issued on site are to be recorded in triplicate in a site instruction book which is to be provided and maintained on site by the contractor"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Warranties for materials and workmanship\nWhere warranties for materials are called for, the contractor shall obtain a written warranty, addressed to the employer, from the firm supplying the materials and/or doing the work and shall deliver same to the principal agent on the certified completion of the contract.  The warranty shall state that workmanship, materials and installation are warranteed for a specified period from the date of certified completion of the contract, and that any defects that may arise during the specified period shall be made good at the expense of the firm supplying the materials and/or doing the work, upon written notice to do so.  The warranty will not be enforced if the work is damaged by defects in the construction of the building in which case the responsibility for replacement shall rest entirely with the contractor."]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Co-operation of contractor for cost management\nIt is specifically agreed that the contractor accepts the obligation of assisting the principal agent in implementing proper cost management.  The contractor will be advised by the principal agent of all cost management procedures which will be implemented to ensure that the final building cost does not exceed the budget.  The principal agent undertakes to make available to the contractor all budgetary allowances and cost assessments/reports to enable the proper procedures to be implemented and the contractor shall attend all cost plan review and cost management meetings.  The contractor undertakes to extend these procedures, as necessary, to all subcontractors"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["The contractor undertakes to maintain in confidence any and all information regarding this project and shall obtain appropriate similar undertakings from all subcontractors and suppliers.  Such information shall not be used in any way except in connection with the execution of the works\nNo information regarding this project shall be published or disclosed without the prior written consent of the employer"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Propping of floors below\nThe contractor is advised that propping of floors below may be required if he wishes to use any areas of completed suspended reinforced concrete slabs for vehicle access, storage of materials and goods and location of plant, scaffolding, etc.  The location of these areas and any necessary propping shall be approved by the principal agent and the cost thereof shall be borne by the contractor"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Testing of windows for watertightness\nEach window shall be tested for watertightness with water sprayed on by means of a 20mm hosepipe using adequate pressure.  If in the opinion of the principal agent, the pressure proves to be inadequate, then the pressure in the hosepipe shall be boosted by means of compressed air or other approved means"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Testing of flat roof waterproofing for watertightness\nFlat roof waterproof areas shall be prepared with small sand dykes around them of a size and enclosing an area approved by the principal agent, flooded with water and kept \"ponded\" for at least 36 hours as a test to ensure the watertightness of the waterproofing and before any further construction work is carried out above the waterproofing"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Wherever a trade name for any product has been described in the bills of quantities, the tenderers attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained\nprior to the closing date for submission of tenders\nIf prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for Contract drawings"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Occupational Health and Safety\nAllowance to be made under this clause for compliance with all requirements of the occupational health and safety act and regulations"]
[]
["Health & Safety (clause C15)\nThe Contractor shall allow for Health and Safety according to the Occupational Health and Safety Act, 1993, Construction Regulations 2014 as per Government Notice. Contractor to include all OHS requirements such as PPE, safety file, training, medicals, signage, safety officer and covid regulations"]
[]
["Occupational Health and Safety Act\nThe contractor shall comply with all the requirements set out in the Construction Regulations, 2014 issued under the Occupational Health and Safety Act, 1993 (Act No 85 of 1993) It is required of the contractor to thoroughly study the Health and Safety Specification that must be read together with and is deemed to be incorporated under this Section of the bills of quantities/ lump sum document The contractor must take note that compliance with the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is compulsory.\nIn the event of partial or total non-compliance, the Employer, notwithstanding the provisions of clause A31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance. The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment Provision for pricing of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is made under this clause, as well as the clauses that follow hereafter and it is explicitly pointed out that all requirements of the aforementioned are deemed to be priced under these clauses and no additional claims in this regard shall be entertained"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["The contractor shall also comply with the additional requirements with regard to the Coronavirus pandemic in terms of all Covid-19 legislation, regulations and guidelines. It is explicitly pointed out that all requirements of the aforementioned are deemed to be priced under this clause and the specific related clauses hereafter and no additional claims in this regard shall be entertained"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of protective personal equipment (PPE)\nProvision of reflective vests"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of hard hats"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of protective footwear"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of ear plugs"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of dust masks"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of gloves"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of high visibility overalls to SARTSM Chapter 13 Level 3"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of SANS approved ear defenders"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["Provision of of face masks (Covid -19)"]
["F:  .......................","V:  .......................","T:  ......................."]
[{"$nulls":3},"Item"]
["Provision of of face shields (Covid -19)"]
["F:  .......................","V:  .......................","T:  ......................."]
[]
["Provision of hand sanitiser (min 70% alchoholl, foot press stands and paper towels (Covid -19)",null,null,"Item"]
["F:  .......................","V:  .......................","T:  ......................."]
[]
["Provision of full time construction health and safety officer (SACPCMP Registered)"]
["F:  .......................","V:  .......................","T:  .......................","Item"]
[]
["SUMMARY OF CATEGORIES\nCategories\nCategory: Fixed F:..............................\nCategory: Value V:..............................\nCategory: Time T:................................"]
["Category: Fixed F:..............................\r\n",null,null,"Item"]
["\r\n"]
["Category: Value V:..............................\r\n"]
["\r\n"]
["Category: Time T:................................"]
[]
["SECTION NO. 1 PRELIMINARIES SECTION SUMMARY\nPreliminaries"]

{"sheet":"Bills Of Quantities","index":1,"n_rows":1256,"n_cols":6,"rows_kept":1256,"flags":["formulas_cached_only"]}
["Item","Description","Uom","Quantity","Rate","Amount"]
[]
[null,"SECTION NO. 1 : PRELIMINARIES"]
[]
[]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]
[]
[]
[null,"SECTION NO. 2 : BUILDINGS"]
[]
[]
[null,"BILL NO.1 : ALTERATIONS"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"View site"]
[]
[null,"Before submitting his tender the tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials salvageable from the alterations.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,"General"]
[]
[null,"Note to tenderers: The removal, storage ,disposal, etc  of asbestos sheeting, etc to be executed in strict accordance to the bye laws (OHS) regarding same by a specialist asbestos sub-contractor. Prices to include for this."]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to tenants in the building and to adjoining premises and their tenants. He shall provide proper protection and provide , erect and remove when directed , any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to remain the property of the employer shall be carefully taken out, temporarily stored"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to be re-used shall be thoroughly overhauled before refixing including taking off, easing and rehanging, cramping up, re-wedging as required and making good cramps, dowels, etc, and oiling, adjusting and repairing ironmongery  as  necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described . Re-painting or re-varnishing is given separately"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Demolition"]
[]
["1","Demolition of existing block complete comprising of surface bed, brickwork, roof, etc.","m²",{"v":208,"d":"208.00"}]
[]
[null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement"]
[]
["2","170mm Thick surface beds","m²",{"v":382,"d":"382.00"}]
[]
[null,"Breaking down and removing brickwork etc"]
[]
["3","One brick walls","m²",{"v":2,"d":"2.00"}]
[]
[null,"Taking out and removing doors, windows, etc, including thresholds, sills, etc"]
[]
["4","Timber single door and frame, size 813 x 2032mm high","No",{"v":5,"d":"5.00"}]
[]
["5","Timber double door and frame, size 1500 x 2032mm high","No",{"v":1,"d":"1.00"}]
[]
["6","Single security gate, 925 x 2032mm high","No",{"v":1,"d":"1.00"}]
[]
["7","Double security gate, 3 500 x 2032mm high","No",{"v":2,"d":"2.00"}]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc"]
[]
["8","Corrugated sheet steel roof covering and timber purlins","m²","  1 402"]
[]
["9","Corrugated asbestos roof covering and timber purlins","m²","  2 469"]
[]
["10","Roof insulation","m²","  3 343"]
[]
["11","Fibre cement fascias and bargeboards","m","  1 483"]
[]
["12","Gutters and rainwater pipes","m","  1 254"]
[]
["13","Gypsum plasterboard ceilings, including timber brandering, cornices, etc","m²","  8 986"]
[]
[null,"Taking out and removing sundry joinery work, fittings, etc"]
[]
["14","Timber skirtings","m","  2 945"]
[]
[null,"Taking up and removing wood block floor coverings, vinyl floor coverings, carpets, etc and preparing screeds for new floor coverings"]
[]
["15","Vinyl tile floor covering","m²","  6 714"]
[]
[null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc"]
[]
["16","30mm Screed from floor","m²",{"v":27,"d":"27.00"}]
[]
[null,"Hacking up/off and removing ceramic tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc"]
[]
["17","Tiles to floors","m²",{"v":112,"d":"112.00"}]
[]
["18","Tiles to walls","m²",{"v":196,"d":"196.00"}]
[]
[null,"Taking out and removing sanitary fittings, tanks, geysers, etc, including disconnecting from pipes, traps, etc and making good floor and wall finishes (making good tiling and paintwork elsewhere)"]
[]
["19","Vitreous china wash hand basin","No",{"v":19,"d":"19.00"}]
[]
["20","Vitreous china WC pan with cistern and flush pipe","No",{"v":10,"d":"10.00"}]
[]
["21","Steel urinal","No",{"v":4,"d":"4.00"}]
[]
["22","CP star pillar taps","No",{"v":6,"d":"6.00"}]
[]
[null,"Servicing of existing work"]
[]
["23","Investigate and isolate tap leak and repair","No",{"v":2,"d":"2.00"}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES"]
[]
[null,"MAKING GOOD OF FINISHES ETC"]
[]
[null,"Pavelite steel trowelled on existing screed"]
[]
["24","Average 4mm thick on floors and landings","m²","  6 339"]
[]
[null,"Wire brush along length of crack and ream open cracks 20mm width x 20mm deep and scratch out any debris that may block the crack in the sides of the hole. Epoxy R8 bars in grooves at 250mm centres over the crack length. Fill the \"V\" grooves and plaster with structural mortar and mesh ref 100."]
[]
["25","On cracks on plastered walls","m",{"v":53,"d":"53.00"}]
[]
[null,"Chip open the crack to form a \"V\" shape 20mm wide x 10mm deep and scratch out the debris that may block the crack in the sides of the hole. Grinding in the floor approximately 200mm to 300mm apart from the rebar to be placed into an epoxy repair mortar 'SIKA TOP-ARMATEC 100'. Fill the crack with structural epoxy repair mortar 'SIKA MONO TOP 615HB'"]
[]
["26","On cracks on concrete floors, walkways, roofs, etc","m",{"v":48,"d":"48.00"}]
[]
[null,"Resealing of joints"]
[]
["27","Ream out joint and install UV resistant polysulphide sealant","m",{"v":32,"d":"32.00"}]
[]
[null,"Pressure cleaning existing buildings"]
[]
["28","External facebrick","m²",{"v":296,"d":"296.00"}]
[]
["29","Existing floors","m²",{"v":110,"d":"110.00"}]
[]
[null,"BUDGETARY ALLOWANCE"]
[]
["30","Allow a budgetary amount of R100 000.00 for Remedial Works","Item",null,{"v":100000,"d":"100,000.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.2 : EARTHWORKS"]
[]
[null,"EARTHWORKS (PROVISIONAL)"]
[]
[null,"EXCAVATION, FILLING, ETC OTHER THAN BULK"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["1","Reduced levels under floors","m³",{"v":128,"d":"128.00"}]
[]
["2","Trenches","m³",{"v":69,"d":"69.00"}]
[]
["3","Narrow pit","m³",{"v":231,"d":"231.00"}]
[]
["4","Underpinning in 1m alternating sections under existing foundations","m³",{"v":58,"d":"58.00"}]
[]
[null,"Extra over bulk excavations in earth for excavation in"]
[]
["5","Soft rock","m³",{"v":41,"d":"41.00"}]
[]
["6","Intermediate","m³",{"v":39,"d":"39.00"}]
[]
["7","Hard rock","m³",{"v":20,"d":"20.00"}]
[]
[null,"Back excavation of vertical sides of excavations in earth for working space including backfilling compacted to ?% Mod AASHTO density"]
[]
["8","Not exceeding 500mm deep for placing and removing formwork to walls from excavated face","m²",{"v":196,"d":"196.00"}]
[]
[null,"Extra over all excavations for carting away"]
[]
["9","Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m³",{"v":196,"d":"196.00"}]
[]
[null,"Risk of collapse of excavations"]
[]
["10","Sides of excavations not exceeding 1,5m deep","m²",{"v":199,"d":"199.00"}]
[]
["11","Sides of excavations exceeding 1,5m deep","m²",{"v":290,"d":"290.00"}]
[]
[null,"Keeping excavations free of water"]
[]
["12","Keeping excavations free of all water other than subterranean water","Item",{"v":1,"d":"1.00"}]
[]
[null,"FILLING, ETC"]
[]
[null,"Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 95% Mod AASHTO density"]
[]
["13","Under floors, steps, pavings, etc","m³",{"v":56,"d":"56.00"}]
[]
["14","Backfilling to trenches, holes, etc.","m³",{"v":119,"d":"119.00"}]
[]
[null,"Filling of G7 supplied by the contractor, compacted to 95% Mod AASHTO density"]
[]
["15","Backfilling to trenches, holes, etc","m³",{"v":132,"d":"132.00"}]
[]
["16","Under floors, steps, paving, etc.","m³",{"v":78,"d":"78.00"}]
[]
[null,"Filling of coarse river sand supplied by the contractor, consolidated"]
[]
["17","Under floors etc","m³",{"v":15,"d":"15.00"}]
[]
[null,"Compaction of ground surfaces"]
[]
["18","Compaction of natural or excavated ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to ?% Mod AASHTO density","m²",{"v":431,"d":"431.00"}]
[]
["19","Bottoms of trenches, holes, etc","m²",{"v":267,"d":"267.00"}]
[]
[null,"WEED KILLERS, INSECTICIDES, ETC"]
[]
[null,"Soil insecticide in accordance with SANS 5859"]
[]
["20","Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m²",{"v":531,"d":"531.00"}]
[]
["21","To bottoms and sides of trenches etc","m²",{"v":461,"d":"461.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.3 : CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES"]
[]
[null,"15Mpa/19mm concrete"]
[]
["1","Surface blinding under footings","m³",{"v":14,"d":"14.00"}]
[]
[null,"REINFORCED CONCRETE"]
[]
[null,"25 Mpa/19mm Concrete:"]
[]
["2","Strip footings","m³",{"v":18,"d":"18.00"}]
[]
["3","Surface beds on waterproofing","m³",{"v":75,"d":"75.00"}]
[]
["4","Underpinning strip footings in 1m alternating sections under existing footings","m³",{"v":58,"d":"58.00"}]
[]
[null,"TEST BLOCKS"]
[]
[null,"Test blocks:"]
[]
["5","Making and testing set of three 150 x 150 x 150mm concrete strength test cubes.","Sets",{"v":24,"d":"24.00"}]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete smooth with a wood float"]
[]
["6","Surface beds, slabs, etc","m²",{"v":531,"d":"531.00"}]
[]
[null,"ROUGH FORMWORK (DEGREE OF ACCURACY II)"]
[]
[null,"Rough Formwork to Sides:"]
[]
["7","Footings","m",{"v":392,"d":"392.00"}]
[]
[null,"Boxing in rough formwork to form"]
[]
["8","25 x 25mm Chamfers along top or bottom edges","m",{"v":22,"d":"22.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Slip joints with three layers of damp proof sheeting between horizontal concrete and brick surfaces including cement mortar bed:"]
[]
["9","Not exceeding 300mm wide.","m",{"v":249,"d":"249.00"}]
[]
[null,"Expansion joints with bitumen emulsion paint between horizontal concrete and brick surfaces:"]
[]
["10","Joints not exceeding 300mm high.","m",{"v":73,"d":"73.00"}]
[]
[null,"Saw cut joints:"]
[]
["11","3 x 25mm Saw cut joints in two operations in top of concrete.","m",{"v":476,"d":"476.00"}]
[]
[null,"REINFORCEMENT"]
[]
[null,"Mild steel reinforcement to structural concrete work:"]
[]
["12","Bars of varying diameters.","Tonnes",{"v":5,"d":"5.00"}]
[]
["13","Bars of varying diameters.","Tonnes",{"v":3,"d":"3.00"}]
[]
[null,"Fabric reinforcement:"]
[]
["14","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m²",{"v":531,"d":"531.00"}]
[]
[null,"TEST BLOCKS"]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.4 : MASONRY"]
[]
[null,"BRICKWORK IN FOUNDATIONS (PROVISIONAL)"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive strength) in class II mortar"]
[]
["1","One brick walls","m²",{"v":70,"d":"70.00"}]
[]
[null,"Fair face to brickwork of selected building bricks in horizontal stretcher bond pointed with flush horizontal and vertical joints"]
[]
["2","Extra over for fair face","m²",{"v":14,"d":"14.00"}]
[]
[null,"2.5mm Brickwork reinforcement"]
[]
["3","150mm Wide reinforcement built in horizontally","m",{"v":325,"d":"325.00"}]
[]
[null,"BRICKWORK IN SUPERSTRUCTURE"]
[]
[null,"Brickwork in NFP bricks in  Class II mortar:"]
[]
["4","Piers.","m³","   1,0"]
[]
["5","Half brick walls.","m²",{"v":5,"d":"5.00"}]
[]
["6","Half brick walls in beamfilling.","m²",{"v":11,"d":"11.00"}]
[]
["7","One brick walls","m²",{"v":61,"d":"61.00"}]
[]
["8","One brick walls (firewalls)","m²",{"v":12,"d":"12.00"}]
[]
["9","One brick walls of two half brick skins bagged and sealed.","m²",{"v":215,"d":"215.00"}]
[]
["10","One brick walls of two half brick skins bagged and sealed (gable walls).","m²",{"v":3,"d":"3.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brickwork reinforcement:"]
[]
["11","75mm Wide reinforcement built in horizontally.","m",{"v":21,"d":"21.00"}]
[]
["12","150mm Wide reinforcement built in horizontally.","m","  1 120"]
[]
[null,"Prestressed concrete fabricated lintels:"]
[]
["13","90 x 114mm Lintels laid side by side in lengths not exceeding 3m.","m",{"v":176,"d":"176.00"}]
[]
[null,"Turning pieces:"]
[]
["14","110mm Wide turning piece to lintels etc.","m",{"v":27,"d":"27.00"}]
[]
[null,"Galvanised hoop iron cramps, ties, etc:"]
[]
["15","30 x 1,6mm Roof tie 1,5m long with one end fixed to timber and other end built into brickwork.","No",{"v":36,"d":"36.00"}]
[]
[null,"Air bricks etc:"]
[]
["16","Set of two Terra-cotta 229 x 152mm clay vermin proof air bricks.","No",{"v":6,"d":"6.00"}]
[]
[null,"FACE BRICKWORK"]
[]
[null,"Corobrik Ruby Light Satin FBS or Equivalent/similar approved face bricks pointed with recessed horizontal and vertical joints:"]
[]
["17","Extra over brickwork for face brickwork externally.","m²",{"v":111,"d":"111.00"}]
[]
["18","Extra over brickwork for face brickwork in beamfilling.","m²",{"v":82,"d":"82.00"}]
[]
["19","Extra over brickwork for brick-on-edge header course lintel pointed on one face and 220mm soffit.","m",{"v":20,"d":"20.00"}]
[]
["20","Fair raking cutting.","m",{"v":20,"d":"20.00"}]
[]
["21","Fair splay cutting.","m",{"v":18,"d":"18.00"}]
[]
[null,"Brick-on-edge header course copings, sills, etc of Corobrik Ruby Light Satin SBS face bricks, pointed with flush joints on all exposed faces"]
[]
["22","170 mm Wide sills set sloping and slightly projecting","m",{"v":20,"d":"20.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.5 : WATERPROOFING"]
[]
[null,"DAMPPROOFING OF WALLS AND FLOORS"]
[]
[null,"Brikgrip SABS approved DPC embossed damp proof course:"]
[]
["1","In walls","m²",{"v":68,"d":"68.00"}]
[]
["2","In walls under cills.","m²",{"v":12,"d":"12.00"}]
[]
[null,"One layer of 250 micron Consol Plastics Gunplas USB Green waterproof sheeting sealed at laps with Gunplas Pressure Sensitive Tape:"]
[]
["3","Under surface beds.","m²",{"v":531,"d":"531.00"}]
[]
[null,"FLASHINGS ETC."]
[]
[null,"One coat primer and three coats SABS approved acrylic emulsion."]
[]
["4","Bandage flashing 300mm wide.","m",{"v":22,"d":"22.00"}]
[]
[null,"JOINT SEALANTS ETC"]
[]
[null,"Approved clear silicone sealant:"]
[]
["5","In joints between steel frames and walls","m",{"v":60,"d":"60.00"}]
[]
[null,"Two - part polysulphide sealing compound including backing cord, bond breaker, primer, etc"]
[]
["6","3 x 25 mm In saw cut joints in floors.","m",{"v":476,"d":"476.00"}]
[]
["7","10 x 10mm In expansion / seperation joints in floors including raking out expansion joint filler as necessary.","m",{"v":322,"d":"322.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.6 : ROOF COVERINGS"]
[]
[null,"RIBBED METAL SHEETING AND ACCESSORIES"]
[]
[null,"Safintra Saflok 700 AZ 200 0.55mm thick concealed"]
[null,"fixing roof sheeting with Colorplus pre-painted white"]
[null,"finish fixed to steel purlins at about 1600mm centres"]
[null,"in accordance with manufacturers instruction"]
[]
["1","Roof covering with pitch not exceeding 25 degrees, in transportable lengths not exceeding 20m.","m²","  3 934"]
[]
[null,"Flashings:"]
[]
["2","Ridge capping 462mm girth, three times bent along girth and notched on site to suit roof profile.","m",{"v":219,"d":"219.00"}]
[]
["3","Polyclosers to suite profile of sheeting.","m",{"v":839,"d":"839.00"}]
[]
["4","Ridge end cap","No",{"v":14,"d":"14.00"}]
[]
[null,"ROOF AND WALL LINING AND INSULATION"]
[]
[null,"Super Sisalation® Heavy Industrial Grade 430 - Double sided reflective foil laminate incorporating layers of kraft paper and reinforcing scrim, laminated together with low density polyethylene (293gsm)."]
[]
["5","Insulation laid taut over timber rafters (at approximately 1200mm centres) and fixed concurrent with tiling battens, purlins, etc.","m²","  4 311"]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.7 : CARPENTRY AND JOINERY"]
[]
[null,"ROOF CONSTRUCTION"]
[]
[null,"Sawn softwood :"]
[]
["1","38 x 114mm Wall plates","m",{"v":44,"d":"44.00"}]
[]
["2","38 x 114mm Bracings.","m",{"v":176,"d":"176.00"}]
[]
["3","50 x 76mm Purlins.","m",{"v":88,"d":"88.00"}]
[]
["4","50 x 76mm Gable trim.","m",{"v":20,"d":"20.00"}]
[]
[null,"Wrought softwood:"]
[]
["5","70 x 70mm Splayed purlins.","m",{"v":44,"d":"44.00"}]
[]
[null,"LAMINATED TIMBER"]
[]
[null,"Wrought softwood Grade 5:"]
[]
["6","50 x 220mm Beams bolted.","m",{"v":14,"d":"14.00"}]
[]
[null,"ROOF SUNDRIES"]
[]
[null,"Sundries:"]
[]
["7","Teco rafter / beam connector.","No",{"v":72,"d":"72.00"}]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Pressed fibre-cement:"]
[]
["8","12 x 225mm  Medium density fascia boards including galvanised steel H-profile jointing strips.","m","  1 243"]
[]
["9","12 x 80 x 200mm Medium density angle section bargeboards including galvanised steel H-profile jointing strips.","m",{"v":334,"d":"334.00"}]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti:"]
[]
["10","19 x 70mm Skirting including 19mm quadrant bead.","m","  3 706"]
[]
[null,"SEMI SOLID CORE FLUSH DOORS"]
[]
[null,"Flush doors with hardboard covering on both sides with hardwood finger-jointed stiles hung to steel frames:"]
[]
["11","40mm Door 813 x 2032mm high","No",{"v":13,"d":"13.00"}]
[]
[null,"SOLID CORE FLUSH DOORS"]
[]
[null,"Flush doors with 3mm thick commercial ply on both sides:"]
[]
["12","44mm Door 813 x 2032mm high","No",{"v":6,"d":"6.00"}]
[]
["13","44mm Door 2100 x 2032mm high","No",{"v":1,"d":"1.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.8 : CEILINGS PARTITIONS AND ACCESS FLOORING"]
[]
[null,"NAILED UP AND SCREW UP CEILINGS"]
[]
[null,"6,4mm 'Rhinoboard' M-Strip ceiling fixed print side up to brandering with 32mm galvanized clout nails or 32mm grabber screws at 150mm centers with 'M-Strip' cover strips over joints with all nail or screw heads stopped and sanded level, all in strict accordance with the manufacturer's instructions:"]
[]
["1","Ceilings including 50 x 50 mm sawn softwood brandering at 400mm centres in one direction only to trusses (elsewhere) at 1,5mm centres.","m²","  10 712"]
[]
["2","Extra over ceiling for 600 x 600mm trap door.","No",{"v":85,"d":"85.00"}]
[]
[null,"Wrot softwood cornices"]
[]
["3","19 x 44mm Cornice nailed","m","  4 445"]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.9 : FLOOR COVERINGS"]
[]
[null,"VINYL FLOOR COVERINGS, WALL LININGS, ETC."]
[]
[null,"All vinyl flooring materials require a smooth, hard, clean, true and level surface, not only for appearance but also for achieving a satisfactory adhesive bond and long term durability"]
[]
[null,"The main contractor shall ensure that the sub-floor is acceptable to receive the vinyl flooring specified in respect of levelness, smoothness, soundness and cleanness"]
[]
[null,"300 x 300 x  2,5mm Thick hard wearing  semi-flexible vinyl floor tiles fixed with 'Marley No.60 Acrylic Adhesive':"]
[]
["1","On floors.","m²","  9 245"]
[]
[null,"POLISH, SEALERS, ETC"]
[]
[null,"Polish, sealers, etc:"]
[]
["2","Two coats wax polish on vinyl flooring.","m²","  9 245"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Resin backed polypropylene needlepunch carpeting"]
[]
["3","On floors","m²",{"v":112,"d":"112.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.10 : IRONMONGERY"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"Manufactured by Union"]
[]
["1","40mm Padlock (gate)","No",{"v":2,"d":"2.00"}]
[]
["2","65mm Padlock (trap door)","No",{"v":85,"d":"85.00"}]
[]
[null,"Manufactured by Geze"]
[]
["3","Ref 730/68 - 76 mm Profile arch sashlock S/S","No",{"v":20,"d":"20.00"}]
[]
["4","Ref  880-66/78 - 5 Pin NP Double cylinder 66mm 3K N.PL","No",{"v":20,"d":"20.00"}]
[]
["5","Master key","No",{"v":3,"d":"3.00"}]
[]
["6","Grand master key","No",{"v":1,"d":"1.00"}]
[]
[null,"Union"]
[]
["7","Four - lever lockset","No",{"v":20,"d":"20.00"}]
[]
[null,"HANDLES"]
[]
[null,"Manufactured by Geze"]
[]
["8","Ref EDE/101C-Daytona19mm/165X165X1.5/PL.CYL","No",{"v":20,"d":"20.00"}]
[]
["9","Ref 295/01 - Helping hand L/H OR R/H","No",{"v":1,"d":"1.00"}]
[]
["10","Ref JD213/305 - B/T S.S P/hand 330X305X25mm","No",{"v":1,"d":"1.00"}]
[]
[null,"PUSH PLATES AND KICK PLATES"]
[]
[null,"Manufactured by 'Geze'"]
[]
["11","160 x 160mm stainless steel push  plate","No",{"v":2,"d":"2.00"}]
[]
["12","813 x 20mm stainless steel kick plate","No",{"v":2,"d":"2.00"}]
[]
[null,"DOOR CLOSERS"]
[]
[null,"Dorma:"]
[]
["13","TS91' Overhead door closer with bracket fixed to metal","No",{"v":1,"d":"1.00"}]
[]
[null,"LETTERS, NAMEPLATES, ETC."]
[]
[null,"Manufactured by 'Geze'"]
[]
["14","90 x 32 x 3mm Thick perspex plate with 25mm high engraved and painted letters or numerals.","No",{"v":3,"d":"3.00"}]
[]
["15","Ref 079/160E-S/ST P/PL 160 x 160 x 1.2mm annodised aluminium plate with male or female symbol.","No",{"v":2,"d":"2.00"}]
[]
["16","Ref 079/160E-S/ST P/PL 160 x 160 x 1.2mm anodised aluminium plate with paraplegic symbol.","No",{"v":1,"d":"1.00"}]
[]
["17","200 x 200 x 3mm Thick perspex plate  with fire exit, fire extinguisher, fire hose reel or fire hydrant symbol.","No",{"v":5,"d":"5.00"}]
[]
[null,"BATHROOM FITTINGS"]
[]
[null,"Kimberley-Clark:"]
[]
["18","Approved lockable two roll toilet roll holder, size 144 x 138 x 301mm, plugged.","No",{"v":1,"d":"1.00"}]
[]
["19","Approved liquid soap dispenser, size 200 x 85 x 140mm, grade 304 stainless steel unit, plugged.","No",{"v":1,"d":"1.00"}]
[]
["20","19mm Diameter chromium plated towel rail 600mm long including end brackets.","No",{"v":1,"d":"1.00"}]
[]
[null,"SUNDRIES"]
[]
[null,"Geze:"]
[]
["21","Ref 140/83 - Door stop floor mounted","No",{"v":15,"d":"15.00"}]
[]
[null,"Chairman Industries:"]
[]
["22","32mm Stainless steel side grab rail plugged.","No",{"v":1,"d":"1.00"}]
[]
["23","32mm Stainless steel rear grab rail plugged.","No",{"v":1,"d":"1.00"}]
[]
[null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC"]
[]
[null,"Parrot:"]
[]
["24","Educational board side panel green writing board 1220 x 920mm high (ED2068) with aluminium chalk rail plugged (AL0120A).","No",{"v":2,"d":"2.00"}]
[]
["25","Edu BD Centre Panel magnetic white board 1820 x 1220mm high (ED7068) with aluminium chalk rail plugged (AL0120B).","No",{"v":2,"d":"2.00"}]
[]
["26","Pinning board 3000 x 1200mm high plugged","No",{"v":2,"d":"2.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.11 : METALWORK"]
[]
[null,"GALVANISED STEEL BALUSTRADING"]
[]
[null,"Framed and welded balustrading to access balconies (unpainted):"]
[]
["1","1100mm High balustrading comprising 25 x 50 x 2,5mm hollow section top and bottom rails, filled with 12 x 12mm solid section balusters at 100mm cenres, 40 x 40 x 3mm hollow section baluster with 100 x 150 x 8mm base plate welded on and twice bolted at 1500mm centres (As per drawing).","m",{"v":232,"d":"232.00"}]
[]
[null,"WELDED GALVANISED SCREENS, GATES, ETC."]
[]
[null,"Screens and gates"]
[]
["2","Gate 925 x 2032mm high, 10 x 10mm mild steel bars placed at 100mm centres at a 45egress angle with outer frame and inner frame including a pair of suitable hinges welded to frame and lockable sliding bolt with keep in frame","No",{"v":1,"d":"1.00"}]
[]
["3","Gate 3500 x 2032mm high of outer frame and inner frame with a pair of suitable hinges welded to frame and lockable sliding bolt with keep in frame","No",{"v":2,"d":"2.00"}]
[]
[null,"GALVANISED PRESSED STEEL DOOR FRAMES"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls"]
[]
["4","Frame for door 813 x 2032mm high","No",{"v":15,"d":"15.00"}]
[]
[null,"GALVANISED STEEL WINDOWS, DOORS, ETC."]
[]
[null,"All windows shall be fitted with standard brass fittings recommended by the manufacturer."]
[]
[null,"Burglar bars shall be standard pattern 5 x 20mm flat section bars corresponding horizontally and vertically with glazing bars."]
[]
[null,"Burglar bars to be fitted to all opening sections only unless otherwise described."]
[]
[null,"Standard school windows:"]
[]
["5","Composite window, 457 x 889mm high","No",{"v":3,"d":"3.00"}]
[]
["6","Composite window, 950 x 1400mm high","No",{"v":4,"d":"4.00"}]
[]
["7","Composite window, 1500 x 900mm high","No",{"v":4,"d":"4.00"}]
[]
["8","Composite window, 1800 x 1200mm high","No",{"v":3,"d":"3.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.12 : PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"All vinyl flooring materials require a smooth, hard, clean, true and level surface, not only for appearance but also for achieving satisfactory adhesive bond and long term durability"]
[]
[null,"The main contractor should ensure the sub-floor is acceptable to receive vinyl flooring specified in respect of levelness. Smoothness, soundness and cleanness"]
[]
[null,"Screeds on concrete:"]
[]
["1","20mm Thick on floors and landings to falls to receive floor tiles.","m²",{"v":112,"d":"112.00"}]
[]
["2","23mm Thick on floors and landings to receive vinyl tiles.","m²",{"v":27,"d":"27.00"}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork:"]
[]
["3","On walls.","m²",{"v":474,"d":"474.00"}]
[]
["4","On walls to receive tiles.","m²",{"v":91,"d":"91.00"}]
[]
[null,"CORNER PROTECTORS, DIVIDING STRIPS, ETC"]
[]
[null,"Corner protectors, dividing strips, etc"]
[]
["5","25 x 3mm Flat section brass dividing strips between different floor finishes.","m",{"v":24,"d":"24.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.13 : TILING"]
[]
[null,"WALL TILING"]
[]
[null,"200 x 200 x 4mm White glazed wall tiles  fixed with adhesive to plaster (elsewhere) and flush pointed with tinted jointing compound:"]
[]
["1","On walls","m²",{"v":195,"d":"195.00"}]
[]
["2","On splashbacks.","m²",{"v":10,"d":"10.00"}]
[]
["3","Fair exposed cutting and fitting around pipe not exceeding 50mm diameter.","No",{"v":1,"d":"1.00"}]
[]
["4","Ditto but exceeding 50mm and not exceeding 100mm diameter.","No",{"v":1,"d":"1.00"}]
[]
[null,"FLOOR TILING"]
[]
[null,"300 x 300 x 8mm Colour glazed floor tiles ( PC. Of R100.00m2 net supply only excluding VAT) fixed with adhesive to screeded (elsewhere)  concrete floors and flush pointed with tinted waterproof jointing compound including approved expansion joints:"]
[]
["5","On floors and landings.","m²",{"v":112,"d":"112.00"}]
[]
["6","Skirting 100mm high of cut tiles.","m",{"v":220,"d":"220.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.14 : PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Ogee  aluminium:"]
[]
["1","125mm Ogee eaves gutters.","m","  1 109"]
[]
["2","Extra over Ogee  eaves gutter for stopped end.","No",{"v":52,"d":"52.00"}]
[]
["3","Extra over Ogee eaves gutter for outlet for 100 x 75mm pipe.","No",{"v":71,"d":"71.00"}]
[]
["4","100 x 75mm Rainwater pipes.","m",{"v":307,"d":"307.00"}]
[]
["5","Extra over 100 x 75mm  rainwater pipe for bend.","No",{"v":213,"d":"213.00"}]
[]
["6","Extra over 100 x 75mm  rainwater pipe for shoe.","No",{"v":79,"d":"79.00"}]
[]
[null,"SANITARY FITTINGS"]
[]
[null,"Prices are to include for sealing all round with approved silicone waterproofing sealant at junction/gaps with tiled walls, timber fittings, vanity tops, etc."]
[]
[null,"Lecico Sanitaryware' vitreous china wash hand basins and pedestals:"]
[]
["7","410 x 500mm 'Atlas' white vitreous china lavatory basin (product code ATLDUOBAS0500BE) with one taphole including integrated overflow and chainstay hole, fixed with stainless steel screws and washers to plugs in wall  (tap and waste fitting elsewhere).","No",{"v":24,"d":"24.00"}]
[]
[null,"Lecico Sanitaryware' vitreous china WC suites:"]
[]
["8","Madison' white vitreous china close couple suite  (product code MADBOXDFL0SCSBE) with 100mm outlet  and matching 6 litre cistern including lid, fitments, flushpipe, etc., bedded in 4:1 cement mortar on concrete floors.","No",{"v":15,"d":"15.00"}]
[]
[null,"Plumline' vitreous china urinals:"]
[]
["9","Amaro' urinal  (code 031129) size 300 x 245 x 400mm high or equal approved with top inlet spreader and waste outlet including wall mounting brackets and connected to water supply, sealed with silicone sealant where urinal meets wall","No",{"v":7,"d":"7.00"}]
[]
[null,"WASTE UNIONS ETC"]
[]
[null,"Cobra Watertech':"]
[]
["10","32 mm CP basin waste union.","No",{"v":18,"d":"18.00"}]
[]
[null,"TRAPS ETC"]
[]
[null,"Priced are to include for jointing to uPVC pipe with and including the necessary adaptors unless otherwise described."]
[]
[null,"Butyl rubber:"]
[]
["11","32 mm deep seal \"P\" or \"S\" trap.","No",{"v":18,"d":"18.00"}]
[]
[null,"TAPS,VALVES, ETC"]
[]
[null,"Priced are to include  for jointing to copper pipe with and including the necessary fittings unless otherwise described."]
[]
[null,"Brass."]
[]
["12","15 mm Fulway gate valve.","No",{"v":1,"d":"1.00"}]
[]
["13","22 mm Fulway gate valve.","No",{"v":1,"d":"1.00"}]
[]
["14","28 mm Fulway gate valve.","No",{"v":1,"d":"1.00"}]
[]
[null,"Plumline"]
[]
["15","15 mm CP Ballostop.","No",{"v":1,"d":"1.00"}]
[]
["16","22 mm CP Ballostop.","No",{"v":1,"d":"1.00"}]
[]
["17","15 mm CP Star pillartaps.","No",{"v":18,"d":"18.00"}]
[]
[null,"SANITARY PLUMBING"]
[]
[null,"uPVC pipes:"]
[]
["18","50mm Pipes.","m",{"v":1,"d":"1.00"}]
[]
["19","110mm Pipes.","m",{"v":1,"d":"1.00"}]
[]
["20","50mm Pipes under surface beds.","m",{"v":1,"d":"1.00"}]
[]
["21","110mm Pipes under surface beds.","m",{"v":1,"d":"1.00"}]
[]
["22","110mm Pipes laid in and including trenches not exceeding 1m deep.","m",{"v":1,"d":"1.00"}]
[]
["23","50mm Pipes chased into brick walls.","m",{"v":1,"d":"1.00"}]
[]
[null,"Extra over uPVC pipes for fittings:"]
[]
["24","110mm Reducer.","No",{"v":1,"d":"1.00"}]
[]
["25","50mm Bend.","No",{"v":1,"d":"1.00"}]
[]
["26","110mm Bend.","No",{"v":1,"d":"1.00"}]
[]
["27","50mm Junction.","No",{"v":1,"d":"1.00"}]
[]
["28","110mm Junction.","No",{"v":1,"d":"1.00"}]
[]
["29","110mm Pan connector.","No",{"v":1,"d":"1.00"}]
[]
["30","110mm Acess bent pan connector.","No",{"v":1,"d":"1.00"}]
[]
["31","50mm Acess bend.","No",{"v":1,"d":"1.00"}]
[]
["32","110mm Acess bend.","No",{"v":1,"d":"1.00"}]
[]
["33","50mm Acess junction.","No",{"v":1,"d":"1.00"}]
[]
["34","110mm Acess junction.","No",{"v":1,"d":"1.00"}]
[]
["35","110mm Acess reducing junction.","No",{"v":1,"d":"1.00"}]
[]
["36","110mm Acess double junction.","No",{"v":1,"d":"1.00"}]
[]
[null,"WATER SUPPLIES"]
[]
[null,"Class 1 copper pipes:"]
[]
["37","15mm Pipes.","m",{"v":1,"d":"1.00"}]
[]
["38","22mm Pipes.","m",{"v":1,"d":"1.00"}]
[]
["39","28mm Pipes.","m",{"v":1,"d":"1.00"}]
[]
["40","15mm Pipes chased into brick walls.","m",{"v":1,"d":"1.00"}]
[]
["41","22mm Pipes chased into brick walls.","m",{"v":1,"d":"1.00"}]
[]
[null,"Extra over copper pipe for capillary fitting:"]
[]
["42","15mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
["43","22mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
["44","28mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
[null,"Extra over copper pipe for brass compression fitting:"]
[]
["45","15mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
["46","22mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
["47","28mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
[null,"Copper overflow and service pipes:"]
[]
["48","15mm Bent service pipe average 450mm girth and joint to copper pipe and fittings.","No",{"v":1,"d":"1.00"}]
[]
["49","22mm Bent overflow pipe average 450mm girth and joint to fittings.","No",{"v":1,"d":"1.00"}]
[]
[null,"FIRE APPLIANCES ETC."]
[]
[null,"Chubb':"]
[]
["50","Everyway' hose reel complete with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket.","No",{"v":1,"d":"1.00"}]
[]
["51","4,5kg DPC fire extinguisher complete with backboard and wall bracket plugged to wall.","No",{"v":1,"d":"1.00"}]
[]
["52","Ditto but 9kg.","No",{"v":1,"d":"1.00"}]
[]
["53","Watertight high impact, UV- stablised clear acrylic fire hose reel cupboard with numbered twist-action closer seal fixed to brick wall.","No",{"v":1,"d":"1.00"}]
[]
[null,"WATER SUPPLIES TO FIRE APPLIANCES"]
[]
[null,"Class 1 copper pipes:"]
[]
["54","28mm Pipes.","m",{"v":1,"d":"1.00"}]
[]
["55","28mm Pipes under surface bed.","m",{"v":1,"d":"1.00"}]
[]
[null,"Extra over class 1 copper pipes for capillary fittings:"]
[]
["56","28mm Fittings.","No",{"v":1,"d":"1.00"}]
[]
[null,"TESTING"]
[]
["57","Testing all pipe systems.","Item",{"v":1,"d":"1.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.15 : GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"6.38 mm Clear laminated safety glass"]
[]
["1","Panes exceeding 0,5m2 and not exceeding 2.5m2.","m²",{"v":55,"d":"55.00"}]
[]
[null,"4 mm Patterned toughened glass:"]
[]
["2","Panes exceeding 0,1m2 and not exceeding 0.5m2.","m²",{"v":5,"d":"5.00"}]
[]
[null,"TOPS, SHELVES, DOORS, MIRRORS, ETC."]
[]
[null,"3mm Silvered float glass copper backed mirrors with polished edges fixed with double sided adhesive tape:"]
[]
["3","Frameless mirror 700 x 450 mm high.","No",{"v":5,"d":"5.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.16 : PAINTWORK"]
[]
[null,"PAINTWORK ETC. TO NEW SURFACES"]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coat Alkali Resistant Plaster Primer  and two coats superior quality acrylic emulsion paint:"]
[]
["1","On interior walls.","m²",{"v":484,"d":"484.00"}]
[]
[null,"ON PLASTER BOARD"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coatAlkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:"]
[]
["2","On internal ceilings and cornices.","m²","  9 963"]
[]
["3","On external ceilings and cornices.","m²",{"v":150,"d":"150.00"}]
[]
[null,"ON FIBRE-CEMENT, ETC."]
[]
[null,"Prepare surfaces and remove all loose material, apply one coat Alkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:"]
[]
["4","On exterior fascias and barge boards.","m²",{"v":774,"d":"774.00"}]
[]
[null,"ON METAL"]
[]
[null,"Prepare surfaces and remove all loose material, dust, grease, salts and contamination with one coat ater based primer, one coat alkyd based universal  undercoat  and two coats superior quality universal enamel paint on: galvanised steel or aluminium:"]
[]
["5","On door frames.","m²",{"v":26,"d":"26.00"}]
[]
["6","On window frames with burglar bars (bsm).","m²",{"v":50,"d":"50.00"}]
[]
["7","On security gates","m²",{"v":9,"d":"9.00"}]
[]
[null,"ON WOOD, WOOD BOARD"]
[]
[null,"Stop, fill, sand down and prepare wood surfaces and apply three coats superior quality clear gloss varnish"]
[]
["8","On interior / exterior doors.","m²",{"v":91,"d":"91.00"}]
[]
["9","On interior / exterior skirtings, rails, etc not exceeding 300mm girth.","m","  3 799"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"PREPARATORY WORK TO EXISTING WORK"]
[]
[null,"Previously painted plastered surfaces"]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[null,"Previously painted metal surfaces"]
[null,"Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[null,"Previously painted wood surfaces"]
[null,"Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth"]
[]
[null,"ON PREVIOUSLY PAINTED SURFACES"]
[]
[null,"ON EXISTING INTERNAL FLOATED PLASTER SURFACES"]
[]
[null,"Two coats superior quality acrylic emulsion paint for interior and exterior use"]
[]
["10","Walls","m²","  24 726"]
[]
[null,"ON EXISTING PLASTERBOARD SURFACES"]
[]
[null,"Two coats superior quality acrylic emulsion paint for interior and exterior use"]
[]
["11","Ceilings and cornices  (White colour group)","m²",{"v":845,"d":"845.00"}]
[]
[null,"ON EXISTING FIBRE-CEMENT BOARD SURFACES"]
[]
[null,"Two coats extremely durable UV-resistant washable pure acrylic paint, on work in poor condition"]
[]
["12","Cills","m²",{"v":35,"d":"35.00"}]
[]
[null,"ON EXISTING METAL SURFACES"]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint"]
[]
["13","Door frames","m²",{"v":46,"d":"46.00"}]
[]
["14","Security gates","m²",{"v":90,"d":"90.00"}]
[]
["15","On window frames with burglar bars (bsm).","m²","  2 824"]
[]
["16","On steel balustrades (bsm)","m²",{"v":264,"d":"264.00"}]
[]
["17","On roof sheeting","m²",{"v":380,"d":"380.00"}]
[]
[null,"ON EXISTING WOOD SURFACES"]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint"]
[]
["18","Doors","m²",{"v":256,"d":"256.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]
[]
[]
[null,"SECTION NO. 3 : EXTERNAL WORKS"]
[]
[]
[null,"BILL NO.1 : EXTERNAL WORKS (PROVISIONAL)"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Note to tenderers: The removal, storage ,disposal, etc  of asbestos sheeting, etc to be executed in strict accordance to the bye laws (OHS) regarding same by a specialist asbestos sub-contractor. Prices to include for this."]
[]
[null,"All work to be demolished, etc is to be removed off site, unless otherwise stated, prices to include for this."]
[]
[null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement including layerworks"]
[]
["1","Concrete V-drains 900mm wide","m",{"v":18,"d":"18.00"}]
[]
["2","Take up and remove 60mm thick corobrik block paving including 200mm thick layer works, and set aside paving"]
[null,"including later relaying in new position","m²",{"v":200,"d":"200.00"}]
[]
[null,"ALTERATIONS"]
[]
[null,"JOINT SEALANTS"]
[]
[null,"Chip open the crack to form a \"V\" shape 20mm wide x 10mm deep and scratch out the debris that may block the crack in the sides of the hole. Grinding in the floor approximately 200mm to 300mm apart from the rebar to be placed into an"]
[null,"epoxy repair mortar 'SIKA TOP-ARMATEC 100'. Fill the crack with structural epoxy repair mortar SIKA MONO TOP 615HB'"]
[]
["3","Concrete V-drains, walkways, etc.","m",{"v":9,"d":"9.00"}]
[]
[null,"Resealing of joints"]
[]
["4","Ream out joint and install UV resistant polysulphide sealant","m",{"v":25,"d":"25.00"}]
[]
[null,"TEMPORARY WORKS"]
[]
["5","1,5m High 'Bonnox' wire mesh temporary fencing with shade cloth.","m",{"v":315,"d":"315.00"}]
[]
["6","Single gate 900 x 1,5m high.","No",{"v":1,"d":"1.00"}]
[]
[null,"GENERAL SITE CLEARANCE, ETC."]
[]
[null,"Site clearance, etc.:"]
[]
["7","Allow for clearing of the site all grass, weeds, shrubs, debris, etc and cartwawy all vegetation and stockpile","m²",{"v":350,"d":"350.00"}]
[]
[null,"KEEPING EXCAVATIONS FREE OF WATER"]
[]
[null,"Keeping excavations free of water:"]
[]
["8","Keeping excavations free of all water other than subterranean water through out this bill .","Item",{"v":1,"d":"1.00"}]
[]
[null,"APRONS, PAVING, RAMPS, PATHS AND STEPS"]
[]
[null,"Earthworks:"]
[]
["9","Excavate in soft excavations in earth to reduce levels under ramps, pavings, aprons.","m³",{"v":20,"d":"20.00"}]
[]
["10","Extra over excavations for excavating in soft rock.","m³",{"v":2,"d":"2.00"}]
[]
["11","Extra over excavations for carting away surplus material off site.","m³",{"v":30,"d":"30.00"}]
[]
["12","Approved filling supplied by the Contractor under pavings and paths compacted to a density of 93% Mod AASHTO.","m³",{"v":20,"d":"20.00"}]
[]
["13","Over site of G5 material as sub -base layer in accordance with SABS 1200DM 125mm layer compacted to 95% Mod AASHTO density and trim to grades","m³",{"v":15,"d":"15.00"}]
[]
["14","Over site of G2 material as base layer in according with SABS 1200DM 125mm layer compacted to 98% Mod AASHTO density and trim to grades.","m³",{"v":15,"d":"15.00"}]
[]
["15","Trim, level, excavate and scarify for a depth of 150mm ground surface to receive concrete paving and compact to 93% Mod AASHTO density.","m²",{"v":200,"d":"200.00"}]
[]
["16","Approved weed killer to surface of earth under pavings, aprons, etc.","m²",{"v":200,"d":"200.00"}]
[]
[null,"Take from where set aside and relay paving"]
[]
["17","Relay corobrik block paving","m²",{"v":200,"d":"200.00"}]
[]
[null,"Monetary Allowance"]
[]
["18","Allow a provisional allowance of R 150 000.00 (One Hundred and Fifty Thousand Rands) for external works to be ascertained on site","Item"]
[]
[]
[null,"Bill Total"]
[]
[]
[]
[null,"BILL NO.2 : PLUMBING AND DRAINAGE (PROVISIONAL)"]
[]
[null,"STORM WATER CHANNELS."]
[]
[null,"Smooth finished in-situ reinforced concrete 25Mpa/13mm channels:"]
[]
["1","900 x 130mm Smooth  finished open V shaped  channel to detail, cast in alternative panels and to falls, including excavations, shaping and grading ground as required, formwork, mesh Ref 193.","m",{"v":143,"d":"143.00"}]
[]
["2","Extra for angles, intersections, ends, dressing into sides of catchpits, etc.","No",{"v":4,"d":"4.00"}]
[]
["3","12mm Thick bitumen impregnated softboard between vertical concrete surfaces of channels.","m",{"v":143,"d":"143.00"}]
[]
["4","Approved polysulphide sealing compound to joints of channels.","m",{"v":143,"d":"143.00"}]
[]
[null,"Monetary Allowance"]
[]
["5","Allow a monetary allowance fo R 50 000.00 for proving and cleaning pipework","Item"]
[]
["6","Allow a monetary allowance of R 25 000.00 for cleaning of all sewer and stormwater manholes","Item"]
[]
[null,"TESTING"]
[]
["7","Testing all plumbing systems.","Item",{"v":1,"d":"1.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]
[]
[]
[null,"SECTION NO. 4 : PROVISIONAL SUMS"]
[]
[]
[null,"BILL NO.1 : PROVISIONAL SUMS"]
[]
[null,"The following Provisional Amounts are all Net amounts Exclusive of commision for the Contractor. These amounts are for the work to be executed complete by the Nominated/Selected Sub-Contractors:"]
[]
[null,"LANDSCAPING"]
[]
["1","Provide the amount of R 35,000.00 (Thirty Five Thousand Rands) for Landscaping, etc.","Item",{"v":1,"d":"1.00"},null,{"v":35000,"d":"35,000.00"}]
[]
["2","Profit on above item.","Item",{"v":1,"d":"1.00"}]
[]
["3","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"SIGNAGE"]
[]
["4","Provide the amount of R 20,000.00 (Twenty Thousand Rands) for Signage.","Item",{"v":1,"d":"1.00"},null,{"v":20000,"d":"20,000.00"}]
[]
["5","Profit on above item.","Item",{"v":1,"d":"1.00"}]
[]
["6","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
["7","Provide the amount of R 360,000.00 (Three Hundred and Sixty Thousand Rands) for Plumbing & Drainage related items","Item",{"v":1,"d":"1.00"},null,{"v":360000,"d":"360,000.00"}]
[]
["8","Profit on above item","Item",{"v":1,"d":"1.00"}]
[]
["9","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"TEMPORARY ACCOMMODATION & ABLUTIONS"]
[]
["10","Provide the amount of R 3 305 000.00  (Three Million Three Hundred and Five Thousand Rands Only Rands) for the purchase, transportation, ground works and erection of mobile classrooms and ablution facilities, including the regular maintenance of the ablution facilities for the duration of the contract. The units are to be made good upon project completion and relocated to another site determined by the principal Agent and/or client, less or equal to 200km from the site, all as per Architectural / Engineering specifications, to be performed by a specialist where required","Item",{"v":1,"d":"1.00"},null,{"v":3305000,"d":"3,305,000.00"}]
[]
["11","Profit on above item.","Item",{"v":1,"d":"1.00"}]
[]
["12","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"GEOTECH & SURVEY"]
[]
["13","Provide the amount of R 100,000.00 (One Hundred Thousand Rands) for Geotech and Survey","Item",{"v":1,"d":"1.00"},null,{"v":100000,"d":"100,000.00"}]
[]
["14","Profit on above item","Item",{"v":1,"d":"1.00"}]
[]
["15","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"CARPENTRY & JOINERY"]
[]
["16","Provide the amount of R 100,000.00 (One Hundred Thousand Rands) for Carpentry & Joinery","Item",{"v":1,"d":"1.00"},null,{"v":100000,"d":"100,000.00"}]
[]
["17","Profit on above item","Item",{"v":1,"d":"1.00"}]
[]
["18","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"The following Electrical Works are to be undertaken by direct contractors, selected at the client's discretion"]
[]
[null,"ELECTRICAL INSTALLATION"]
[]
["19","Provide the amount of R 620 000.00 (Six Hundred and Twenty Thousand Rands) for Electrical Installation","Item",{"v":1,"d":"1.00"},null,{"v":620000,"d":"620,000.00"}]
[]
["20","Profit on above item.","Item",{"v":1,"d":"1.00"}]
[]
["21","Attendance on ditto.","Item",{"v":1,"d":"1.00"}]
[]
[null,"BUDGETARY ALLOWANCES"]
[]
["22","Allow a budgetary amount of R 187 500.00 (One Hundred and Eighty Seven Thousand Rands) for Community Liaison Officer (CLO)","Item",{"v":1,"d":"1.00"},null,{"v":187500,"d":"187,500.00"}]
[]
["23","Allow a budgetary amount of R 200 000.00 (Two Hundred Thousand Rands) for the provision of skills development and mentorship of"]
[null,"candidates for the duration of construction","Item",{"v":1,"d":"1.00"},null,{"v":200000,"d":"200,000.00"}]
[]
[null,"BUILDER'S WORK IN CONNECTION WITH PROVISIONAL SUMS"]
[]
["24","Provide the amount of R 50 000.00 (Fifty Thousand Rands) for Builder's Work in connection with Provisional Sums.","Item",{"v":1,"d":"1.00"},null,{"v":50000,"d":"50,000.00"}]
[]
[]
[null,"Bill Total"]
[]
[]
[null,"Section Total "]

{"sheet":"Final Summary","index":2,"n_rows":60,"n_cols":3,"rows_kept":60,"merged":[[4,0,4,2],[5,0,5,2]],"flags":["formulas_cached_only"]}
[]
["HTS WELKOM HIGH SCHOOL "]
[]
[]
[]
[]
[]
["FINAL SUMMARY"]
[]
[]
[]
[null,"PAGE","AMOUNT"]
[]
[]
["CONDITIONS OF CONTRACT"]
[]
[]
["SECTION 1        :  PRELIMINARIES","1-32"]
[]
["SECTION 2        :  BUILDINGS","2-62"]
[]
["SECTION 3        : EXTERNAL WORKS ","3-6"]
[]
["SECTION 4        : PROVISIONAL SUMS","4-4"]
[]
[]
[]
[]
[]
[]
["SUB TOTAL","R"]
[]
["ADD: ESCALATION (PRE & POST TENDER)","R",{"v":900000,"d":"900,000.00"}]
[]
[]
["SUB TOTAL","R"]
[]
[]
[]
["ADD: CONTINGENCIES ","R",{"v":2420000,"d":"2,420,000.00"}]
[]
[]
[]
["SUB TOTAL","R"]
[]
[]
["VALUE ADDED TAX"]
[]
["Value added tax @ 15%","R"]
[]
[]
[]
["TOTAL CARRIED TO FORM OF OFFER","R"]
[]
[]
[]
[]
[]
[]
["FS-1"]